[NOTE ]  coreboot-24.12-758-g1e7ba810c6bb Thu Mar 06 19:02:27 UTC 2025 x86_32 bootblock starting (log level: 7)...
[DEBUG]  FMAP: Found "FLASH" version 1.1 at 0xaa0000.
[DEBUG]  FMAP: base = 0xff000000 size = 0x1000000 #areas = 4
[DEBUG]  FMAP: area COREBOOT found @ aa0200 (5635584 bytes)
[INFO ]  CBFS: mcache @0xfeff0e00 built for 16 files, used 0x344 of 0x4000 bytes
[INFO ]  CBFS: Found 'fallback/romstage' @0x68c0 size 0x17050 in mcache @0xfeff0e5c
[DEBUG]  BS: bootblock times (exec / console): total (unknown) / 45 ms


[NOTE ]  coreboot-24.12-758-g1e7ba810c6bb Thu Mar 06 19:02:27 UTC 2025 x86_32 romstage starting (log level: 7)...
[DEBUG]  SMBus controller enabled
[ERROR]  early_usb_init: USB00: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB01: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB02: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB03: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB04: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB05: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB06: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB07: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB09: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB10: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB11: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB12: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[ERROR]  early_usb_init: USB13: USBIR_TXRX_GAIN_MOBILE_LOW is an invalid setting for desktop!
[INFO ]  Detected system type: desktop
[DEBUG]  Setting up static northbridge registers... done
[DEBUG]  Initializing Graphics...
[DEBUG]  Back from systemagent_early_init()
[INFO ]  Intel ME early init
[INFO ]  Intel ME firmware is ready
[DEBUG]  ME: Requested 32MB UMA
[DEBUG]  Starting native Platform init
[DEBUG]  DMI: Running at X4 @ 5000MT/s
[DEBUG]  FMAP: area RW_MRC_CACHE found @ a90000 (65536 bytes)
[DEBUG]  Trying stored timings.
[DEBUG]  Starting Ivy Bridge RAM training (fast boot).
[DEBUG]  100MHz reference clock support: yes
[DEBUG]  PLL_REF100_CFG value: 0x2
[DEBUG]  Trying CAS 11, tCK 320.
[DEBUG]  Found compatible clock, CAS pair.
[DEBUG]  Selected DRAM frequency: 800 MHz
[DEBUG]  Selected CAS latency   : 11T
[DEBUG]  MPLL busy... done in 10 us
[DEBUG]  MPLL frequency is set at : 800 MHz
[DEBUG]  Done dimm mapping
[DEBUG]  Update PCI-E configuration space:
[DEBUG]  PCI(0, 0, 0)[a0] = 0
[DEBUG]  PCI(0, 0, 0)[a4] = 6
[DEBUG]  PCI(0, 0, 0)[bc] = 82a00000
[DEBUG]  PCI(0, 0, 0)[a8] = 7b600000
[DEBUG]  PCI(0, 0, 0)[ac] = 6
[DEBUG]  PCI(0, 0, 0)[b8] = 80000000
[DEBUG]  PCI(0, 0, 0)[b0] = 80a00000
[DEBUG]  PCI(0, 0, 0)[b4] = 80800000
[DEBUG]  PCI(0, 0, 0)[7c] = 7f
[DEBUG]  PCI(0, 0, 0)[70] = fe000000
[DEBUG]  PCI(0, 0, 0)[74] = 5
[DEBUG]  PCI(0, 0, 0)[78] = fe000c00
[DEBUG]  Done memory map
[DEBUG]  Done io registers
[DEBUG]  t123: 1767, 6000, 6120
[NOTE ]  ME: Wrong mode : 4
[NOTE ]  ME: FWS2: 0x101f013e
[NOTE ]  ME:  Bist in progress: 0x0
[NOTE ]  ME:  ICC Status      : 0x3
[NOTE ]  ME:  Invoke MEBx     : 0x1
[NOTE ]  ME:  CPU replaced    : 0x1
[NOTE ]  ME:  MBP ready       : 0x1
[NOTE ]  ME:  MFS failure     : 0x0
[NOTE ]  ME:  Warm reset req  : 0x0
[NOTE ]  ME:  CPU repl valid  : 0x1
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  FW update req   : 0x0
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  Current state   : 0x1f
[NOTE ]  ME:  Current PM event: 0x0
[NOTE ]  ME:  Progress code   : 0x1
[NOTE ]  Full training required
[NOTE ]  PASSED! Tell ME that DRAM is ready
[NOTE ]  ME: FWS2: 0x1052013e
[NOTE ]  ME:  Bist in progress: 0x0
[NOTE ]  ME:  ICC Status      : 0x3
[NOTE ]  ME:  Invoke MEBx     : 0x1
[NOTE ]  ME:  CPU replaced    : 0x1
[NOTE ]  ME:  MBP ready       : 0x1
[NOTE ]  ME:  MFS failure     : 0x0
[NOTE ]  ME:  Warm reset req  : 0x0
[NOTE ]  ME:  CPU repl valid  : 0x1
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  FW update req   : 0x0
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  Current state   : 0x52
[NOTE ]  ME:  Current PM event: 0x0
[NOTE ]  ME:  Progress code   : 0x1
[NOTE ]  ME: Requested BIOS Action: Continue to boot
[DEBUG]  ME: FW Partition Table      : OK
[DEBUG]  ME: Bringup Loader Failure  : NO
[DEBUG]  ME: Firmware Init Complete  : NO
[DEBUG]  ME: Manufacturing Mode      : NO
[DEBUG]  ME: Boot Options Present    : NO
[DEBUG]  ME: Update In Progress      : NO
[DEBUG]  ME: Current Working State   : Normal
[DEBUG]  ME: Current Operation State : Bring up
[DEBUG]  ME: Current Operation Mode  : Security Override via Jumper
[DEBUG]  ME: Error Code              : No Error
[DEBUG]  ME: Progress Phase          : BUP Phase
[DEBUG]  ME: Power Management Event  : Clean Moff->Mx wake
[DEBUG]  ME: Progress Phase State    : 0x52
[DEBUG]  memcfg DDR3 ref clock 133 MHz
[DEBUG]  memcfg DDR3 clock 1596 MHz
[DEBUG]  memcfg channel assignment: A: 0, B  1, C  2
[DEBUG]  memcfg channel[0] config (00631020):
[DEBUG]     ECC inactive
[DEBUG]     enhanced interleave mode on
[DEBUG]     rank interleave on
[DEBUG]     DIMMA 8192 MB width x8 dual rank
[DEBUG]     DIMMB 4096 MB width x8 single rank, selected
[DEBUG]  memcfg channel[1] config (00631020):
[DEBUG]     ECC inactive
[DEBUG]     enhanced interleave mode on
[DEBUG]     rank interleave on
[DEBUG]     DIMMA 8192 MB width x8 dual rank
[DEBUG]     DIMMB 4096 MB width x8 single rank, selected
[DEBUG]  CBMEM:
[DEBUG]  IMD: root @ 0x7ffff000 254 entries.
[DEBUG]  IMD: root @ 0x7fffec00 62 entries.
[DEBUG]  FMAP: area COREBOOT found @ aa0200 (5635584 bytes)
[DEBUG]  External stage cache:
[DEBUG]  IMD: root @ 0x803ff000 254 entries.
[DEBUG]  IMD: root @ 0x803fec00 62 entries.
[DEBUG]  CBMEM entry for DIMM info: 0x7ffdb000
[DEBUG]  SMM Memory Map
[DEBUG]  SMRAM       : 0x80000000 0x800000
[DEBUG]   Subregion 0: 0x80000000 0x300000
[DEBUG]   Subregion 1: 0x80300000 0x100000
[DEBUG]   Subregion 2: 0x80400000 0x400000
[DEBUG]  Normal boot
[INFO ]  CBFS: Found 'fallback/postcar' @0x46580 size 0x5e68 in mcache @0xfeff103c
[DEBUG]  Loading module at 0x7ffcf000 with entry 0x7ffcf031. filesize: 0x5a88 memsize: 0xbdd8
[DEBUG]  Processing 232 relocs. Offset value of 0x7dfcf000
[DEBUG]  BS: romstage times (exec / console): total (unknown) / 619 ms


[NOTE ]  coreboot-24.12-758-g1e7ba810c6bb Thu Mar 06 19:02:27 UTC 2025 x86_32 postcar starting (log level: 7)...
[DEBUG]  Normal boot
[DEBUG]  FMAP: area COREBOOT found @ aa0200 (5635584 bytes)
[INFO ]  CBFS: Found 'fallback/ramstage' @0x1d980 size 0x1d865 in mcache @0x7ffdd0bc
[DEBUG]  Loading module at 0x7fe83000 with entry 0x7fe83000. filesize: 0x3b260 memsize: 0x14a3d0
[DEBUG]  Processing 4357 relocs. Offset value of 0x7be83000
[DEBUG]  BS: postcar times (exec / console): total (unknown) / 43 ms


[NOTE ]  coreboot-24.12-758-g1e7ba810c6bb Thu Mar 06 19:02:27 UTC 2025 x86_32 ramstage starting (log level: 7)...
[DEBUG]  Normal boot
[INFO ]  Enumerating buses...
[DEBUG]  Root Device scanning...
[DEBUG]  CPU_CLUSTER: 0 enabled
[DEBUG]  DOMAIN: 00000000 enabled
[DEBUG]  DOMAIN: 00000000 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 00
[DEBUG]  PCI: 00:00:00.0 [8086/0158] enabled
[DEBUG]  PCI: 00:00:01.0 [8086/0151] enabled
[DEBUG]  PCI: 00:00:02.0 [8086/016a] enabled
[DEBUG]  PCI: 00:00:14.0 [8086/1e31] enabled
[DEBUG]  PCI: 00:00:16.0 [8086/1e3a] enabled
[DEBUG]  PCI: 00:00:16.1: Disabling device
[DEBUG]  PCI: 00:00:16.2: Disabling device
[INFO ]  PCI: Static device PCI: 00:00:16.3 not found, disabling it.
[DEBUG]  PCI: 00:00:19.0 [8086/1502] enabled
[DEBUG]  PCI: 00:00:1a.0 [8086/1e2d] enabled
[DEBUG]  PCI: 00:00:1b.0 [8086/1e20] enabled
[DEBUG]  PCI: 00:00:1c.0: No downstream device
[INFO ]  PCH: PCIe Root Port coalescing is enabled
[DEBUG]  PCI: 00:00:1c.0: Disabling device
[DEBUG]  PCI: 00:00:1c.0: check set enabled
[DEBUG]  PCI: 00:00:1c.1: Found a downstream device
[DEBUG]  PCI: 00:00:1c.1: Disabling device
[DEBUG]  PCI: 00:00:1c.2: Found a downstream device
[DEBUG]  PCI: 00:00:1c.2: Disabling device
[DEBUG]  PCI: 00:00:1c.3: Found a downstream device
[DEBUG]  PCI: 00:00:1c.3: Disabling device
[DEBUG]  PCI: 00:00:1c.4: No downstream device
[DEBUG]  PCI: 00:00:1c.4: Disabling device
[DEBUG]  PCI: 00:00:1c.4: check set enabled
[DEBUG]  PCI: 00:00:1c.5: No downstream device
[DEBUG]  PCI: 00:00:1c.5: Disabling device
[DEBUG]  PCI: 00:00:1c.6: No downstream device
[DEBUG]  PCI: 00:00:1c.6: Disabling device
[DEBUG]  PCI: 00:00:1c.7: No downstream device
[DEBUG]  PCI: 00:00:1c.7: Disabling device
[DEBUG]  PCI: 00:00:1d.0 [8086/1e26] enabled
[DEBUG]  PCI: 00:00:1e.0 [8086/244e] enabled
[DEBUG]  PCI: 00:00:1f.0 [8086/1e48] enabled
[DEBUG]  PCI: 00:00:1f.2 [8086/1e00] enabled
[DEBUG]  PCI: 00:00:1f.3 [8086/1e22] enabled
[DEBUG]  PCI: 00:00:1f.5: Disabling device
[DEBUG]  PCI: 00:00:1f.5 [8086/1e08] disabled No operations
[DEBUG]  PCI: 00:00:1f.6: Disabling device
[DEBUG]  PCI: 00:00:1f.6 [8086/1e24] disabled No operations
[WARN ]  PCI: Leftover static devices:
[WARN ]  PCI: 00:00:01.1
[WARN ]  PCI: 00:00:01.2
[WARN ]  PCI: 00:00:04.0
[WARN ]  PCI: 00:00:06.0
[WARN ]  PCI: 00:00:16.3
[WARN ]  PCI: Check your devicetree.cb.
[DEBUG]  PCI: 00:00:01.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 01
[INFO ]  PCI: 00:00:01.0: Setting Max_Payload_Size to 256 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:01.0 finished in 14 msecs
[DEBUG]  PCI: 00:00:1e.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 02
[DEBUG]  scan_bus: bus PCI: 00:00:1e.0 finished in 5 msecs
[DEBUG]  PCI: 00:00:1f.0 scanning...
[DEBUG]  PNP: 002e.ff enabled
[INFO ]  Found TPM 1.2 SLB9635 TT 1.2 (0x000b) by Infineon (0x15d1)
[DEBUG]  PNP: 004e.0 enabled
[DEBUG]  PNP: 002e.ff scanning...
[DEBUG]  PNP: 002e.0 disabled
[DEBUG]  PNP: 002e.1 enabled
[DEBUG]  PNP: 002e.2 disabled
[DEBUG]  PNP: 002e.3 enabled
[DEBUG]  PNP: 002e.4 enabled
[DEBUG]  PNP: 002e.5 enabled
[DEBUG]  PNP: 002e.6 enabled
[DEBUG]  PNP: 002e.7 enabled
[DEBUG]  PNP: 002e.8 enabled
[DEBUG]  PNP: 002e.f enabled
[DEBUG]  PNP: 002e.15 enabled
[DEBUG]  PNP: 002e.1c enabled
[DEBUG]  PNP: 002e.1e enabled
[DEBUG]  scan_bus: bus PNP: 002e.ff finished in 43 msecs
[DEBUG]  scan_bus: bus PCI: 00:00:1f.0 finished in 65 msecs
[DEBUG]  PCI: 00:00:1f.3 scanning...
[DEBUG]  scan_bus: bus PCI: 00:00:1f.3 finished in 0 msecs
[DEBUG]  scan_bus: bus DOMAIN: 00000000 finished in 342 msecs
[DEBUG]  scan_bus: bus Root Device finished in 360 msecs
[INFO ]  done
[DEBUG]  BS: BS_DEV_ENUMERATE run times (exec / console): 1 / 374 ms
[DEBUG]  found VGA at PCI: 00:00:02.0
[DEBUG]  Setting up VGA for PCI: 00:00:02.0
[DEBUG]  Setting PCI_BRIDGE_CTL_VGA for bridge DOMAIN: 00000000
[DEBUG]  Setting PCI_BRIDGE_CTL_VGA for bridge Root Device
[INFO ]  Allocating resources...
[INFO ]  Reading resources...
[DEBUG]  Adding PCIe enhanced config space BAR 0xf0000000-0xf4000000.
[DEBUG]  TOUUD 0x67b600000 TOLUD 0x82a00000 TOM 0x600000000
[DEBUG]  MEBASE 0x5fe000000
[DEBUG]  IGD decoded, subtracting 32M UMA and 2M GTT
[DEBUG]  TSEG base 0x80000000 size 8M
[INFO ]  Available memory below 4GB: 2048M
[INFO ]  Available memory above 4GB: 22454M
[INFO ]  Done reading resources.
[INFO ]  === Resource allocator: DOMAIN: 00000000 - Pass 1 (relative placement) ===
[INFO ]  === Resource allocator: DOMAIN: 00000000 - Pass 2 (allocating resources) ===
[DEBUG]  DOMAIN: 00000000 io: base: 0 size: 0 align: 0 gran: 0 limit: ffff
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 10000000 base 00000000 limit 00000fff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.ff 00 base 0000002e limit 0000002f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.1 60 base 00000378 limit 0000037f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.2 60 base 000002f8 limit 000002ff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.3 60 base 000003f8 limit 000003ff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.4 60 base 00000600 limit 00000607 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.4 62 base 00000610 limit 0000061f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.6 60 base 00000060 limit 00000060 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.6 62 base 00000064 limit 00000064 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.7 60 base 00000620 limit 0000063f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.8 60 base 00000800 limit 000008ff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.15 60 base 00000680 limit 0000068f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.15 62 base 00000690 limit 0000069f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.1c 60 base 00000640 limit 0000065f io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.1e 60 base 00000660 limit 0000067f io (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.3 20 base 00000400 limit 0000041f io (fixed)
[INFO ]   DOMAIN: 00000000: Resource ranges:
[INFO ]   * Base: 1000, Size: f000, Tag: 100
[DEBUG]    PCI: 00:00:02.0 20 *  [0xffc0 - 0xffff] limit: ffff io
[DEBUG]    PCI: 00:00:19.0 18 *  [0xffa0 - 0xffbf] limit: ffbf io
[DEBUG]    PCI: 00:00:1f.2 20 *  [0xff80 - 0xff9f] limit: ff9f io
[DEBUG]    PCI: 00:00:1f.2 10 *  [0xff78 - 0xff7f] limit: ff7f io
[DEBUG]    PCI: 00:00:1f.2 18 *  [0xff70 - 0xff77] limit: ff77 io
[DEBUG]    PCI: 00:00:1f.2 14 *  [0xff6c - 0xff6f] limit: ff6f io
[DEBUG]    PCI: 00:00:1f.2 1c *  [0xff68 - 0xff6b] limit: ff6b io
[DEBUG]  DOMAIN: 00000000 io: base: 0 size: 0 align: 0 gran: 0 limit: ffff done
[DEBUG]  DOMAIN: 00000000 mem: base: 80000000 size: 0 align: 0 gran: 0 limit: efffffff
[DEBUG]  DOMAIN: 00000000 mem: base: 100000000 size: 0 align: 0 gran: 0 limit: fffffffff
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 60 base f0000000 limit f3ffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 03 base 00000000 limit 0009ffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 04 base 00100000 limit 7fffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 05 base 100000000 limit 67b5fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 06 base 80000000 limit 829fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 07 base 000a0000 limit 000bffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 08 base 000c0000 limit 000fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 09 base fed90000 limit fed90fff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 0a base fed91000 limit fed91fff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 10000100 base ff000000 limit ffffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 03 base fec00000 limit fec00fff mem (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 004e.0 00 base fed40000 limit fed44fff mem (fixed)
[INFO ]   DOMAIN: 00000000: Resource ranges:
[INFO ]   * Base: 82a00000, Size: 6d600000, Tag: 200
[INFO ]   * Base: 67b600000, Size: 984a00000, Tag: 200
[DEBUG]    PCI: 00:00:02.0 18 *  [0xe0000000 - 0xefffffff] limit: efffffff prefmem
[DEBUG]    PCI: 00:00:02.0 10 *  [0xdfc00000 - 0xdfffffff] limit: dfffffff mem
[DEBUG]    PCI: 00:00:19.0 10 *  [0xdfbe0000 - 0xdfbfffff] limit: dfbfffff mem
[DEBUG]    PCI: 00:00:14.0 10 *  [0xdfbd0000 - 0xdfbdffff] limit: dfbdffff mem
[DEBUG]    PCI: 00:00:1b.0 10 *  [0xdfbcc000 - 0xdfbcffff] limit: dfbcffff mem
[DEBUG]    PCI: 00:00:19.0 14 *  [0xdfbcb000 - 0xdfbcbfff] limit: dfbcbfff mem
[DEBUG]    PCI: 00:00:1f.2 24 *  [0xdfbca000 - 0xdfbca7ff] limit: dfbca7ff mem
[DEBUG]    PCI: 00:00:1a.0 10 *  [0xdfbc9000 - 0xdfbc93ff] limit: dfbc93ff mem
[DEBUG]    PCI: 00:00:1d.0 10 *  [0xdfbc8000 - 0xdfbc83ff] limit: dfbc83ff mem
[DEBUG]    PCI: 00:00:1f.3 10 *  [0xdfbc7000 - 0xdfbc70ff] limit: dfbc70ff mem
[DEBUG]    PCI: 00:00:16.0 10 *  [0xdfbc6000 - 0xdfbc600f] limit: dfbc600f mem
[DEBUG]  DOMAIN: 00000000 mem: base: 80000000 size: 0 align: 0 gran: 0 limit: efffffff done
[DEBUG]  DOMAIN: 00000000 mem: base: 100000000 size: 0 align: 0 gran: 0 limit: fffffffff done
[INFO ]  === Resource allocator: DOMAIN: 00000000 - resource allocation complete ===
[DEBUG]  PCI: 00:00:01.0 1c <- [0x000000000000ffff - 0x000000000000fffe] size 0x00000000 gran 0x0c seg 00 bus 01 io
[DEBUG]  PCI: 00:00:01.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 01 prefmem
[DEBUG]  PCI: 00:00:01.0 20 <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x14 seg 00 bus 01 mem
[DEBUG]  PCI: 00:00:02.0 10 <- [0x00000000dfc00000 - 0x00000000dfffffff] size 0x00400000 gran 0x16 mem64
[DEBUG]  PCI: 00:00:02.0 18 <- [0x00000000e0000000 - 0x00000000efffffff] size 0x10000000 gran 0x1c prefmem64
[DEBUG]  PCI: 00:00:02.0 20 <- [0x000000000000ffc0 - 0x000000000000ffff] size 0x00000040 gran 0x06 io
[DEBUG]  PCI: 00:00:14.0 10 <- [0x00000000dfbd0000 - 0x00000000dfbdffff] size 0x00010000 gran 0x10 mem64
[DEBUG]  PCI: 00:00:16.0 10 <- [0x00000000dfbc6000 - 0x00000000dfbc600f] size 0x00000010 gran 0x04 mem64
[DEBUG]  PCI: 00:00:19.0 10 <- [0x00000000dfbe0000 - 0x00000000dfbfffff] size 0x00020000 gran 0x11 mem
[DEBUG]  PCI: 00:00:19.0 14 <- [0x00000000dfbcb000 - 0x00000000dfbcbfff] size 0x00001000 gran 0x0c mem
[DEBUG]  PCI: 00:00:19.0 18 <- [0x000000000000ffa0 - 0x000000000000ffbf] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:00:1a.0 10 <- [0x00000000dfbc9000 - 0x00000000dfbc93ff] size 0x00000400 gran 0x0a mem
[DEBUG]  PCI: 00:00:1b.0 10 <- [0x00000000dfbcc000 - 0x00000000dfbcffff] size 0x00004000 gran 0x0e mem64
[DEBUG]  PCI: 00:00:1d.0 10 <- [0x00000000dfbc8000 - 0x00000000dfbc83ff] size 0x00000400 gran 0x0a mem
[DEBUG]  PCI: 00:00:1e.0 1c <- [0x000000000000ffff - 0x000000000000fffe] size 0x00000000 gran 0x0c seg 00 bus 02 io
[DEBUG]  PCI: 00:00:1e.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 02 prefmem
[DEBUG]  PCI: 00:00:1e.0 20 <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x14 seg 00 bus 02 mem
[DEBUG]  PNP: 002e.1 14 <- [0x000000000000009c - 0x000000000000009b] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 1c <- [0x00000000000000a8 - 0x00000000000000a7] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 1d <- [0x0000000000000008 - 0x0000000000000007] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 22 <- [0x000000000000003f - 0x000000000000003e] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 1a <- [0x00000000000000b0 - 0x00000000000000af] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 1b <- [0x000000000000001e - 0x000000000000001d] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 27 <- [0x0000000000000008 - 0x0000000000000007] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 2a <- [0x0000000000000020 - 0x000000000000001f] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 2d <- [0x0000000000000001 - 0x0000000000000000] size 0x00000000 gran 0x00 irq
[DEBUG]  PNP: 002e.1 60 <- [0x0000000000000378 - 0x000000000000037f] size 0x00000008 gran 0x03 io
[DEBUG]  PNP: 002e.1 70 <- [0x0000000000000007 - 0x0000000000000007] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.1 74 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.3 60 <- [0x00000000000003f8 - 0x00000000000003ff] size 0x00000008 gran 0x03 io
[DEBUG]  PNP: 002e.3 70 <- [0x0000000000000004 - 0x0000000000000004] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.4 60 <- [0x0000000000000600 - 0x0000000000000607] size 0x00000008 gran 0x03 io
[DEBUG]  PNP: 002e.4 62 <- [0x0000000000000610 - 0x000000000000061f] size 0x00000010 gran 0x04 io
[NOTE ]  PNP: 002e.4 70 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f0 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f1 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f2 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f3 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f4 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f5 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f6 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f7 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f8 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 f9 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 fa irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 fb irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 fc irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 fd irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.4 fe irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.5 70 <- [0x000000000000000c - 0x000000000000000c] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.6 60 <- [0x0000000000000060 - 0x0000000000000060] size 0x00000001 gran 0x00 io
[DEBUG]  PNP: 002e.6 62 <- [0x0000000000000064 - 0x0000000000000064] size 0x00000001 gran 0x00 io
[DEBUG]  PNP: 002e.6 70 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.6 f0 <- [0x0000000000000040 - 0x000000000000003f] size 0x00000000 gran 0x00 drq
[DEBUG]  PNP: 002e.7 60 <- [0x0000000000000620 - 0x000000000000063f] size 0x00000020 gran 0x05 io
[NOTE ]  PNP: 002e.7 f8 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 f9 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 fa irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 fb irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 fc irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 fd irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.7 fe irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.8 60 <- [0x0000000000000800 - 0x00000000000008ff] size 0x00000100 gran 0x08 io
[DEBUG]  PNP: 002e.8 f0 <- [0x0000000000000020 - 0x0000000000000020] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f1 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f2 <- [0x0000000000000040 - 0x0000000000000040] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f3 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f4 <- [0x0000000000000066 - 0x0000000000000066] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f5 <- [0x0000000000000067 - 0x0000000000000067] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f6 <- [0x0000000000000066 - 0x0000000000000066] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.8 f7 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[NOTE ]  PNP: 002e.8 70 irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.f f1 <- [0x0000000000000097 - 0x0000000000000097] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.f f2 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.f f5 <- [0x0000000000000008 - 0x0000000000000008] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.f fe <- [0x0000000000000080 - 0x0000000000000080] size 0x00000001 gran 0x00 drq
[NOTE ]  PNP: 002e.f f0 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f3 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f4 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f6 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f7 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f8 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f f9 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f fa irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f fb irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f fc irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.f fd irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.15 60 <- [0x0000000000000680 - 0x000000000000068f] size 0x00000010 gran 0x04 io
[DEBUG]  PNP: 002e.15 62 <- [0x0000000000000690 - 0x000000000000069f] size 0x00000010 gran 0x04 io
[NOTE ]  PNP: 002e.15 70 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f0 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f1 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f2 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f3 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f4 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f5 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f6 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f7 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f8 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 f9 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 fa irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 fb irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 fc irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 fd irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.15 fe irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.1c 60 <- [0x0000000000000640 - 0x000000000000065f] size 0x00000020 gran 0x05 io
[DEBUG]  PNP: 002e.1e 60 <- [0x0000000000000660 - 0x000000000000067f] size 0x00000020 gran 0x05 io
[DEBUG]  PNP: 002e.1e f4 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 drq
[NOTE ]  PNP: 002e.1e f0 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.1e f1 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.1e f2 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.1e f3 irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.ff 00 <- [0x000000000000002e - 0x000000000000002f] size 0x00000002 gran 0x00 io
[DEBUG]  PCI: 00:00:1f.2 10 <- [0x000000000000ff78 - 0x000000000000ff7f] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:00:1f.2 14 <- [0x000000000000ff6c - 0x000000000000ff6f] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:00:1f.2 18 <- [0x000000000000ff70 - 0x000000000000ff77] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:00:1f.2 1c <- [0x000000000000ff68 - 0x000000000000ff6b] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:00:1f.2 20 <- [0x000000000000ff80 - 0x000000000000ff9f] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:00:1f.2 24 <- [0x00000000dfbca000 - 0x00000000dfbca7ff] size 0x00000800 gran 0x0b mem
[DEBUG]  PCI: 00:00:1f.3 10 <- [0x00000000dfbc7000 - 0x00000000dfbc70ff] size 0x00000100 gran 0x08 mem64
[INFO ]  Done setting resources.
[INFO ]  Done allocating resources.
[DEBUG]  BS: BS_DEV_RESOURCES run times (exec / console): 1 / 1563 ms
[INFO ]  Enabling resources...
[DEBUG]  PCI: 00:00:00.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:00.0 cmd <- 06
[DEBUG]  PCI: 00:00:01.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:01.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:01.0 cmd <- 00
[DEBUG]  PCI: 00:00:02.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:02.0 cmd <- 03
[DEBUG]  PCI: 00:00:14.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:14.0 cmd <- 102
[DEBUG]  PCI: 00:00:16.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:16.0 cmd <- 02
[DEBUG]  PCI: 00:00:19.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:19.0 cmd <- 103
[DEBUG]  PCI: 00:00:1a.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1a.0 cmd <- 102
[DEBUG]  PCI: 00:00:1b.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1b.0 cmd <- 102
[DEBUG]  PCI: 00:00:1d.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1d.0 cmd <- 102
[DEBUG]  PCI: 00:00:1e.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:1e.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1e.0 cmd <- 100
[DEBUG]  PCI: 00:00:1f.0 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1f.0 cmd <- 107
[DEBUG]  PCI: 00:00:1f.2 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1f.2 cmd <- 03
[DEBUG]  PCI: 00:00:1f.3 subsystem <- 103c/3397
[DEBUG]  PCI: 00:00:1f.3 cmd <- 103
[INFO ]  done.
[DEBUG]  BS: BS_DEV_ENABLE run times (exec / console): 0 / 129 ms
[INFO ]  Initializing devices...
[DEBUG]  CPU_CLUSTER: 0 init
[INFO ]  LAPIC 0x0 in XAPIC mode.
[DEBUG]  MTRR: Physical address space:
[DEBUG]  0x0000000000000000 - 0x000000000009ffff size 0x000a0000 type 6
[DEBUG]  0x00000000000a0000 - 0x00000000000bffff size 0x00020000 type 0
[DEBUG]  0x00000000000c0000 - 0x000000007fffffff size 0x7ff40000 type 6
[DEBUG]  0x0000000080000000 - 0x00000000dfffffff size 0x60000000 type 0
[DEBUG]  0x00000000e0000000 - 0x00000000efffffff size 0x10000000 type 1
[DEBUG]  0x00000000f0000000 - 0x00000000ffffffff size 0x10000000 type 0
[DEBUG]  0x0000000100000000 - 0x000000067b5fffff size 0x57b600000 type 6
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x250 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x258 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x259 0x0000000000000000
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x268 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x269 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26a 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26b 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26c 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26d 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26e 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26f 0x0606060606060606
[DEBUG]  apic_id 0x0 setup mtrr for CPU physical address size: 36 bits
[DEBUG]  MTRR: default type WB/UC MTRR counts: 4/5.
[DEBUG]  MTRR: WB selected as default type.
[DEBUG]  MTRR: 0 base 0x0000000080000000 mask 0x0000000fc0000000 type 0
[DEBUG]  MTRR: 1 base 0x00000000c0000000 mask 0x0000000fe0000000 type 0
[DEBUG]  MTRR: 2 base 0x00000000e0000000 mask 0x0000000ff0000000 type 1
[DEBUG]  MTRR: 3 base 0x00000000f0000000 mask 0x0000000ff0000000 type 0

[DEBUG]  MTRR check
[DEBUG]  Fixed MTRRs   : Enabled
[DEBUG]  Variable MTRRs: Enabled

[DEBUG]  CPU has 4 cores, 4 threads enabled.
[DEBUG]  Setting up SMI for CPU
[INFO ]  Will perform SMM setup.
[DEBUG]  microcode: sig=0x306a9 pf=0x2 revision=0x21
[DEBUG]  FMAP: area COREBOOT found @ aa0200 (5635584 bytes)
[INFO ]  CBFS: Found 'cpu_microcode_blob.bin' @0x80 size 0x6800 in mcache @0x7ffdd02c
[INFO ]  CPU: Intel(R) Xeon(R) CPU E3-1225 V2 @ 3.20GHz.
[INFO ]  LAPIC 0x0 in XAPIC mode.
[DEBUG]  CPU: APIC: 00 enabled
[DEBUG]  CPU: APIC: 01 enabled
[DEBUG]  CPU: APIC: 02 enabled
[DEBUG]  CPU: APIC: 03 enabled
[DEBUG]  Loading module at 0x00030000 with entry 0x00030000. filesize: 0x178 memsize: 0x178
[DEBUG]  Processing 16 relocs. Offset value of 0x00030000
[DEBUG]  Attempting to start 3 APs
[DEBUG]  Waiting for 10ms after sending INIT.
[DEBUG]  Waiting for SIPI to complete...
[DEBUG]  done.
[DEBUG]  Waiting for SIPI to complete...
[DEBUG]  done.
[INFO ]  LAPIC 0x2 in XAPIC mode.
[INFO ]  AP: slot 1 apic_id 2, MCU rev: 0x00000021
[INFO ]  LAPIC 0x4 in XAPIC mode.
[INFO ]  AP: slot 2 apic_id 4, MCU rev: 0x00000021
[INFO ]  LAPIC 0x6 in XAPIC mode.
[INFO ]  AP: slot 3 apic_id 6, MCU rev: 0x00000021
[DEBUG]  Loading module at 0x00038000 with entry 0x00038000. filesize: 0x1a0 memsize: 0x1a0
[DEBUG]  Processing 9 relocs. Offset value of 0x00038000
[DEBUG]  smm_module_setup_stub: stack_top = 0x80001000
[DEBUG]  smm_module_setup_stub: per cpu stack_size = 0x400
[DEBUG]  smm_module_setup_stub: runtime.smm_size = 0x10000
[DEBUG]  SMM Module: stub loaded at 38000. Will call 0x7fea32cc
[DEBUG]  Installing permanent SMM handler to 0x80000000
[DEBUG]  HANDLER      [0x802fe000-0x802ff1ef]

[DEBUG]  CPU 0
[DEBUG]    ss0        [0x802fdc00-0x802fdfff]
[DEBUG]    stub0      [0x802f6000-0x802f619f]

[DEBUG]  CPU 1
[DEBUG]    ss1        [0x802fd800-0x802fdbff]
[DEBUG]    stub1      [0x802f5c00-0x802f5d9f]

[DEBUG]  CPU 2
[DEBUG]    ss2        [0x802fd400-0x802fd7ff]
[DEBUG]    stub2      [0x802f5800-0x802f599f]

[DEBUG]  CPU 3
[DEBUG]    ss3        [0x802fd000-0x802fd3ff]
[DEBUG]    stub3      [0x802f5400-0x802f559f]

[DEBUG]  stacks       [0x80000000-0x80000fff]
[DEBUG]  Loading module at 0x802fe000 with entry 0x802fe27b. filesize: 0x11d0 memsize: 0x11f0
[DEBUG]  Processing 56 relocs. Offset value of 0x802fe000
[DEBUG]  Loading module at 0x802f6000 with entry 0x802f6000. filesize: 0x1a0 memsize: 0x1a0
[DEBUG]  Processing 9 relocs. Offset value of 0x802f6000
[DEBUG]  smm_module_setup_stub: stack_top = 0x80001000
[DEBUG]  smm_module_setup_stub: per cpu stack_size = 0x400
[DEBUG]  smm_module_setup_stub: runtime.smm_size = 0x300000
[DEBUG]  SMM Module: placing smm entry code at 802f5c00,  cpu # 0x1
[DEBUG]  SMM Module: placing smm entry code at 802f5800,  cpu # 0x2
[DEBUG]  SMM Module: placing smm entry code at 802f5400,  cpu # 0x3
[DEBUG]  SMM Module: stub loaded at 802f6000. Will call 0x802fe27b
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ee000, cpu = 0
[DEBUG]  In relocation handler: cpu 0
[DEBUG]  New SMBASE=0x802ee000 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802edc00, cpu = 1
[DEBUG]  In relocation handler: cpu 1
[DEBUG]  New SMBASE=0x802edc00 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ed400, cpu = 3
[DEBUG]  In relocation handler: cpu 3
[DEBUG]  New SMBASE=0x802ed400 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ed800, cpu = 2
[DEBUG]  In relocation handler: cpu 2
[DEBUG]  New SMBASE=0x802ed800 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  Initializing CPU #0
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[INFO ]  CPU: Intel(R) Xeon(R) CPU E3-1225 V2 @ 3.20GHz.
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  VMX status: enabled
[DEBUG]  IA32_FEATURE_CONTROL status: locked
[INFO ]  APIC: 00: PP0 current limit not set in devicetree
[INFO ]  APIC: 00: PP0 PSI0 not set in devicetree
[INFO ]  APIC: 00: PP0 PSI1 not set in devicetree
[INFO ]  APIC: 00: PP0 PSI2 not set in devicetree
[INFO ]  APIC: 00: PP1 current limit not set in devicetree
[INFO ]  APIC: 00: PP1 PSI0 not set in devicetree
[INFO ]  APIC: 00: PP1 PSI1 not set in devicetree
[INFO ]  APIC: 00: PP1 PSI2 not set in devicetree
[INFO ]  APIC: 00: Programmable ratio limit for turbo mode is disabled
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 3200
[INFO ]  Turbo is available but hidden
[INFO ]  Turbo is available and visible
[INFO ]  CPU #0 initialized
[INFO ]  Initializing CPU #1
[INFO ]  Initializing CPU #3
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[INFO ]  Initializing CPU #2
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[INFO ]  CPU: Intel(R) Xeon(R) CPU E3-1225 V2 @ 3.20GHz.
[INFO ]  CPU: Intel(R) Xeon(R) CPU E3-1225 V2 @ 3.20GHz.
[INFO ]  CPU: Intel(R) Xeon(R) CPU E3-1225 V2 @ 3.20GHz.
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  VMX status: enabled
[DEBUG]  VMX status: enabled
[DEBUG]  IA32_FEATURE_CONTROL status: locked
[DEBUG]  IA32_FEATURE_CONTROL status: locked
[INFO ]  APIC: 04: Programmable ratio limit for turbo mode is disabled
[INFO ]  APIC: 04: Programmable ratio limit for turbo mode is disabled
[DEBUG]  cpu: energy policy set to 6
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 3200
[INFO ]  CPU #1 initialized
[DEBUG]  model_x06ax: frequency set to 3200
[INFO ]  CPU #2 initialized
[DEBUG]  VMX status: enabled
[DEBUG]  IA32_FEATURE_CONTROL status: locked
[INFO ]  APIC: 06: Programmable ratio limit for turbo mode is disabled
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 3200
[INFO ]  CPU #3 initialized
[INFO ]  bsp_do_flight_plan done after 610 msecs.
[DEBUG]  SMI_STS:
[DEBUG]  GPE0_STS: GPIO14 GPIO10 GPIO9 GPIO7 GPIO0
[DEBUG]  ALT_GP_SMI_STS: GPI14 GPI13 GPI11 GPI10 GPI9 GPI7 GPI6 GPI5 GPI4 GPI3 GPI2 GPI1 GPI0
[DEBUG]  TCO_STS:
[DEBUG]  Locking SMM.
[DEBUG]  CPU_CLUSTER: 0 init finished in 919 msecs
[DEBUG]  PCI: 00:00:00.0 init
[DEBUG]  Disabling PEG12.
[DEBUG]  Disabling PEG11.
[DEBUG]  Disabling Device 4.
[DEBUG]  Disabling PEG60.
[DEBUG]  Disabling Device 7.
[DEBUG]  Set BIOS_RESET_CPL
[DEBUG]  CPU TDP: 77 Watts
[DEBUG]  PCI: 00:00:00.0 init finished in 22 msecs
[DEBUG]  PCI: 00:00:01.0 init
[DEBUG]  PCI: 00:00:01.0 init finished in 0 msecs
[DEBUG]  PCI: 00:00:02.0 init
[INFO ]  CBFS: Found 'vbt.bin' @0x45b80 size 0x4c6 in mcache @0x7ffdd1e4
[INFO ]  Found a VBT of 3777 bytes
[INFO ]  GMA: Found VBT in CBFS
[INFO ]  GMA: Found valid VBT in CBFS
[DEBUG]  GT Power Management Init
[DEBUG]  IVB GT2 35W Power Meter Weights
[DEBUG]  GT Power Management Init (post VBIOS)
[DEBUG]  PCI: 00:00:02.0 init finished in 47 msecs
[DEBUG]  PCI: 00:00:14.0 init
[DEBUG]  XHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:14.0 init finished in 4 msecs
[DEBUG]  PCI: 00:00:16.0 init
[DEBUG]  ME: FW Partition Table      : OK
[DEBUG]  ME: Bringup Loader Failure  : NO
[DEBUG]  ME: Firmware Init Complete  : NO
[DEBUG]  ME: Manufacturing Mode      : NO
[DEBUG]  ME: Boot Options Present    : NO
[DEBUG]  ME: Update In Progress      : NO
[DEBUG]  ME: Current Working State   : Normal
[DEBUG]  ME: Current Operation State : Bring up
[DEBUG]  ME: Current Operation Mode  : Security Override via Jumper
[DEBUG]  ME: Error Code              : No Error
[DEBUG]  ME: Progress Phase          : BUP Phase
[DEBUG]  ME: Power Management Event  : Clean Moff->Mx wake
[DEBUG]  ME: Progress Phase State    : 0x52
[NOTE ]  ME: BIOS path: Disable
[DEBUG]  ME: me_state=0, me_state_prev=0
[DEBUG]  PCI: 00:00:16.0: Disabling device
[DEBUG]  PCI: 00:00:16.0 init finished in 75 msecs
[DEBUG]  PCI: 00:00:19.0 init
[DEBUG]  PCI: 00:00:19.0 init finished in 0 msecs
[DEBUG]  PCI: 00:00:1a.0 init
[DEBUG]  EHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:1a.0 init finished in 4 msecs
[DEBUG]  PCI: 00:00:1b.0 init
[DEBUG]  Azalia: base = 0xdfbcc000
[DEBUG]  Azalia: codec_mask = 09
[DEBUG]  azalia_audio: initializing codec #3...
[DEBUG]  azalia_audio:  - vendor/device id: 0x80862806
[DEBUG]  azalia_audio:  - verb size: 16
[DEBUG]  azalia_audio:  - verb loaded
[DEBUG]  azalia_audio: initializing codec #0...
[DEBUG]  azalia_audio:  - vendor/device id: 0x10ec0221
[DEBUG]  azalia_audio:  - verb size: 44
[DEBUG]  azalia_audio:  - verb loaded
[DEBUG]  PCI: 00:00:1b.0 init finished in 48 msecs
[DEBUG]  PCI: 00:00:1d.0 init
[DEBUG]  EHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:1d.0 init finished in 4 msecs
[DEBUG]  PCI: 00:00:1e.0 init
[DEBUG]  PCI init.
[DEBUG]  PCI: 00:00:1e.0 init finished in 2 msecs
[DEBUG]  PCI: 00:00:1f.0 init
[DEBUG]  pch: lpc_init
[INFO ]  PCH: detected Q75, device id: 0x1e48, rev id 0x4
[DEBUG]  IOAPIC: Initializing IOAPIC at fec00000
[DEBUG]  IOAPIC: ID = 0x00
[DEBUG]  IOAPIC: 24 interrupts
[DEBUG]  IOAPIC: Clearing IOAPIC at fec00000
[DEBUG]  IOAPIC: Bootstrap Processor Local APIC = 0x00
[INFO ]  Set power off after power failure.
[INFO ]  NMI sources disabled.
[DEBUG]  PantherPoint PM init
[DEBUG]  RTC: failed = 0x0
[DEBUG]  RTC Init
[DEBUG]  apm_control: Disabling ACPI.
[DEBUG]  APMC done.
[DEBUG]  pch_spi_init
[DEBUG]  PCI: 00:00:1f.0 init finished in 56 msecs
[DEBUG]  PCI: 00:00:1f.2 init
[DEBUG]  SATA: Initializing...
[DEBUG]  SATA: Controller in AHCI mode.
[DEBUG]  ABAR: 0xdfbca000
[DEBUG]  PCI: 00:00:1f.2 init finished in 10 msecs
[DEBUG]  PCI: 00:00:1f.3 init
[DEBUG]  PCI: 00:00:1f.3 init finished in 0 msecs
[DEBUG]  PNP: 002e.1 init
[DEBUG]  PNP: 002e.1 init finished in 0 msecs
[DEBUG]  PNP: 002e.3 init
[DEBUG]  PNP: 002e.3 init finished in 0 msecs
[DEBUG]  PNP: 002e.4 init
[DEBUG]  PNP: 002e.4 init finished in 0 msecs
[DEBUG]  PNP: 002e.5 init
[DEBUG]  PNP: 002e.5 init finished in 0 msecs
[DEBUG]  PNP: 002e.6 init
[DEBUG]  PNP: 002e.6 init finished in 0 msecs
[DEBUG]  PNP: 002e.7 init
[DEBUG]  PNP: 002e.7 init finished in 0 msecs
[DEBUG]  PNP: 002e.8 init
[INFO ]  NPCD378: PSU fan PWM 0x77
[DEBUG]  PNP: 002e.8 init finished in 3 msecs
[DEBUG]  PNP: 002e.f init
[DEBUG]  PNP: 002e.f init finished in 0 msecs
[DEBUG]  PNP: 002e.15 init
[DEBUG]  PNP: 002e.15 init finished in 0 msecs
[DEBUG]  PNP: 002e.1c init
[DEBUG]  PNP: 002e.1c init finished in 0 msecs
[DEBUG]  PNP: 002e.1e init
[DEBUG]  PNP: 002e.1e init finished in 0 msecs
[INFO ]  Devices initialized
[DEBUG]  BS: BS_DEV_INIT run times (exec / console): 328 / 1085 ms
[DEBUG]  TPM: Startup
[DEBUG]  TPM: command 0x99 returned 0x0
[DEBUG]  TPM: Asserting physical presence
[DEBUG]  TPM: command 0x4000000a returned 0x0
[DEBUG]  TPM: command 0x65 returned 0x0
[DEBUG]  TPM: flags disable=0, deactivated=0, nvlocked=1
[INFO ]  TPM: setup succeeded
[DEBUG]  BS: BS_DEV_INIT exit times (exec / console): 49 / 29 ms
[INFO ]  Finalize devices...
[DEBUG]  PCI: 00:00:1f.0 final
[INFO ]  Manufacturer: 20
[INFO ]  SF: Detected 20 ba18 with sector size 0x1000, total 0x1000000
[DEBUG]  apm_control: Finalizing SMM.
[DEBUG]  APMC done.
[INFO ]  Devices finalized
[DEBUG]  BS: BS_POST_DEVICE run times (exec / console): 0 / 26 ms
[INFO ]  CBFS: Found 'fallback/dsdt.aml' @0x43600 size 0x2537 in mcache @0x7ffdd1b8
[WARN ]  CBFS: 'fallback/slic' not found.
[INFO ]  ACPI: Writing ACPI tables at 7fe43000.
[DEBUG]  ACPI:    * FACS
[DEBUG]  ACPI:    * FACP
[DEBUG]  ACPI: added table 1/32, length now 44
[DEBUG]  Found 1 CPU(s) with 4 core(s) each.
[DEBUG]  Supported C-states:  C0 C1 C1E C3 C6
[DEBUG]  PSS: 3201MHz power 77000 control 0x2400 status 0x2400
[DEBUG]  PSS: 3200MHz power 77000 control 0x2000 status 0x2000
[DEBUG]  PSS: 2800MHz power 64275 control 0x1c00 status 0x1c00
[DEBUG]  PSS: 2400MHz power 52610 control 0x1800 status 0x1800
[DEBUG]  PSS: 2000MHz power 41772 control 0x1400 status 0x1400
[DEBUG]  PSS: 1600MHz power 31801 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 3201MHz power 77000 control 0x2400 status 0x2400
[DEBUG]  PSS: 3200MHz power 77000 control 0x2000 status 0x2000
[DEBUG]  PSS: 2800MHz power 64275 control 0x1c00 status 0x1c00
[DEBUG]  PSS: 2400MHz power 52610 control 0x1800 status 0x1800
[DEBUG]  PSS: 2000MHz power 41772 control 0x1400 status 0x1400
[DEBUG]  PSS: 1600MHz power 31801 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 3201MHz power 77000 control 0x2400 status 0x2400
[DEBUG]  PSS: 3200MHz power 77000 control 0x2000 status 0x2000
[DEBUG]  PSS: 2800MHz power 64275 control 0x1c00 status 0x1c00
[DEBUG]  PSS: 2400MHz power 52610 control 0x1800 status 0x1800
[DEBUG]  PSS: 2000MHz power 41772 control 0x1400 status 0x1400
[DEBUG]  PSS: 1600MHz power 31801 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 3201MHz power 77000 control 0x2400 status 0x2400
[DEBUG]  PSS: 3200MHz power 77000 control 0x2000 status 0x2000
[DEBUG]  PSS: 2800MHz power 64275 control 0x1c00 status 0x1c00
[DEBUG]  PSS: 2400MHz power 52610 control 0x1800 status 0x1800
[DEBUG]  PSS: 2000MHz power 41772 control 0x1400 status 0x1400
[DEBUG]  PSS: 1600MHz power 31801 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PCI space above 4GB MMIO is at 0x67b600000, len = 0x984a00000
[DEBUG]  Generating ACPI PIRQ entries
[DEBUG]  \_SB.PCI0.LPCB.SIO0: PNP: 002e.ff
[INFO ]  \_SB_.PCI0.TPM: LPC TPM PNP: 004e.0
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L010: PNP: 002e.1
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L030: PNP: 002e.3
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L040: PNP: 002e.4
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L050: PNP: 002e.5
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L060: PNP: 002e.6
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L070: PNP: 002e.7
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L080: PNP: 002e.8
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L0F0: PNP: 002e.f
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L150: PNP: 002e.15
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L1C0: PNP: 002e.1c
[DEBUG]  \_SB.PCI0.LPCB.SIO0.L1E0: PNP: 002e.1e
[DEBUG]  ACPI:    * SSDT
[DEBUG]  ACPI: added table 2/32, length now 52
[DEBUG]  ACPI:    * MCFG
[DEBUG]  ACPI: added table 3/32, length now 60
[DEBUG]  TCPA log created at 0x7fe33000
[DEBUG]  ACPI:    * TCPA
[DEBUG]  ACPI: added table 4/32, length now 68
[DEBUG]  IOAPIC: 24 interrupts
[DEBUG]  ACPI:    * APIC
[DEBUG]  ACPI: added table 5/32, length now 76
[DEBUG]  ACPI:    * SPCR
[DEBUG]  ACPI: added table 6/32, length now 84
[DEBUG]  current = 7fe47bf0
[DEBUG]  ACPI:     * DMAR
[DEBUG]  ACPI: added table 7/32, length now 92
[DEBUG]  current = 7fe47cb0
[DEBUG]  ACPI:    * HPET
[DEBUG]  ACPI: added table 8/32, length now 100
[INFO ]  ACPI: done.
[DEBUG]  ACPI tables: 19696 bytes.
[DEBUG]  smbios_write_tables: 7fe2b000
[DEBUG]  SMBIOS firmware version is set to coreboot_version: '24.12-758-g1e7ba810c6bb'
[INFO ]  Create SMBIOS type 16
[INFO ]  Create SMBIOS type 17
[INFO ]  Create SMBIOS type 20
[INFO ]  Root Device (HP HP Compaq 8300 Elite SFF)
[DEBUG]  SMBIOS tables: 1358 bytes.
[DEBUG]  Writing table forward entry at 0x00000500
[DEBUG]  Wrote coreboot table at: 0x00000500, 0x10 bytes, checksum ff8
[DEBUG]  Writing coreboot table at 0x7fe67000
[DEBUG]   0. 0000000000000000-0000000000000fff: CONFIGURATION TABLES
[DEBUG]   1. 0000000000001000-000000000009ffff: RAM
[DEBUG]   2. 00000000000a0000-00000000000f5fff: RESERVED
[DEBUG]   3. 00000000000f6000-00000000000f6fff: CONFIGURATION TABLES
[DEBUG]   4. 00000000000f7000-00000000000fffff: RESERVED
[DEBUG]   5. 0000000000100000-000000007fe2afff: RAM
[DEBUG]   6. 000000007fe2b000-000000007fe82fff: CONFIGURATION TABLES
[DEBUG]   7. 000000007fe83000-000000007ffcdfff: RAMSTAGE
[DEBUG]   8. 000000007ffce000-000000007fffffff: CONFIGURATION TABLES
[DEBUG]   9. 0000000080000000-00000000829fffff: RESERVED
[DEBUG]  10. 00000000f0000000-00000000f3ffffff: RESERVED
[DEBUG]  11. 00000000fed40000-00000000fed44fff: RESERVED
[DEBUG]  12. 00000000fed90000-00000000fed91fff: RESERVED
[DEBUG]  13. 0000000100000000-000000067b5fffff: RAM
[DEBUG]  Wrote coreboot table at: 0x7fe67000, 0x400 bytes, checksum 329c
[DEBUG]  coreboot table: 1048 bytes.
[DEBUG]  IMD ROOT    0. 0x7ffff000 0x00001000
[DEBUG]  IMD SMALL   1. 0x7fffe000 0x00001000
[DEBUG]  CONSOLE     2. 0x7ffde000 0x00020000
[DEBUG]  RO MCACHE   3. 0x7ffdd000 0x00000344
[DEBUG]  TIME STAMP  4. 0x7ffdc000 0x00000910
[DEBUG]  MEM INFO    5. 0x7ffdb000 0x00000f48
[DEBUG]  AFTER CAR   6. 0x7ffce000 0x0000d000
[DEBUG]  RAMSTAGE    7. 0x7fe82000 0x0014c000
[DEBUG]  SMM BACKUP  8. 0x7fe72000 0x00010000
[DEBUG]  IGD OPREGION 9. 0x7fe6f000 0x00003000
[DEBUG]  COREBOOT   10. 0x7fe67000 0x00008000
[DEBUG]  ACPI       11. 0x7fe43000 0x00024000
[DEBUG]  TCPA TCGLOG12. 0x7fe33000 0x00010000
[DEBUG]  SMBIOS     13. 0x7fe2b000 0x00008000
[DEBUG]  IMD small region:
[DEBUG]    IMD ROOT    0. 0x7fffec00 0x00000400
[DEBUG]    FMAP        1. 0x7fffeb20 0x000000e0
[DEBUG]    ROMSTAGE    2. 0x7fffeb00 0x00000004
[DEBUG]    ROMSTG STCK 3. 0x7fffea40 0x000000a8
[DEBUG]    ACPI GNVS   4. 0x7fffe940 0x00000100
[DEBUG]  BS: BS_WRITE_TABLES run times (exec / console): 2 / 660 ms
[INFO ]  CBFS: Found 'fallback/payload' @0x4c440 size 0x11c5f in mcache @0x7ffdd280
[DEBUG]  Checking segment from ROM address 0xffaec66c
[DEBUG]  Payload being loaded at below 1MiB without region being marked as RAM usable.
[DEBUG]  Checking segment from ROM address 0xffaec688
[DEBUG]  Loading segment from ROM address 0xffaec66c
[DEBUG]    code (compression=1)
[DEBUG]    New segment dstaddr 0x000de1a0 memsize 0x21e60 srcaddr 0xffaec6a4 filesize 0x11c27
[DEBUG]  Loading Segment: addr: 0x000de1a0 memsz: 0x0000000000021e60 filesz: 0x0000000000011c27
[DEBUG]  using LZMA
[DEBUG]  Loading segment from ROM address 0xffaec688
[DEBUG]    Entry Point 0x000fd246
[DEBUG]  BS: BS_PAYLOAD_LOAD run times (exec / console): 19 / 66 ms
[DEBUG]  ICH-NM10-PCH: watchdog disabled
[DEBUG]  Jumping to boot code at 0x000fd246(0x7fe67000)
SeaBIOS (version rel-1.16.3-0-ga6ed6b70)
BUILD: gcc: (coreboot toolchain v2025-01-29_cdcd580bce) 14.2.0 binutils: (GNU Binutils) 2.43.1
SeaBIOS (version rel-1.16.3-0-ga6ed6b70)
BUILD: gcc: (coreboot toolchain v2025-01-29_cdcd580bce) 14.2.0 binutils: (GNU Binutils) 2.43.1
Found coreboot cbmem console @ 7ffde000
Found mainboard HP HP Compaq 8300 Elite SFF
Relocating init from 0x000df900 to 0x7ee1dc20 (size 54080)
Found CBFS header at 0xffaa022c
multiboot: eax=7febd8dc, ebx=7febd8a4
Found 12 PCI devices (max PCI bus is 02)
Copying SMBIOS from 0x7fe2b000 to 0x000f5b40
Copying SMBIOS 3.0 from 0x7fe2b020 to 0x000f5b20
Copying ACPI RSDP from 0x7fe43000 to 0x000f5af0
table(50434146)=0x7fe457d0 (via xsdt)
Using pmtimer, ioport 0x508
table(41504354)=0x7fe47ad0 (via xsdt)
Scan for VGA option rom
Running option rom at c000:0003
Start SeaVGABIOS (version rel-1.16.3-0-ga6ed6b70)
VGABUILD: gcc: (coreboot toolchain v2025-01-29_cdcd580bce) 14.2.0 binutils: (GNU Binutils) 2.43.1
enter vga_post:
   a=00000000  b=0000ffff  c=00000000  d=0000ffff ds=0000 es=f000 ss=0000
  si=00000000 di=000066e0 bp=00000000 sp=00006da2 cs=f000 ip=cff4  f=0000
coreboot vga init
Did not find coreboot framebuffer - assuming EGA text
Attempting to allocate 512 bytes lowmem via pmm call to f000:d06c
pmm call arg1=0
VGA stack allocated at ec180
Hooking hardware timer irq (old=f000fea5 new=c0003ef8)
Turning on vga text mode console
set VGA mode 3
SeaBIOS (version rel-1.16.3-0-ga6ed6b70)
PCI: XHCI at 00:14.0 (mmio 0xdfbd0000)
XHCI init: regs @ 0xdfbd0000, 8 ports, 32 slots, 32 byte contexts
XHCI    protocol USB  2.00, 4 ports (offset 1), def 3001
XHCI    protocol USB  3.00, 4 ports (offset 5), def 1000
XHCI    extcap 0xc1 @ 0xdfbd8040
XHCI    extcap 0xc0 @ 0xdfbd8070
XHCI    extcap 0x1 @ 0xdfbd8330
EHCI init on dev 00:1a.0 (regs=0xdfbc9020)
EHCI init on dev 00:1d.0 (regs=0xdfbc8020)
AHCI controller at 00:1f.2, iobase 0xdfbca000, irq 11
Searching bootorder for: HALT
Found 1 lpt ports
Found 1 serial ports
Got ps2 nak (status=51)
Searching bootorder for: /pci@i0cf8/*@1f,2/drive@2/disk@0
Searching bios-geometry for: /pci@i0cf8/*@1f,2/drive@2/disk@0
AHCI/2: registering: "DVD/CD [AHCI/2: hp       CDDVDW SH-216BB ATAPI-8 DVD/CD]"
XHCI no devices found
USB mouse initialized
USB keyboard initialized
ehci_wait_td error - status=80010d40
Searching bootorder for: /pci@i0cf8/usb@1d/hub@1/storage@3/*@0/*@0,0
Searching bootorder for: /pci@i0cf8/usb@1d/hub@1/usb-*@3
USB MSC vendor='JetFlash' product='Transcend 8GB' rev='8.07' type=0 removable=1
USB MSC blksize=512 sectors=15687680
Initialized USB HUB (1 ports used)
Initialized USB HUB (2 ports used)
Searching bootorder for: /pci@i0cf8/*@1f,2/drive@1/disk@0
AHCI/1: Set transfer mode to UDMA-5
Searching bios-geometry for: /pci@i0cf8/*@1f,2/drive@1/disk@0
AHCI/1: registering: "AHCI/1: WDC WD5000AAKX-60U6AA0 ATA-8 Hard-Disk (465 GiBytes)"
All threads complete.
Scan for option roms

Press ESC for boot menu.

Select boot device:

1. DVD/CD [AHCI/2: hp       CDDVDW SH-216BB ATAPI-8 DVD/CD]
2. AHCI/1: WDC WD5000AAKX-60U6AA0 ATA-8 Hard-Disk (465 GiBytes)
3. USB MSC Drive JetFlash Transcend 8GB 8.07

t. TPM Configuration
