

[NOTE ]  coreboot-25.03-250-g59e4095ecfcb-dirty Mon Apr 21 05:10:24 UTC 2025 x86_32 bootblock starting (log level: 8)...
[INFO ]  Timestamp - end of bootblock: 277129459
[INFO ]  Timestamp - start of romstage: 291600901
[DEBUG]  SMBus controller enabled
[INFO ]  Detected system type: desktop
[DEBUG]  Setting up static northbridge registers... done
[DEBUG]  Graphics ffff not supported by this CPU/chipset.
[DEBUG]  Initializing Graphics...
[SPEW ]  CBFS DEBUG: _cbfs_alloc(name='cmos_layout.bin', alloc=0x00000000(0x00000000), force_ro=true, type=-1)
[DEBUG]  FMAP: Found "FLASH" version 1.1 at 0x210000.
[DEBUG]  FMAP: base = 0x0 size = 0x800000 #areas = 4
[DEBUG]  FMAP: area COREBOOT found @ 210200 (6225408 bytes)
[SPEW ]  CBFS DEBUG: Looking for next file @0x0...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x0 (type 2, attr +0x0, data +0x2c, length 0x20)
[SPEW ]  CBFS DEBUG: File name: 'cbfs_master_header'
[SPEW ]  CBFS DEBUG: Looking for next file @0x4c...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x80 (type 83, attr +0x0, data +0x30, length 0x6800)
[SPEW ]  CBFS DEBUG: File name: 'cpu_microcode_blob.bin'
[SPEW ]  CBFS DEBUG: Looking for next file @0x68b0...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x68c0 (type 17, attr +0x2c, data +0x54, length 0x1fe6e)
[SPEW ]  CBFS DEBUG: File name: 'fallback/ramstage'
[SPEW ]  CBFS DEBUG: Looking for next file @0x26782...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x267c0 (type 80, attr +0x0, data +0x30, length 0x7200)
[SPEW ]  CBFS DEBUG: File name: 'vgaroms/seavgabios.bin'
[SPEW ]  CBFS DEBUG: Looking for next file @0x2d9f0...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x2da00 (type 80, attr +0x20, data +0x30, length 0xe80)
[SPEW ]  CBFS DEBUG: File name: 'config'
[SPEW ]  CBFS DEBUG: Looking for next file @0x2e8b0...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x2e8c0 (type 80, attr +0x0, data +0x24, length 0x2d7)
[SPEW ]  CBFS DEBUG: File name: 'revision'
[SPEW ]  CBFS DEBUG: Looking for next file @0x2ebbb...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x2ebc0 (type 80, attr +0x0, data +0x24, length 0x60)
[SPEW ]  CBFS DEBUG: File name: 'build_info'
[SPEW ]  CBFS DEBUG: Looking for next file @0x2ec44...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x2ec80 (type 80, attr +0x0, data +0x2c, length 0x2332)
[SPEW ]  CBFS DEBUG: File name: 'fallback/dsdt.aml'
[SPEW ]  CBFS DEBUG: Looking for next file @0x30fde...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x31000 (type 80, attr +0x20, data +0x30, length 0x4e1)
[SPEW ]  CBFS DEBUG: File name: 'vbt.bin'
[SPEW ]  CBFS DEBUG: Looking for next file @0x31511...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x31540 (type 170, attr +0x0, data +0x28, length 0x100)
[SPEW ]  CBFS DEBUG: File name: 'cmos.default'
[SPEW ]  CBFS DEBUG: Looking for next file @0x31668...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x31680 (type 426, attr +0x0, data +0x28, length 0x5ac)
[SPEW ]  CBFS DEBUG: File name: 'cmos_layout.bin'
[SPEW ]  CBFS DEBUG: Looking for next file @0x31c54...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x31c80 (type 17, attr +0x2c, data +0x44, length 0x81a8)
[SPEW ]  CBFS DEBUG: File name: 'fallback/postcar'
[SPEW ]  CBFS DEBUG: Looking for next file @0x39e6c...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x39e80 (type 32, attr +0x0, data +0x28, length 0xa9f0)
[SPEW ]  CBFS DEBUG: File name: 'img/coreinfo'
[SPEW ]  CBFS DEBUG: Looking for next file @0x44898...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x448c0 (type 32, attr +0x0, data +0x28, length 0xc6eb)
[SPEW ]  CBFS DEBUG: File name: 'img/nvramcui'
[SPEW ]  CBFS DEBUG: Looking for next file @0x50fd3...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x51000 (type 32, attr +0x0, data +0x2c, length 0x11c61)
[SPEW ]  CBFS DEBUG: File name: 'fallback/payload'
[SPEW ]  CBFS DEBUG: Looking for next file @0x62c8d...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x62cc0 (type 80, attr +0x0, data +0x28, length 0x6ae)
[SPEW ]  CBFS DEBUG: File name: 'payload_config'
[SPEW ]  CBFS DEBUG: Looking for next file @0x63396...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x633c0 (type 80, attr +0x0, data +0x2c, length 0xee)
[SPEW ]  CBFS DEBUG: File name: 'payload_revision'
[SPEW ]  CBFS DEBUG: Looking for next file @0x634da...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x63500 (type 80, attr +0x0, data +0x28, length 0x6e2)
[SPEW ]  CBFS DEBUG: File name: 'etc/grub.cfg'
[SPEW ]  CBFS DEBUG: Looking for next file @0x63c0a...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x63c40 (type 32, attr +0x0, data +0x24, length 0x80c95)
[SPEW ]  CBFS DEBUG: File name: 'img/grub2'
[SPEW ]  CBFS DEBUG: Looking for next file @0xe48f9...
[SPEW ]  CBFS DEBUG: Found CBFS header @0xe4900 (type 80, attr +0x0, data +0x28, length 0x8)
[SPEW ]  CBFS DEBUG: File name: 'etc/sercon-port'
[SPEW ]  CBFS DEBUG: Looking for next file @0xe4930...
[SPEW ]  CBFS DEBUG: Found CBFS header @0xe4940 (type -1, attr +0x0, data +0x1c, length 0x4f1464)
[SPEW ]  CBFS DEBUG: Looking for next file @0x5d5dc0...
[SPEW ]  CBFS DEBUG: Found CBFS header @0x5d5dc0 (type 1, attr +0x0, data +0x40, length 0x1a000)
[SPEW ]  CBFS DEBUG: File name: 'bootblock'
[SPEW ]  CBFS DEBUG: Looking for next file @0x5efe00...
[SPEW ]  CBFS DEBUG: End of CBFS reached
[INFO ]  CBFS: mcache @0xfeff0e00 built for 21 files, used 0x3d0 of 0x4000 bytes
[INFO ]  CBFS: Found 'cmos_layout.bin' @0x31680 size 0x5ac in mcache @0xfeff0fdc
[DEBUG]  Back from systemagent_early_init()
[INFO ]  POST: 0x38
[INFO ]  POST: 0x39
[INFO ]  POST: 0x3a
[INFO ]  Timestamp - before RAM initialization: 1796638646
[INFO ]  Intel ME early init
[INFO ]  Intel ME firmware is ready
[DEBUG]  ME: Requested 16MB UMA
[DEBUG]  Starting native Platform init
[DEBUG]  DMI: Running at X4 @ 5000MT/s
[DEBUG]  FMAP: area RW_MRC_CACHE found @ 200000 (65536 bytes)
[NOTE ]  MRC: no data in 'RW_MRC_CACHE'
[DEBUG]  ECC supported: no ECC forced: no
[INFO ]  ECC RAM unsupported.
[DEBUG]  SPD probe channel0, slot0
[DEBUG]  Not a DDR3 SPD!
[DEBUG]  No valid XMP profile found.
[DEBUG]  Not a DDR3 SPD!
[DEBUG]  SPD probe channel0, slot1
[DEBUG]    Revision           : 11
[DEBUG]    Type               : b
[DEBUG]    Key                : 2
[DEBUG]    Banks              : 8
[DEBUG]    Capacity           : 4 Gb
[DEBUG]    Supported voltages : 1.35V 1.5V
[DEBUG]    SDRAM width        : 8
[DEBUG]    Bus extension      : 0 bits
[DEBUG]    Bus width          : 64
[DEBUG]    FTB timings        : yes
[DEBUG]    Optional features  : DLL-Off_mode RZQ/7 RZQ/6
[DEBUG]    Thermal features   : PASR ext_temp_range
[DEBUG]    Thermal sensor     : no
[DEBUG]    Standard SDRAM     : yes
[DEBUG]    Rank1 Address bits : mirrored
[DEBUG]    DIMM Reference card: H
[DEBUG]    Manufacturer ID    : 9801
[DEBUG]    Part number        : 99U5471-050.A00L
[DEBUG]  Not a DDR3 XMP profile!
[DEBUG]  No valid XMP profile found.
[DEBUG]    Revision           : 11
[DEBUG]    Type               : b
[DEBUG]    Key                : 2
[DEBUG]    Banks              : 8
[DEBUG]    Capacity           : 4 Gb
[DEBUG]    Supported voltages : 1.35V 1.5V
[DEBUG]    SDRAM width        : 8
[DEBUG]    Bus extension      : 0 bits
[DEBUG]    Bus width          : 64
[DEBUG]    FTB timings        : yes
[DEBUG]    Optional features  : DLL-Off_mode RZQ/7 RZQ/6
[DEBUG]    Thermal features   : PASR ext_temp_range
[DEBUG]    Thermal sensor     : no
[DEBUG]    Standard SDRAM     : yes
[DEBUG]    Rank1 Address bits : mirrored
[DEBUG]    DIMM Reference card: H
[DEBUG]    Manufacturer ID    : 9801
[DEBUG]    Part number        : 99U5471-050.A00L
[INFO ]    Row    addr bits  : 16
[INFO ]    Column addr bits  : 10
[INFO ]    Number of ranks   : 2
[INFO ]    DIMM Capacity     : 8192 MB
[INFO ]    CAS latencies     : 6 7 8 9 10 11
[INFO ]    tCKmin            :   1.250 ns
[INFO ]    tAAmin            :  13.125 ns
[INFO ]    tWRmin            :  15.000 ns
[INFO ]    tRCDmin           :  13.125 ns
[INFO ]    tRRDmin           :   6.000 ns
[INFO ]    tRPmin            :  13.125 ns
[INFO ]    tRASmin           :  35.000 ns
[INFO ]    tRCmin            :  48.125 ns
[INFO ]    tRFCmin           : 260.000 ns
[INFO ]    tWTRmin           :   7.500 ns
[INFO ]    tRTPmin           :   7.500 ns
[INFO ]    tFAWmin           :  30.000 ns
[DEBUG]  channel[0] rankmap = 0xc
[DEBUG]  SPD probe channel1, slot0
[DEBUG]  Not a DDR3 SPD!
[DEBUG]  No valid XMP profile found.
[DEBUG]  Not a DDR3 SPD!
[DEBUG]  SPD probe channel1, slot1
[DEBUG]    Revision           : 11
[DEBUG]    Type               : b
[DEBUG]    Key                : 2
[DEBUG]    Banks              : 8
[DEBUG]    Capacity           : 4 Gb
[DEBUG]    Supported voltages : 1.35V 1.5V
[DEBUG]    SDRAM width        : 8
[DEBUG]    Bus extension      : 0 bits
[DEBUG]    Bus width          : 64
[DEBUG]    FTB timings        : yes
[DEBUG]    Optional features  : DLL-Off_mode RZQ/7 RZQ/6
[DEBUG]    Thermal features   : PASR ext_temp_range
[DEBUG]    Thermal sensor     : no
[DEBUG]    Standard SDRAM     : yes
[DEBUG]    Rank1 Address bits : mirrored
[DEBUG]    DIMM Reference card: H
[DEBUG]    Manufacturer ID    : 9801
[DEBUG]    Part number        : 99U5471-050.A00L
[DEBUG]  Not a DDR3 XMP profile!
[DEBUG]  No valid XMP profile found.
[DEBUG]    Revision           : 11
[DEBUG]    Type               : b
[DEBUG]    Key                : 2
[DEBUG]    Banks              : 8
[DEBUG]    Capacity           : 4 Gb
[DEBUG]    Supported voltages : 1.35V 1.5V
[DEBUG]    SDRAM width        : 8
[DEBUG]    Bus extension      : 0 bits
[DEBUG]    Bus width          : 64
[DEBUG]    FTB timings        : yes
[DEBUG]    Optional features  : DLL-Off_mode RZQ/7 RZQ/6
[DEBUG]    Thermal features   : PASR ext_temp_range
[DEBUG]    Thermal sensor     : no
[DEBUG]    Standard SDRAM     : yes
[DEBUG]    Rank1 Address bits : mirrored
[DEBUG]    DIMM Reference card: H
[DEBUG]    Manufacturer ID    : 9801
[DEBUG]    Part number        : 99U5471-050.A00L
[INFO ]    Row    addr bits  : 16
[INFO ]    Column addr bits  : 10
[INFO ]    Number of ranks   : 2
[INFO ]    DIMM Capacity     : 8192 MB
[INFO ]    CAS latencies     : 6 7 8 9 10 11
[INFO ]    tCKmin            :   1.250 ns
[INFO ]    tAAmin            :  13.125 ns
[INFO ]    tWRmin            :  15.000 ns
[INFO ]    tRCDmin           :  13.125 ns
[INFO ]    tRRDmin           :   6.000 ns
[INFO ]    tRPmin            :  13.125 ns
[INFO ]    tRASmin           :  35.000 ns
[INFO ]    tRCmin            :  48.125 ns
[INFO ]    tRFCmin           : 260.000 ns
[INFO ]    tWTRmin           :   7.500 ns
[INFO ]    tRTPmin           :   7.500 ns
[INFO ]    tFAWmin           :  30.000 ns
[DEBUG]  channel[1] rankmap = 0xc
[DEBUG]  ECC is disabled
[DEBUG]  Starting Ivy Bridge RAM training (full initialization).
[DEBUG]  100MHz reference clock support: yes
[DEBUG]  PLL_REF100_CFG value: 0x2
[DEBUG]  Trying CAS 11, tCK 320.
[DEBUG]  Found compatible clock, CAS pair.
[DEBUG]  Selected DRAM frequency: 800 MHz
[DEBUG]  Selected CAS latency   : 11T
[DEBUG]  MPLL busy... done in 10 us
[DEBUG]  MPLL frequency is set at : 800 MHz
[DEBUG]  Selected CWL latency   : 8T
[DEBUG]  Selected tRCD          : 11T
[DEBUG]  Selected tRP           : 11T
[DEBUG]  Selected tRAS          : 28T
[DEBUG]  Selected tWR           : 12T
[DEBUG]  Selected tFAW          : 24T
[DEBUG]  Selected tRRD          : 5T
[DEBUG]  Selected tRTP          : 6T
[DEBUG]  Selected tWTR          : 6T
[DEBUG]  Selected tRFC          : 208T
[DEBUG]  XOVER CLK [c14] = c000000
[DEBUG]  XOVER CMD [320c] = 4004000
[DEBUG]  XOVER CLK [d14] = c000000
[DEBUG]  XOVER CMD [330c] = 4004000
[DEBUG]  DBP [4000] = 1c8bbb
[DEBUG]  RAP [4004] = cc186465
[DEBUG]  OTHP [400c] = 58b4
[DEBUG]  OTHP [400c] = 58b4
[DEBUG]  REFI [4298] = 6cd01860
[DEBUG]  SRFTP [42a4] = 41f88200
[DEBUG]  DBP [4400] = 1c8bbb
[DEBUG]  RAP [4404] = cc186465
[DEBUG]  OTHP [440c] = 58b4
[DEBUG]  OTHP [440c] = 58b4
[DEBUG]  REFI [4698] = 6cd01860
[DEBUG]  SRFTP [46a4] = 41f88200
[DEBUG]  Done dimm mapping
[DEBUG]  Update PCI-E configuration space:
[DEBUG]  PCI(0, 0, 0)[a0] = 0
[DEBUG]  PCI(0, 0, 0)[a4] = 4
[DEBUG]  PCI(0, 0, 0)[bc] = 84a00000
[DEBUG]  PCI(0, 0, 0)[a8] = 7a600000
[DEBUG]  PCI(0, 0, 0)[ac] = 4
[DEBUG]  PCI(0, 0, 0)[b8] = 80000000
[DEBUG]  PCI(0, 0, 0)[b0] = 80a00000
[DEBUG]  PCI(0, 0, 0)[b4] = 80800000
[DEBUG]  PCI(0, 0, 0)[7c] = 7f
[DEBUG]  PCI(0, 0, 0)[70] = ff000000
[DEBUG]  PCI(0, 0, 0)[74] = 3
[DEBUG]  PCI(0, 0, 0)[78] = ff000c00
[DEBUG]  Done memory map
[DEBUG]  RCOMP...done
[DEBUG]  COMP2 done
[DEBUG]  COMP1 done
[DEBUG]  FORCE RCOMP and wait 20us...done
[DEBUG]  Done io registers
[DEBUG]  Done jedec reset
[DEBUG]  Done MRS commands
[DEBUG]  rcven: 0, 2, 0:    9-  38-  68
[DEBUG]  rcven: 0, 2, 1:   24-  53-  83
[DEBUG]  rcven: 0, 2, 2:   44-  75- 106
[DEBUG]  rcven: 0, 2, 3:   59-  90- 121
[DEBUG]  rcven: 0, 2, 4:   92- 121-  23
[DEBUG]  rcven: 0, 2, 5:  107-   7-  36
[DEBUG]  rcven: 0, 2, 6:    0-  26-  53
[DEBUG]  rcven: 0, 2, 7:   16-  46-  76
[DEBUG]  4024++;
[DEBUG]  4028++;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4028 += 2;
[DEBUG]  increment 0, 2, 5
[DEBUG]  increment 0, 2, 6
[DEBUG]  increment 0, 2, 7
[DEBUG]  4024 += 1;
[DEBUG]  4028 += 1;
[DEBUG]  lane 0: -3, 8
[DEBUG]  Aval: 0, 2, 0:   70
[DEBUG]  lane 1: -7, 4
[DEBUG]  Aval: 0, 2, 1:   82
[DEBUG]  lane 2: -4, 5
[DEBUG]  Aval: 0, 2, 2:  106
[DEBUG]  lane 3: -3, 5
[DEBUG]  Aval: 0, 2, 3:  122
[DEBUG]  lane 4: -5, 4
[DEBUG]  Aval: 0, 2, 4:  151
[DEBUG]  lane 5: -3, 7
[DEBUG]  Aval: 0, 2, 5:  166
[DEBUG]  lane 6: -1, 11
[DEBUG]  Aval: 0, 2, 6:  186
[DEBUG]  lane 7: -2, 7
[DEBUG]  Aval: 0, 2, 7:  206
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4028 -= 1;
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4/8: 0, 2,   49,    7
[DEBUG]  final results:
[DEBUG]  Aval: 0, 2, 0:    6
[DEBUG]  Aval: 0, 2, 1:   18
[DEBUG]  Aval: 0, 2, 2:   42
[DEBUG]  Aval: 0, 2, 3:   58
[DEBUG]  Aval: 0, 2, 4:   87
[DEBUG]  Aval: 0, 2, 5:  102
[DEBUG]  Aval: 0, 2, 6:  122
[DEBUG]  Aval: 0, 2, 7:  142
[DEBUG]  rcven: 0, 3, 0:    8-  39-  71
[DEBUG]  rcven: 0, 3, 1:   23-  54-  85
[DEBUG]  rcven: 0, 3, 2:   46-  76- 107
[DEBUG]  rcven: 0, 3, 3:   61-  91- 122
[DEBUG]  rcven: 0, 3, 4:   91- 120-  22
[DEBUG]  rcven: 0, 3, 5:  108-  11-  43
[DEBUG]  rcven: 0, 3, 6:  126-  28-  58
[DEBUG]  rcven: 0, 3, 7:   18-  47-  77
[DEBUG]  4024++;
[DEBUG]  4028++;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4028 += 2;
[DEBUG]  increment 0, 3, 5
[DEBUG]  increment 0, 3, 6
[DEBUG]  increment 0, 3, 7
[DEBUG]  4024 += 1;
[DEBUG]  4028 += 1;
[DEBUG]  lane 0: -5, 4
[DEBUG]  Aval: 0, 3, 0:   71
[DEBUG]  lane 1: -5, 4
[DEBUG]  Aval: 0, 3, 1:   85
[DEBUG]  lane 2: -4, 5
[DEBUG]  Aval: 0, 3, 2:  107
[DEBUG]  lane 3: -3, 5
[DEBUG]  Aval: 0, 3, 3:  123
[DEBUG]  lane 4: -3, 6
[DEBUG]  Aval: 0, 3, 4:  151
[DEBUG]  lane 5: -5, 5
[DEBUG]  Aval: 0, 3, 5:  171
[DEBUG]  lane 6: -2, 7
[DEBUG]  Aval: 0, 3, 6:  188
[DEBUG]  lane 7: -2, 9
[DEBUG]  Aval: 0, 3, 7:  208
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4028 -= 1;
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4/8: 0, 3,   49,    7
[DEBUG]  final results:
[DEBUG]  Aval: 0, 3, 0:    7
[DEBUG]  Aval: 0, 3, 1:   21
[DEBUG]  Aval: 0, 3, 2:   43
[DEBUG]  Aval: 0, 3, 3:   59
[DEBUG]  Aval: 0, 3, 4:   87
[DEBUG]  Aval: 0, 3, 5:  107
[DEBUG]  Aval: 0, 3, 6:  124
[DEBUG]  Aval: 0, 3, 7:  144
[DEBUG]  rcven: 1, 2, 0:   47-  75- 104
[DEBUG]  rcven: 1, 2, 1:   61-  91- 121
[DEBUG]  rcven: 1, 2, 2:   84- 116-  20
[DEBUG]  rcven: 1, 2, 3:   96- 127-  31
[DEBUG]  rcven: 1, 2, 4:    1-  33-  66
[DEBUG]  rcven: 1, 2, 5:   18-  49-  81
[DEBUG]  rcven: 1, 2, 6:   36-  68- 100
[DEBUG]  rcven: 1, 2, 7:   52-  84- 116
[DEBUG]  4024++;
[DEBUG]  4028++;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4028 += 2;
[DEBUG]  increment 1, 2, 4
[DEBUG]  increment 1, 2, 5
[DEBUG]  increment 1, 2, 6
[DEBUG]  increment 1, 2, 7
[DEBUG]  4024 += 1;
[DEBUG]  4028 += 1;
[DEBUG]  lane 0: -2, 9
[DEBUG]  Aval: 1, 2, 0:  107
[DEBUG]  lane 1: -2, 6
[DEBUG]  Aval: 1, 2, 1:  123
[DEBUG]  lane 2: -8, 1
[DEBUG]  Aval: 1, 2, 2:  145
[DEBUG]  lane 3: -5, 4
[DEBUG]  Aval: 1, 2, 3:  159
[DEBUG]  lane 4: -9, 1
[DEBUG]  Aval: 1, 2, 4:  190
[DEBUG]  lane 5: -9, 1
[DEBUG]  Aval: 1, 2, 5:  205
[DEBUG]  lane 6: -6, 4
[DEBUG]  Aval: 1, 2, 6:  227
[DEBUG]  lane 7: -6, 4
[DEBUG]  Aval: 1, 2, 7:  243
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4028 -= 1;
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4/8: 1, 2,   49,    7
[DEBUG]  final results:
[DEBUG]  Aval: 1, 2, 0:   43
[DEBUG]  Aval: 1, 2, 1:   59
[DEBUG]  Aval: 1, 2, 2:   81
[DEBUG]  Aval: 1, 2, 3:   95
[DEBUG]  Aval: 1, 2, 4:  126
[DEBUG]  Aval: 1, 2, 5:  141
[DEBUG]  Aval: 1, 2, 6:  163
[DEBUG]  Aval: 1, 2, 7:  179
[DEBUG]  rcven: 1, 3, 0:   44-  76- 109
[DEBUG]  rcven: 1, 3, 1:   65-  95- 126
[DEBUG]  rcven: 1, 3, 2:   84- 114-  17
[DEBUG]  rcven: 1, 3, 3:  100-   1-  31
[DEBUG]  rcven: 1, 3, 4:    4-  35-  66
[DEBUG]  rcven: 1, 3, 5:   16-  47-  79
[DEBUG]  rcven: 1, 3, 6:   42-  72- 102
[DEBUG]  rcven: 1, 3, 7:   54-  84- 114
[DEBUG]  4024++;
[DEBUG]  4028++;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4024 -= 2;
[DEBUG]  4028 += 2;
[DEBUG]  increment 1, 3, 3
[DEBUG]  increment 1, 3, 4
[DEBUG]  increment 1, 3, 5
[DEBUG]  increment 1, 3, 6
[DEBUG]  increment 1, 3, 7
[DEBUG]  4024 += 1;
[DEBUG]  4028 += 1;
[DEBUG]  lane 0: -7, 4
[DEBUG]  Aval: 1, 3, 0:  108
[DEBUG]  lane 1: -7, 3
[DEBUG]  Aval: 1, 3, 1:  124
[DEBUG]  lane 2: -7, 4
[DEBUG]  Aval: 1, 3, 2:  144
[DEBUG]  lane 3: -4, 5
[DEBUG]  Aval: 1, 3, 3:  159
[DEBUG]  lane 4: -6, 5
[DEBUG]  Aval: 1, 3, 4:  194
[DEBUG]  lane 5: -7, 4
[DEBUG]  Aval: 1, 3, 5:  206
[DEBUG]  lane 6: -4, 6
[DEBUG]  Aval: 1, 3, 6:  231
[DEBUG]  lane 7: -7, 5
[DEBUG]  Aval: 1, 3, 7:  241
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4028 -= 1;
[DEBUG]  4024 += 0;
[DEBUG]  4028 += 0;
[DEBUG]  4/8: 1, 3,   49,    7
[DEBUG]  final results:
[DEBUG]  Aval: 1, 3, 0:   44
[DEBUG]  Aval: 1, 3, 1:   60
[DEBUG]  Aval: 1, 3, 2:   80
[DEBUG]  Aval: 1, 3, 3:   95
[DEBUG]  Aval: 1, 3, 4:  130
[DEBUG]  Aval: 1, 3, 5:  142
[DEBUG]  Aval: 1, 3, 6:  167
[DEBUG]  Aval: 1, 3, 7:  177
[DEBUG]  discover falling edges:
[DEBUG]  [4eb0] = 300
[DEBUG]  eval 0, 2, 0:   42
[DEBUG]  eval 0, 2, 1:   39
[DEBUG]  eval 0, 2, 2:   41
[DEBUG]  eval 0, 2, 3:   41
[DEBUG]  eval 0, 2, 4:   39
[DEBUG]  eval 0, 2, 5:   40
[DEBUG]  eval 0, 2, 6:   39
[DEBUG]  eval 0, 2, 7:   41
[DEBUG]  eval 0, 3, 0:   41
[DEBUG]  eval 0, 3, 1:   40
[DEBUG]  eval 0, 3, 2:   41
[DEBUG]  eval 0, 3, 3:   40
[DEBUG]  eval 0, 3, 4:   40
[DEBUG]  eval 0, 3, 5:   39
[DEBUG]  eval 0, 3, 6:   40
[DEBUG]  eval 0, 3, 7:   41
[DEBUG]  eval 1, 2, 0:   43
[DEBUG]  eval 1, 2, 1:   43
[DEBUG]  eval 1, 2, 2:   43
[DEBUG]  eval 1, 2, 3:   43
[DEBUG]  eval 1, 2, 4:   41
[DEBUG]  eval 1, 2, 5:   42
[DEBUG]  eval 1, 2, 6:   41
[DEBUG]  eval 1, 2, 7:   42
[DEBUG]  eval 1, 3, 0:   44
[DEBUG]  eval 1, 3, 1:   42
[DEBUG]  eval 1, 3, 2:   42
[DEBUG]  eval 1, 3, 3:   41
[DEBUG]  eval 1, 3, 4:   41
[DEBUG]  eval 1, 3, 5:   41
[DEBUG]  eval 1, 3, 6:   41
[DEBUG]  eval 1, 3, 7:   41
[DEBUG]  discover rising edges:
[DEBUG]  [4eb0] = 200
[DEBUG]  eval 0, 2, 0:   40
[DEBUG]  eval 0, 2, 1:   39
[DEBUG]  eval 0, 2, 2:   40
[DEBUG]  eval 0, 2, 3:   41
[DEBUG]  eval 0, 2, 4:   39
[DEBUG]  eval 0, 2, 5:   38
[DEBUG]  eval 0, 2, 6:   37
[DEBUG]  eval 0, 2, 7:   39
[DEBUG]  eval 0, 3, 0:   39
[DEBUG]  eval 0, 3, 1:   38
[DEBUG]  eval 0, 3, 2:   39
[DEBUG]  eval 0, 3, 3:   41
[DEBUG]  eval 0, 3, 4:   39
[DEBUG]  eval 0, 3, 5:   38
[DEBUG]  eval 0, 3, 6:   38
[DEBUG]  eval 0, 3, 7:   39
[DEBUG]  eval 1, 2, 0:   43
[DEBUG]  eval 1, 2, 1:   40
[DEBUG]  eval 1, 2, 2:   42
[DEBUG]  eval 1, 2, 3:   43
[DEBUG]  eval 1, 2, 4:   41
[DEBUG]  eval 1, 2, 5:   41
[DEBUG]  eval 1, 2, 6:   39
[DEBUG]  eval 1, 2, 7:   43
[DEBUG]  eval 1, 3, 0:   41
[DEBUG]  eval 1, 3, 1:   41
[DEBUG]  eval 1, 3, 2:   42
[DEBUG]  eval 1, 3, 3:   41
[DEBUG]  eval 1, 3, 4:   41
[DEBUG]  eval 1, 3, 5:   42
[DEBUG]  eval 1, 3, 6:   41
[DEBUG]  eval 1, 3, 7:   43
[DEBUG]  CPE
[DEBUG]  tx_dqs: 0, 2, 0:   68-  97- 126
[DEBUG]  tx_dqs: 0, 2, 1:   91- 122-  26
[DEBUG]  tx_dqs: 0, 2, 2:  121-  24-  56
[DEBUG]  tx_dqs: 0, 2, 3:    5-  36-  67
[DEBUG]  tx_dqs: 0, 2, 4:   32-  63-  94
[DEBUG]  tx_dqs: 0, 2, 5:   41-  72- 104
[DEBUG]  tx_dqs: 0, 2, 6:   49-  80- 112
[DEBUG]  tx_dqs: 0, 2, 7:   57-  88- 120
[DEBUG]  tx_dqs: 0, 3, 0:   64-  94- 124
[DEBUG]  tx_dqs: 0, 3, 1:   95- 126-  30
[DEBUG]  tx_dqs: 0, 3, 2:  117-  22-  55
[DEBUG]  tx_dqs: 0, 3, 3:    9-  39-  69
[DEBUG]  tx_dqs: 0, 3, 4:   32-  63-  95
[DEBUG]  tx_dqs: 0, 3, 5:   44-  74- 104
[DEBUG]  tx_dqs: 0, 3, 6:   51-  82- 113
[DEBUG]  tx_dqs: 0, 3, 7:   57-  87- 118
[DEBUG]  tx_dqs: 1, 2, 0:   70-  95- 121
[DEBUG]  tx_dqs: 1, 2, 1:   85- 118-  24
[DEBUG]  tx_dqs: 1, 2, 2:  115-  20-  54
[DEBUG]  tx_dqs: 1, 2, 3:    5-  35-  66
[DEBUG]  tx_dqs: 1, 2, 4:   30-  61-  92
[DEBUG]  tx_dqs: 1, 2, 5:   44-  75- 106
[DEBUG]  tx_dqs: 1, 2, 6:   42-  73- 104
[DEBUG]  tx_dqs: 1, 2, 7:   60-  91- 123
[DEBUG]  tx_dqs: 1, 3, 0:   67-  97-   0
[DEBUG]  tx_dqs: 1, 3, 1:   92- 123-  26
[DEBUG]  tx_dqs: 1, 3, 2:  121-  23-  54
[DEBUG]  tx_dqs: 1, 3, 3:    3-  34-  66
[DEBUG]  tx_dqs: 1, 3, 4:   33-  64-  95
[DEBUG]  tx_dqs: 1, 3, 5:   47-  78- 110
[DEBUG]  tx_dqs: 1, 3, 6:   54-  84- 114
[DEBUG]  tx_dqs: 1, 3, 7:   64-  94- 125
[DEBUG]  CPF
[DEBUG]  tx_dq: 0, 2, 0:    8-  35-  63
[DEBUG]  tx_dq: 0, 2, 1:   29-  56-  84
[DEBUG]  tx_dq: 0, 2, 2:   56-  85- 114
[DEBUG]  tx_dq: 0, 2, 3:    6-  33-  60
[DEBUG]  tx_dq: 0, 2, 4:   33-  61-  89
[DEBUG]  tx_dq: 0, 2, 5:   46-  74- 102
[DEBUG]  tx_dq: 0, 2, 6:   54-  81- 108
[DEBUG]  tx_dq: 0, 2, 7:   60-  88- 116
[DEBUG]  tx_dq: 0, 3, 0:    3-  30-  57
[DEBUG]  tx_dq: 0, 3, 1:   32-  59-  87
[DEBUG]  tx_dq: 0, 3, 2:   52-  81- 110
[DEBUG]  tx_dq: 0, 3, 3:   11-  37-  64
[DEBUG]  tx_dq: 0, 3, 4:   34-  61-  89
[DEBUG]  tx_dq: 0, 3, 5:   49-  76- 104
[DEBUG]  tx_dq: 0, 3, 6:   56-  83- 110
[DEBUG]  tx_dq: 0, 3, 7:   60-  87- 115
[DEBUG]  tx_dq: 1, 2, 0:    6-  34-  62
[DEBUG]  tx_dq: 1, 2, 1:   25-  51-  78
[DEBUG]  tx_dq: 1, 2, 2:   56-  82- 108
[DEBUG]  tx_dq: 1, 2, 3:    6-  33-  61
[DEBUG]  tx_dq: 1, 2, 4:   31-  59-  87
[DEBUG]  tx_dq: 1, 2, 5:   47-  71-  96
[DEBUG]  tx_dq: 1, 2, 6:   44-  71-  98
[DEBUG]  tx_dq: 1, 2, 7:   63-  89- 116
[DEBUG]  tx_dq: 1, 3, 0:    4-  31-  59
[DEBUG]  tx_dq: 1, 3, 1:   32-  58-  85
[DEBUG]  tx_dq: 1, 3, 2:   62-  87- 113
[DEBUG]  tx_dq: 1, 3, 3:    4-  31-  59
[DEBUG]  tx_dq: 1, 3, 4:   36-  62-  89
[DEBUG]  tx_dq: 1, 3, 5:   49-  75- 102
[DEBUG]  tx_dq: 1, 3, 6:   56-  83- 110
[DEBUG]  tx_dq: 1, 3, 7:    4-  30-  56
[DEBUG]  High adjust 0:0000ffffffffffff
[DEBUG]  Bval+: 0, 2, 0,   68 ->  196
[DEBUG]  High adjust 1:0000ffffffffffff
[DEBUG]  Bval+: 0, 2, 1,   91 ->  219
[DEBUG]  High adjust 2:0000ffffffffffff
[DEBUG]  Bval+: 0, 2, 2,  121 ->  249
[DEBUG]  High adjust 3:00000000ffffffff
[DEBUG]  Bval+: 0, 2, 3,    5 ->  261
[DEBUG]  High adjust 4:00000000ffffffff
[DEBUG]  Bval+: 0, 2, 4,   32 ->  288
[DEBUG]  High adjust 5:00000000ffffffff
[DEBUG]  Bval+: 0, 2, 5,   41 ->  297
[DEBUG]  High adjust 6:00000000ffffffff
[DEBUG]  Bval+: 0, 2, 6,   49 ->  305
[DEBUG]  High adjust 7:00000000ffffffff
[DEBUG]  Bval+: 0, 2, 7,   57 ->  313
[DEBUG]  High adjust 0:0000ffffffffffff
[DEBUG]  Bval+: 0, 3, 0,   64 ->  192
[DEBUG]  High adjust 1:0000ffffffffffff
[DEBUG]  Bval+: 0, 3, 1,   95 ->  223
[DEBUG]  High adjust 2:0000ffffffffffff
[DEBUG]  Bval+: 0, 3, 2,  117 ->  245
[DEBUG]  High adjust 3:00000000ffffffff
[DEBUG]  Bval+: 0, 3, 3,    9 ->  265
[DEBUG]  High adjust 4:00000000ffffffff
[DEBUG]  Bval+: 0, 3, 4,   32 ->  288
[DEBUG]  High adjust 5:00000000ffffffff
[DEBUG]  Bval+: 0, 3, 5,   44 ->  300
[DEBUG]  High adjust 6:00000000ffffffff
[DEBUG]  Bval+: 0, 3, 6,   51 ->  307
[DEBUG]  High adjust 7:00000000ffffffff
[DEBUG]  Bval+: 0, 3, 7,   57 ->  313
[DEBUG]  High adjust 0:0000ffffffffffff
[DEBUG]  Bval+: 1, 2, 0,   70 ->  198
[DEBUG]  High adjust 1:0000ffffffffffff
[DEBUG]  Bval+: 1, 2, 1,   85 ->  213
[DEBUG]  High adjust 2:0000ffffffffffff
[DEBUG]  Bval+: 1, 2, 2,  115 ->  243
[DEBUG]  High adjust 3:00000000ffffffff
[DEBUG]  Bval+: 1, 2, 3,    5 ->  261
[DEBUG]  High adjust 4:00000000ffffffff
[DEBUG]  Bval+: 1, 2, 4,   30 ->  286
[DEBUG]  High adjust 5:00000000ffffffff
[DEBUG]  Bval+: 1, 2, 5,   44 ->  300
[DEBUG]  High adjust 6:00000000ffffffff
[DEBUG]  Bval+: 1, 2, 6,   42 ->  298
[DEBUG]  High adjust 7:00000000ffffffff
[DEBUG]  Bval+: 1, 2, 7,   60 ->  316
[DEBUG]  High adjust 0:0000ffffffffffff
[DEBUG]  Bval+: 1, 3, 0,   67 ->  195
[DEBUG]  High adjust 1:0000ffffffffffff
[DEBUG]  Bval+: 1, 3, 1,   92 ->  220
[DEBUG]  High adjust 2:0000ffffffffffff
[DEBUG]  Bval+: 1, 3, 2,  121 ->  249
[DEBUG]  High adjust 3:00000000ffffffff
[DEBUG]  Bval+: 1, 3, 3,    3 ->  259
[DEBUG]  High adjust 4:00000000ffffffff
[DEBUG]  Bval+: 1, 3, 4,   33 ->  289
[DEBUG]  High adjust 5:00000000ffffffff
[DEBUG]  Bval+: 1, 3, 5,   47 ->  303
[DEBUG]  High adjust 6:00000000ffffffff
[DEBUG]  Bval+: 1, 3, 6,   54 ->  310
[DEBUG]  High adjust 7:00000000ffffffff
[DEBUG]  Bval+: 1, 3, 7,   64 ->  320
[DEBUG]  CP5a
[DEBUG]  CP5b
[DEBUG]  Trying cmd_stretch 0 on channel 0
[DEBUG]  cmd_stretch: 0, 2:   78- 124- 170
[DEBUG]  cmd_stretch: 0, 3:   76- 123- 170
[DEBUG]  Using CMD rate 1T on channel 0
[DEBUG]  Trying cmd_stretch 0 on channel 1
[DEBUG]  cmd_stretch: 1, 2:   80- 125- 171
[DEBUG]  cmd_stretch: 1, 3:   78- 122- 167
[DEBUG]  Using CMD rate 1T on channel 1
[DEBUG]  CP5c
[DEBUG]  discover falling edges aggressive:
[DEBUG]  [4eb0] = 300
[DEBUG]  [3000] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 0, 2, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 2, 0:   15-  40-  66,   28-  53
[DEBUG]  edges: 0, 2, 0:   15-  40-  66,   28-  53
[DEBUG]  edges: 0, 2, 0:   13-  37-  62,   26-  49
[DEBUG]  edges: 0, 2, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 2, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 0, 2, 0:   15-  38-  62,   28-  49
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 2, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 2, 0:   14-  39-  64,   27-  51
[DEBUG]  edges: 0, 2, 0:   14-  39-  64,   27-  51
[DEBUG]  edges: 0, 2, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 2, 0:   14-  37-  61,   27-  48
[DEBUG]  edges: 0, 2, 0:   16-  41-  67,   29-  54
[DEBUG]  edges: 0, 2, 0:   15-  41-  67,   28-  54
[DEBUG]  edges: 0, 2, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 2, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 2, 0:   16-  38-  60,   29-  47
[DEBUG]  edges: 0, 2, 0:   15-  37-  60,   28-  47
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 2, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 2, 0:   16-  41-  66,   29-  53
[DEBUG]  edges: 0, 2, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 2, 0:   13-  37-  62,   26-  49
[DEBUG]  edges: 0, 2, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  [3000] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 2, 1:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 2, 1:   20-  41-  63,   25-  58
[DEBUG]  edges: 0, 2, 1:   20-  41-  62,   25-  57
[DEBUG]  edges: 0, 2, 1:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 2, 1:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 2, 1:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 2, 1:   18-  36-  55,   23-  50
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 1:   22-  40-  59,   27-  54
[DEBUG]  edges: 0, 2, 1:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 2, 1:   21-  41-  62,   26-  57
[DEBUG]  edges: 0, 2, 1:   20-  40-  61,   25-  56
[DEBUG]  edges: 0, 2, 1:   17-  39-  61,   22-  56
[DEBUG]  edges: 0, 2, 1:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 1:   18-  39-  60,   23-  55
[DEBUG]  edges: 0, 2, 1:   18-  38-  59,   23-  54
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 1:   22-  42-  62,   27-  57
[DEBUG]  edges: 0, 2, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 1:   21-  42-  64,   26-  59
[DEBUG]  edges: 0, 2, 1:   20-  41-  63,   25-  58
[DEBUG]  edges: 0, 2, 1:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 2, 1:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 1:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 2, 1:   17-  36-  56,   22-  51
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 1:   22-  42-  63,   27-  58
[DEBUG]  edges: 0, 2, 1:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 1:   21-  42-  63,   26-  58
[DEBUG]  edges: 0, 2, 1:   19-  41-  63,   24-  58
[DEBUG]  edges: 0, 2, 1:   17-  39-  62,   22-  57
[DEBUG]  edges: 0, 2, 1:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 2, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 2, 1:   18-  39-  61,   23-  56
[DEBUG]  [3000] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 2:   20-  41-  62,   25-  57
[DEBUG]  edges: 0, 2, 2:   20-  41-  62,   25-  57
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 2:   19-  37-  55,   24-  50
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 2:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 2, 2:   18-  37-  57,   23-  52
[DEBUG]  edges: 0, 2, 2:   21-  40-  59,   26-  54
[DEBUG]  edges: 0, 2, 2:   20-  40-  60,   25-  55
[DEBUG]  edges: 0, 2, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 2:   20-  38-  56,   25-  51
[DEBUG]  edges: 0, 2, 2:   20-  38-  56,   25-  51
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 2:   21-  40-  60,   26-  55
[DEBUG]  edges: 0, 2, 2:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 2, 2:   21-  42-  63,   26-  58
[DEBUG]  edges: 0, 2, 2:   21-  41-  62,   26-  57
[DEBUG]  edges: 0, 2, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 2:   18-  34-  51,   23-  46
[DEBUG]  edges: 0, 2, 2:   21-  37-  54,   26-  49
[DEBUG]  edges: 0, 2, 2:   21-  37-  54,   26-  49
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 2:   21-  41-  62,   26-  57
[DEBUG]  edges: 0, 2, 2:   19-  37-  56,   24-  51
[DEBUG]  edges: 0, 2, 2:   20-  41-  63,   25-  58
[DEBUG]  edges: 0, 2, 2:   20-  39-  59,   25-  54
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 2:   18-  38-  58,   23-  53
[DEBUG]  edges: 0, 2, 2:   21-  39-  57,   26-  52
[DEBUG]  edges: 0, 2, 2:   21-  40-  59,   26-  54
[DEBUG]  CPA
[DEBUG]  [3000] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 0, 3, 0:   14-  38-  63,   27-  50
[DEBUG]  edges: 0, 3, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 0, 3, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 3, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 0, 3, 0:   13-  37-  62,   26-  49
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 3, 0:   15-  40-  65,   28-  52
[DEBUG]  edges: 0, 3, 0:   15-  40-  65,   28-  52
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   14-  39-  64,   27-  51
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 0:   16-  40-  65,   29-  52
[DEBUG]  edges: 0, 3, 0:   14-  39-  64,   27-  51
[DEBUG]  edges: 0, 3, 0:   15-  40-  65,   28-  52
[DEBUG]  edges: 0, 3, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 3, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 0, 3, 0:   14-  38-  62,   27-  49
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 0, 3, 0:   14-  39-  64,   27-  51
[DEBUG]  edges: 0, 3, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 3, 0:   13-  38-  63,   26-  50
[DEBUG]  edges: 0, 3, 0:   16-  39-  63,   29-  50
[DEBUG]  edges: 0, 3, 0:   14-  39-  64,   27-  51
[DEBUG]  [3000] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 1:   20-  39-  59,   25-  54
[DEBUG]  edges: 0, 3, 1:   17-  38-  60,   22-  55
[DEBUG]  edges: 0, 3, 1:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 1:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 3, 1:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 3, 1:   18-  36-  55,   23-  50
[DEBUG]  edges: 0, 3, 1:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 3, 1:   17-  37-  57,   22-  52
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 1:   22-  41-  61,   27-  56
[DEBUG]  edges: 0, 3, 1:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 1:   20-  40-  61,   25-  56
[DEBUG]  edges: 0, 3, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 3, 1:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 3, 1:   19-  37-  55,   24-  50
[DEBUG]  edges: 0, 3, 1:   18-  40-  62,   23-  57
[DEBUG]  edges: 0, 3, 1:   18-  38-  59,   23-  54
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 1:   21-  41-  62,   26-  57
[DEBUG]  edges: 0, 3, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 1:   20-  40-  61,   25-  56
[DEBUG]  edges: 0, 3, 1:   20-  40-  61,   25-  56
[DEBUG]  edges: 0, 3, 1:   17-  39-  61,   22-  56
[DEBUG]  edges: 0, 3, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 1:   17-  39-  61,   22-  56
[DEBUG]  edges: 0, 3, 1:   17-  38-  59,   22-  54
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 1:   22-  42-  62,   27-  57
[DEBUG]  edges: 0, 3, 1:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 3, 1:   20-  41-  62,   25-  57
[DEBUG]  edges: 0, 3, 1:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 3, 1:   17-  39-  61,   22-  56
[DEBUG]  edges: 0, 3, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 1:   17-  39-  62,   22-  57
[DEBUG]  [3000] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 2:   18-  37-  57,   23-  52
[DEBUG]  edges: 0, 3, 2:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 3, 2:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 3, 2:   20-  39-  59,   25-  54
[DEBUG]  edges: 0, 3, 2:   19-  37-  56,   24-  51
[DEBUG]  edges: 0, 3, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 3, 2:   20-  38-  57,   25-  52
[DEBUG]  edges: 0, 3, 2:   18-  38-  58,   23-  53
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 2:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 2:   19-  39-  60,   24-  55
[DEBUG]  edges: 0, 3, 2:   21-  40-  59,   26-  54
[DEBUG]  edges: 0, 3, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 3, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 3, 2:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 2:   19-  39-  60,   24-  55
[DEBUG]  edges: 0, 3, 2:   18-  37-  57,   23-  52
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 2:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 3, 2:   20-  40-  60,   25-  55
[DEBUG]  edges: 0, 3, 2:   20-  40-  60,   25-  55
[DEBUG]  edges: 0, 3, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 3, 2:   18-  36-  55,   23-  50
[DEBUG]  edges: 0, 3, 2:   21-  38-  56,   26-  51
[DEBUG]  edges: 0, 3, 2:   18-  37-  56,   23-  51
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 2:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 2:   18-  39-  61,   23-  56
[DEBUG]  edges: 0, 3, 2:   19-  41-  63,   24-  58
[DEBUG]  edges: 0, 3, 2:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 3, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 3, 2:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 2:   20-  40-  61,   25-  56
[DEBUG]  edges: 0, 3, 2:   18-  38-  59,   23-  54
[DEBUG]  CPA
[DEBUG]  [3100] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 2, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   17-  41-  66,   30-  53
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   16-  37-  59,   29-  46
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 0:   18-  40-  63,   31-  50
[DEBUG]  edges: 1, 2, 0:   20-  41-  63,   33-  50
[DEBUG]  edges: 1, 2, 0:   18-  41-  64,   31-  51
[DEBUG]  edges: 1, 2, 0:   18-  41-  65,   31-  52
[DEBUG]  edges: 1, 2, 0:   18-  40-  62,   31-  49
[DEBUG]  edges: 1, 2, 0:   19-  39-  60,   32-  47
[DEBUG]  edges: 1, 2, 0:   16-  36-  57,   29-  44
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 0:   19-  40-  62,   32-  49
[DEBUG]  edges: 1, 2, 0:   19-  41-  64,   32-  51
[DEBUG]  edges: 1, 2, 0:   18-  40-  63,   31-  50
[DEBUG]  edges: 1, 2, 0:   17-  41-  65,   30-  52
[DEBUG]  edges: 1, 2, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 2, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 2, 0:   16-  37-  58,   29-  45
[DEBUG]  edges: 1, 2, 0:   17-  38-  59,   30-  46
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 0:   18-  41-  64,   31-  51
[DEBUG]  edges: 1, 2, 0:   18-  41-  65,   31-  52
[DEBUG]  edges: 1, 2, 0:   18-  41-  64,   31-  51
[DEBUG]  edges: 1, 2, 0:   18-  41-  65,   31-  52
[DEBUG]  edges: 1, 2, 0:   18-  41-  64,   31-  51
[DEBUG]  edges: 1, 2, 0:   18-  38-  59,   31-  46
[DEBUG]  edges: 1, 2, 0:   16-  38-  60,   29-  47
[DEBUG]  edges: 1, 2, 0:   17-  38-  60,   30-  47
[DEBUG]  [3100] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 2, 1:   24-  43-  62,   29-  57
[DEBUG]  edges: 1, 2, 1:   24-  43-  62,   29-  57
[DEBUG]  edges: 1, 2, 1:   23-  43-  63,   28-  58
[DEBUG]  edges: 1, 2, 1:   23-  40-  58,   28-  53
[DEBUG]  edges: 1, 2, 1:   24-  41-  58,   29-  53
[DEBUG]  edges: 1, 2, 1:   20-  38-  56,   25-  51
[DEBUG]  edges: 1, 2, 1:   23-  39-  56,   28-  51
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 1:   26-  44-  62,   31-  57
[DEBUG]  edges: 1, 2, 1:   27-  43-  60,   32-  55
[DEBUG]  edges: 1, 2, 1:   26-  43-  61,   31-  56
[DEBUG]  edges: 1, 2, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 1:   22-  37-  53,   27-  48
[DEBUG]  edges: 1, 2, 1:   23-  37-  52,   28-  47
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 1:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 2, 1:   25-  43-  62,   30-  57
[DEBUG]  edges: 1, 2, 1:   24-  43-  62,   29-  57
[DEBUG]  edges: 1, 2, 1:   24-  42-  61,   29-  56
[DEBUG]  edges: 1, 2, 1:   24-  41-  58,   29-  53
[DEBUG]  edges: 1, 2, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 1:   21-  38-  56,   26-  51
[DEBUG]  edges: 1, 2, 1:   23-  38-  54,   28-  49
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 2, 1:   25-  44-  63,   30-  58
[DEBUG]  edges: 1, 2, 1:   25-  44-  63,   30-  58
[DEBUG]  edges: 1, 2, 1:   24-  43-  63,   29-  58
[DEBUG]  edges: 1, 2, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 2, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 1:   20-  38-  57,   25-  52
[DEBUG]  edges: 1, 2, 1:   22-  41-  60,   27-  55
[DEBUG]  [3100] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 2:   23-  41-  59,   28-  54
[DEBUG]  edges: 1, 2, 2:   25-  42-  59,   30-  54
[DEBUG]  edges: 1, 2, 2:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 2, 2:   24-  44-  64,   29-  59
[DEBUG]  edges: 1, 2, 2:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 2, 2:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 2, 2:   23-  39-  55,   28-  50
[DEBUG]  edges: 1, 2, 2:   23-  37-  52,   28-  47
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 2:   25-  41-  57,   30-  52
[DEBUG]  edges: 1, 2, 2:   28-  43-  58,   33-  53
[DEBUG]  edges: 1, 2, 2:   27-  44-  62,   32-  57
[DEBUG]  edges: 1, 2, 2:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 2:   27-  41-  55,   32-  50
[DEBUG]  edges: 1, 2, 2:   23-  37-  52,   28-  47
[DEBUG]  edges: 1, 2, 2:   23-  38-  53,   28-  48
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 2, 2:   28-  44-  60,   33-  55
[DEBUG]  edges: 1, 2, 2:   26-  42-  58,   31-  53
[DEBUG]  edges: 1, 2, 2:   25-  43-  62,   30-  57
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 2:   27-  42-  57,   32-  52
[DEBUG]  edges: 1, 2, 2:   23-  38-  54,   28-  49
[DEBUG]  edges: 1, 2, 2:   23-  38-  53,   28-  48
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 2:   24-  42-  61,   29-  56
[DEBUG]  edges: 1, 2, 2:   26-  43-  61,   31-  56
[DEBUG]  edges: 1, 2, 2:   26-  43-  61,   31-  56
[DEBUG]  edges: 1, 2, 2:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 2, 2:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 2:   26-  40-  55,   31-  50
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  CPA
[DEBUG]  [3100] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 3, 0:   18-  40-  63,   31-  50
[DEBUG]  edges: 1, 3, 0:   18-  41-  64,   31-  51
[DEBUG]  edges: 1, 3, 0:   17-  39-  61,   30-  48
[DEBUG]  edges: 1, 3, 0:   17-  39-  61,   30-  48
[DEBUG]  edges: 1, 3, 0:   16-  38-  61,   29-  48
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 0:   17-  41-  65,   30-  52
[DEBUG]  edges: 1, 3, 0:   19-  39-  60,   32-  47
[DEBUG]  edges: 1, 3, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 3, 0:   18-  40-  62,   31-  49
[DEBUG]  edges: 1, 3, 0:   18-  39-  60,   31-  47
[DEBUG]  edges: 1, 3, 0:   17-  38-  59,   30-  46
[DEBUG]  edges: 1, 3, 0:   16-  38-  60,   29-  47
[DEBUG]  edges: 1, 3, 0:   17-  37-  58,   30-  45
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 3, 0:   19-  39-  60,   32-  47
[DEBUG]  edges: 1, 3, 0:   19-  40-  62,   32-  49
[DEBUG]  edges: 1, 3, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 3, 0:   17-  38-  59,   30-  46
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 3, 0:   17-  38-  59,   30-  46
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 0:   17-  41-  65,   30-  52
[DEBUG]  edges: 1, 3, 0:   18-  39-  61,   31-  48
[DEBUG]  edges: 1, 3, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 3, 0:   17-  39-  61,   30-  48
[DEBUG]  edges: 1, 3, 0:   18-  39-  61,   31-  48
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 3, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 3, 0:   17-  39-  62,   30-  49
[DEBUG]  [3100] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 1:   23-  41-  60,   28-  55
[DEBUG]  edges: 1, 3, 1:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 1:   25-  42-  59,   30-  54
[DEBUG]  edges: 1, 3, 1:   23-  40-  58,   28-  53
[DEBUG]  edges: 1, 3, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 3, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 1:   23-  40-  57,   28-  52
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 3, 1:   28-  42-  56,   33-  51
[DEBUG]  edges: 1, 3, 1:   25-  40-  56,   30-  51
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 1:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 1:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 1:   23-  39-  55,   28-  50
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 1:   26-  43-  60,   31-  55
[DEBUG]  edges: 1, 3, 1:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 1:   23-  40-  57,   28-  52
[DEBUG]  edges: 1, 3, 1:   22-  38-  55,   27-  50
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 3, 1:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 3, 1:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 3, 1:   23-  41-  60,   28-  55
[DEBUG]  edges: 1, 3, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 3, 1:   24-  41-  58,   29-  53
[DEBUG]  edges: 1, 3, 1:   21-  40-  59,   26-  54
[DEBUG]  edges: 1, 3, 1:   21-  40-  59,   26-  54
[DEBUG]  [3100] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 2:   21-  40-  59,   26-  54
[DEBUG]  edges: 1, 3, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 2:   25-  41-  57,   30-  52
[DEBUG]  edges: 1, 3, 2:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 3, 2:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 2:   22-  38-  54,   27-  49
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 2:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 3, 2:   27-  39-  52,   32-  47
[DEBUG]  edges: 1, 3, 2:   28-  44-  61,   33-  56
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   25-  40-  55,   30-  50
[DEBUG]  edges: 1, 3, 2:   26-  39-  53,   31-  48
[DEBUG]  edges: 1, 3, 2:   24-  39-  54,   29-  49
[DEBUG]  edges: 1, 3, 2:   23-  38-  54,   28-  49
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   27-  41-  55,   32-  50
[DEBUG]  edges: 1, 3, 2:   27-  41-  55,   32-  50
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   26-  40-  55,   31-  50
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   23-  38-  54,   28-  49
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 2:   23-  41-  59,   28-  54
[DEBUG]  edges: 1, 3, 2:   25-  40-  56,   30-  51
[DEBUG]  edges: 1, 3, 2:   27-  43-  59,   32-  54
[DEBUG]  edges: 1, 3, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 3, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 2:   25-  40-  55,   30-  50
[DEBUG]  edges: 1, 3, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 2:   23-  39-  56,   28-  51
[DEBUG]  CPA
[DEBUG]  discover rising edges aggressive:
[DEBUG]  [4eb0] = 200
[DEBUG]  [3000] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 0, 2, 0:   12-  38-  64,   25-  51
[DEBUG]  edges: 0, 2, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 2, 0:   15-  37-  60,   28-  47
[DEBUG]  edges: 0, 2, 0:   10-  36-  63,   23-  50
[DEBUG]  edges: 0, 2, 0:    9-  34-  60,   22-  47
[DEBUG]  edges: 0, 2, 0:   11-  36-  62,   24-  49
[DEBUG]  edges: 0, 2, 0:   12-  37-  62,   25-  49
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 2, 0:   13-  38-  63,   26-  50
[DEBUG]  edges: 0, 2, 0:   13-  37-  61,   26-  48
[DEBUG]  edges: 0, 2, 0:   14-  37-  61,   27-  48
[DEBUG]  edges: 0, 2, 0:   12-  38-  64,   25-  51
[DEBUG]  edges: 0, 2, 0:   10-  33-  57,   23-  44
[DEBUG]  edges: 0, 2, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 2, 0:   13-  39-  65,   26-  52
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 0, 2, 0:   13-  37-  61,   26-  48
[DEBUG]  edges: 0, 2, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 0, 2, 0:   15-  37-  59,   28-  46
[DEBUG]  edges: 0, 2, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 2, 0:   11-  35-  60,   24-  47
[DEBUG]  edges: 0, 2, 0:   12-  36-  60,   25-  47
[DEBUG]  edges: 0, 2, 0:   13-  37-  62,   26-  49
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 0, 2, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 2, 0:   13-  36-  59,   26-  46
[DEBUG]  edges: 0, 2, 0:   12-  35-  59,   25-  46
[DEBUG]  edges: 0, 2, 0:   11-  37-  64,   24-  51
[DEBUG]  edges: 0, 2, 0:   10-  35-  61,   23-  48
[DEBUG]  edges: 0, 2, 0:   11-  34-  58,   24-  45
[DEBUG]  edges: 0, 2, 0:   13-  37-  62,   26-  49
[DEBUG]  [3000] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 1:   21-  39-  57,   26-  52
[DEBUG]  edges: 0, 2, 1:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 2, 1:   18-  38-  58,   23-  53
[DEBUG]  edges: 0, 2, 1:   21-  38-  56,   26-  51
[DEBUG]  edges: 0, 2, 1:   15-  37-  59,   20-  54
[DEBUG]  edges: 0, 2, 1:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 2, 1:   17-  37-  57,   22-  52
[DEBUG]  edges: 0, 2, 1:   17-  37-  57,   22-  52
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 2, 1:   19-  39-  60,   24-  55
[DEBUG]  edges: 0, 2, 1:   19-  37-  56,   24-  51
[DEBUG]  edges: 0, 2, 1:   20-  38-  56,   25-  51
[DEBUG]  edges: 0, 2, 1:   15-  37-  60,   20-  55
[DEBUG]  edges: 0, 2, 1:   15-  35-  56,   20-  51
[DEBUG]  edges: 0, 2, 1:   16-  37-  58,   21-  53
[DEBUG]  edges: 0, 2, 1:   17-  39-  61,   22-  56
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 1:   23-  41-  59,   28-  54
[DEBUG]  edges: 0, 2, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 1:   20-  38-  57,   25-  52
[DEBUG]  edges: 0, 2, 1:   21-  38-  56,   26-  51
[DEBUG]  edges: 0, 2, 1:   16-  36-  57,   21-  52
[DEBUG]  edges: 0, 2, 1:   17-  36-  55,   22-  50
[DEBUG]  edges: 0, 2, 1:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 2, 1:   18-  37-  57,   23-  52
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 1:   21-  38-  56,   26-  51
[DEBUG]  edges: 0, 2, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 1:   18-  36-  55,   23-  50
[DEBUG]  edges: 0, 2, 1:   19-  37-  55,   24-  50
[DEBUG]  edges: 0, 2, 1:   16-  37-  59,   21-  54
[DEBUG]  edges: 0, 2, 1:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 2, 1:   17-  36-  55,   22-  50
[DEBUG]  edges: 0, 2, 1:   18-  38-  58,   23-  53
[DEBUG]  [3000] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 2, 2:   15-  37-  59,   20-  54
[DEBUG]  edges: 0, 2, 2:   16-  37-  59,   21-  54
[DEBUG]  edges: 0, 2, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 2:   16-  37-  58,   21-  53
[DEBUG]  edges: 0, 2, 2:   15-  35-  56,   20-  51
[DEBUG]  edges: 0, 2, 2:   16-  37-  58,   21-  53
[DEBUG]  edges: 0, 2, 2:   17-  37-  58,   22-  53
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 2, 2:   21-  40-  60,   26-  55
[DEBUG]  edges: 0, 2, 2:   18-  39-  61,   23-  56
[DEBUG]  edges: 0, 2, 2:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 2, 2:   20-  38-  57,   25-  52
[DEBUG]  edges: 0, 2, 2:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 2, 2:   16-  36-  57,   21-  52
[DEBUG]  edges: 0, 2, 2:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 2, 2:   20-  40-  61,   25-  56
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 2, 2:   22-  41-  61,   27-  56
[DEBUG]  edges: 0, 2, 2:   18-  39-  60,   23-  55
[DEBUG]  edges: 0, 2, 2:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 2, 2:   18-  39-  60,   23-  55
[DEBUG]  edges: 0, 2, 2:   17-  39-  61,   22-  56
[DEBUG]  edges: 0, 2, 2:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 2, 2:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 2, 2:   19-  38-  58,   24-  53
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 2, 2:   20-  41-  62,   25-  57
[DEBUG]  edges: 0, 2, 2:   17-  38-  60,   22-  55
[DEBUG]  edges: 0, 2, 2:   17-  38-  60,   22-  55
[DEBUG]  edges: 0, 2, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 2, 2:   17-  38-  60,   22-  55
[DEBUG]  edges: 0, 2, 2:   16-  37-  58,   21-  53
[DEBUG]  edges: 0, 2, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 2, 2:   20-  40-  60,   25-  55
[DEBUG]  CPA
[DEBUG]  [3000] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 3, 0:   11-  35-  60,   24-  47
[DEBUG]  edges: 0, 3, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 3, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 3, 0:   11-  36-  61,   24-  48
[DEBUG]  edges: 0, 3, 0:   10-  34-  59,   23-  46
[DEBUG]  edges: 0, 3, 0:   12-  34-  57,   25-  44
[DEBUG]  edges: 0, 3, 0:   12-  36-  60,   25-  47
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 3, 0:   12-  36-  61,   25-  48
[DEBUG]  edges: 0, 3, 0:   13-  38-  63,   26-  50
[DEBUG]  edges: 0, 3, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 0, 3, 0:   12-  37-  63,   25-  50
[DEBUG]  edges: 0, 3, 0:   11-  35-  59,   24-  46
[DEBUG]  edges: 0, 3, 0:   13-  37-  61,   26-  48
[DEBUG]  edges: 0, 3, 0:   12-  37-  63,   25-  50
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 0, 3, 0:   13-  37-  62,   26-  49
[DEBUG]  edges: 0, 3, 0:   14-  38-  62,   27-  49
[DEBUG]  edges: 0, 3, 0:   14-  38-  63,   27-  50
[DEBUG]  edges: 0, 3, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 3, 0:   12-  35-  59,   25-  46
[DEBUG]  edges: 0, 3, 0:   13-  36-  60,   26-  47
[DEBUG]  edges: 0, 3, 0:   13-  37-  61,   26-  48
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 0:   15-  38-  61,   28-  48
[DEBUG]  edges: 0, 3, 0:   13-  36-  59,   26-  46
[DEBUG]  edges: 0, 3, 0:   13-  37-  61,   26-  48
[DEBUG]  edges: 0, 3, 0:   12-  37-  62,   25-  49
[DEBUG]  edges: 0, 3, 0:   12-  38-  64,   25-  51
[DEBUG]  edges: 0, 3, 0:   12-  36-  61,   25-  48
[DEBUG]  edges: 0, 3, 0:   12-  35-  58,   25-  45
[DEBUG]  edges: 0, 3, 0:   12-  37-  63,   25-  50
[DEBUG]  [3000] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 3, 1:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 1:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 1:   21-  39-  58,   26-  53
[DEBUG]  edges: 0, 3, 1:   16-  36-  57,   21-  52
[DEBUG]  edges: 0, 3, 1:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 3, 1:   16-  35-  55,   21-  50
[DEBUG]  edges: 0, 3, 1:   17-  37-  57,   22-  52
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 1:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 3, 1:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 1:   19-  39-  60,   24-  55
[DEBUG]  edges: 0, 3, 1:   21-  40-  60,   26-  55
[DEBUG]  edges: 0, 3, 1:   16-  37-  59,   21-  54
[DEBUG]  edges: 0, 3, 1:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 3, 1:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 3, 1:   17-  37-  58,   22-  53
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 1:   22-  40-  59,   27-  54
[DEBUG]  edges: 0, 3, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 3, 1:   19-  38-  57,   24-  52
[DEBUG]  edges: 0, 3, 1:   20-  39-  59,   25-  54
[DEBUG]  edges: 0, 3, 1:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 3, 1:   18-  37-  57,   23-  52
[DEBUG]  edges: 0, 3, 1:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 3, 1:   18-  37-  57,   23-  52
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 0, 3, 1:   19-  37-  55,   24-  50
[DEBUG]  edges: 0, 3, 1:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 3, 1:   18-  38-  58,   23-  53
[DEBUG]  edges: 0, 3, 1:   16-  38-  60,   21-  55
[DEBUG]  edges: 0, 3, 1:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 3, 1:   17-  35-  54,   22-  49
[DEBUG]  edges: 0, 3, 1:   17-  38-  59,   22-  54
[DEBUG]  [3000] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 0, 3, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 3, 2:   15-  36-  57,   20-  52
[DEBUG]  edges: 0, 3, 2:   16-  36-  57,   21-  52
[DEBUG]  edges: 0, 3, 2:   19-  39-  59,   24-  54
[DEBUG]  edges: 0, 3, 2:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 2:   15-  36-  57,   20-  52
[DEBUG]  edges: 0, 3, 2:   17-  36-  55,   22-  50
[DEBUG]  edges: 0, 3, 2:   17-  37-  58,   22-  53
[DEBUG]  using pattern 1
[DEBUG]  edges: 0, 3, 2:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 2:   18-  39-  60,   23-  55
[DEBUG]  edges: 0, 3, 2:   18-  38-  58,   23-  53
[DEBUG]  edges: 0, 3, 2:   20-  40-  60,   25-  55
[DEBUG]  edges: 0, 3, 2:   18-  38-  58,   23-  53
[DEBUG]  edges: 0, 3, 2:   17-  36-  56,   22-  51
[DEBUG]  edges: 0, 3, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 0, 3, 2:   18-  39-  61,   23-  56
[DEBUG]  using pattern 2
[DEBUG]  edges: 0, 3, 2:   19-  40-  61,   24-  56
[DEBUG]  edges: 0, 3, 2:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 3, 2:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 2:   18-  40-  63,   23-  58
[DEBUG]  edges: 0, 3, 2:   18-  39-  60,   23-  55
[DEBUG]  edges: 0, 3, 2:   16-  36-  56,   21-  51
[DEBUG]  edges: 0, 3, 2:   19-  37-  55,   24-  50
[DEBUG]  edges: 0, 3, 2:   19-  37-  56,   24-  51
[DEBUG]  using pattern 3
[DEBUG]  edges: 0, 3, 2:   19-  39-  60,   24-  55
[DEBUG]  edges: 0, 3, 2:   17-  38-  59,   22-  54
[DEBUG]  edges: 0, 3, 2:   17-  38-  60,   22-  55
[DEBUG]  edges: 0, 3, 2:   18-  38-  59,   23-  54
[DEBUG]  edges: 0, 3, 2:   17-  37-  58,   22-  53
[DEBUG]  edges: 0, 3, 2:   16-  37-  59,   21-  54
[DEBUG]  edges: 0, 3, 2:   18-  37-  56,   23-  51
[DEBUG]  edges: 0, 3, 2:   19-  39-  59,   24-  54
[DEBUG]  CPA
[DEBUG]  [3100] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 1, 2, 0:   12-  36-  60,   25-  47
[DEBUG]  edges: 1, 2, 0:   16-  39-  63,   29-  50
[DEBUG]  edges: 1, 2, 0:   15-  38-  61,   28-  48
[DEBUG]  edges: 1, 2, 0:   13-  38-  63,   26-  50
[DEBUG]  edges: 1, 2, 0:   14-  37-  60,   27-  47
[DEBUG]  edges: 1, 2, 0:   13-  38-  64,   26-  51
[DEBUG]  edges: 1, 2, 0:   16-  39-  63,   29-  50
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  edges: 1, 2, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 2, 0:   17-  38-  59,   30-  46
[DEBUG]  edges: 1, 2, 0:   16-  39-  63,   29-  50
[DEBUG]  edges: 1, 2, 0:   16-  36-  57,   29-  44
[DEBUG]  edges: 1, 2, 0:   15-  37-  59,   28-  46
[DEBUG]  edges: 1, 2, 0:   17-  38-  59,   30-  46
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   17-  39-  61,   30-  48
[DEBUG]  edges: 1, 2, 0:   19-  40-  61,   32-  48
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  edges: 1, 2, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 2, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 2, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 1, 2, 0:   16-  38-  60,   29-  47
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 2, 0:   16-  37-  59,   29-  46
[DEBUG]  edges: 1, 2, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  edges: 1, 2, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 1, 2, 0:   17-  37-  57,   30-  44
[DEBUG]  edges: 1, 2, 0:   14-  38-  63,   27-  50
[DEBUG]  edges: 1, 2, 0:   17-  40-  64,   30-  51
[DEBUG]  [3100] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 1:   20-  40-  60,   25-  55
[DEBUG]  edges: 1, 2, 1:   18-  37-  56,   23-  51
[DEBUG]  edges: 1, 2, 1:   22-  40-  58,   27-  53
[DEBUG]  edges: 1, 2, 1:   20-  38-  57,   25-  52
[DEBUG]  edges: 1, 2, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 1, 2, 1:   21-  38-  55,   26-  50
[DEBUG]  edges: 1, 2, 1:   19-  38-  58,   24-  53
[DEBUG]  edges: 1, 2, 1:   21-  40-  59,   26-  54
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 1:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 2, 1:   24-  39-  54,   29-  49
[DEBUG]  edges: 1, 2, 1:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 2, 1:   23-  38-  54,   28-  49
[DEBUG]  edges: 1, 2, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 2, 1:   23-  39-  55,   28-  50
[DEBUG]  edges: 1, 2, 1:   21-  38-  55,   26-  50
[DEBUG]  edges: 1, 2, 1:   24-  40-  57,   29-  52
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 1:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 2, 1:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 1:   26-  41-  56,   31-  51
[DEBUG]  edges: 1, 2, 1:   23-  38-  54,   28-  49
[DEBUG]  edges: 1, 2, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 2, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 2, 1:   21-  39-  57,   26-  52
[DEBUG]  edges: 1, 2, 1:   24-  40-  56,   29-  51
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 1:   24-  43-  62,   29-  57
[DEBUG]  edges: 1, 2, 1:   23-  39-  55,   28-  50
[DEBUG]  edges: 1, 2, 1:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 2, 1:   21-  38-  55,   26-  50
[DEBUG]  edges: 1, 2, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 2, 1:   23-  39-  55,   28-  50
[DEBUG]  edges: 1, 2, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 1, 2, 1:   23-  42-  62,   28-  57
[DEBUG]  [3100] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 2, 2:   21-  41-  61,   26-  56
[DEBUG]  edges: 1, 2, 2:   17-  37-  57,   22-  52
[DEBUG]  edges: 1, 2, 2:   20-  39-  59,   25-  54
[DEBUG]  edges: 1, 2, 2:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 2, 2:   17-  38-  59,   22-  54
[DEBUG]  edges: 1, 2, 2:   20-  38-  56,   25-  51
[DEBUG]  edges: 1, 2, 2:   18-  39-  60,   23-  55
[DEBUG]  edges: 1, 2, 2:   21-  41-  61,   26-  56
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 2, 2:   25-  43-  62,   30-  57
[DEBUG]  edges: 1, 2, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 2, 2:   24-  43-  63,   29-  58
[DEBUG]  edges: 1, 2, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 2, 2:   23-  41-  59,   28-  54
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 2:   21-  38-  56,   26-  51
[DEBUG]  edges: 1, 2, 2:   24-  41-  59,   29-  54
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 2, 2:   23-  41-  59,   28-  54
[DEBUG]  edges: 1, 2, 2:   21-  38-  56,   26-  51
[DEBUG]  edges: 1, 2, 2:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 2, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 2, 2:   22-  39-  56,   27-  51
[DEBUG]  edges: 1, 2, 2:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 2, 2:   19-  38-  57,   24-  52
[DEBUG]  edges: 1, 2, 2:   23-  41-  59,   28-  54
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 2, 2:   25-  44-  63,   30-  58
[DEBUG]  edges: 1, 2, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 2, 2:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 2, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 2, 2:   23-  42-  62,   28-  57
[DEBUG]  edges: 1, 2, 2:   24-  39-  55,   29-  50
[DEBUG]  edges: 1, 2, 2:   21-  40-  59,   26-  54
[DEBUG]  edges: 1, 2, 2:   24-  42-  61,   29-  56
[DEBUG]  CPA
[DEBUG]  [3100] = 0x00000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 1, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 1, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 1, 3, 0:   15-  39-  63,   28-  50
[DEBUG]  edges: 1, 3, 0:   15-  39-  64,   28-  51
[DEBUG]  edges: 1, 3, 0:   15-  38-  61,   28-  48
[DEBUG]  edges: 1, 3, 0:   15-  38-  62,   28-  49
[DEBUG]  edges: 1, 3, 0:   16-  39-  63,   29-  50
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 1, 3, 0:   19-  40-  61,   32-  48
[DEBUG]  edges: 1, 3, 0:   19-  41-  64,   32-  51
[DEBUG]  edges: 1, 3, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 3, 0:   17-  40-  63,   30-  50
[DEBUG]  edges: 1, 3, 0:   17-  39-  61,   30-  48
[DEBUG]  edges: 1, 3, 0:   16-  37-  58,   29-  45
[DEBUG]  edges: 1, 3, 0:   16-  38-  60,   29-  47
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 3, 0:   19-  42-  65,   32-  52
[DEBUG]  edges: 1, 3, 0:   19-  41-  63,   32-  50
[DEBUG]  edges: 1, 3, 0:   17-  38-  60,   30-  47
[DEBUG]  edges: 1, 3, 0:   17-  41-  65,   30-  52
[DEBUG]  edges: 1, 3, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 3, 0:   16-  39-  62,   29-  49
[DEBUG]  edges: 1, 3, 0:   16-  38-  60,   29-  47
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 1, 3, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 3, 0:   17-  40-  64,   30-  51
[DEBUG]  edges: 1, 3, 0:   17-  39-  62,   30-  49
[DEBUG]  edges: 1, 3, 0:   16-  40-  64,   29-  51
[DEBUG]  edges: 1, 3, 0:   16-  38-  61,   29-  48
[DEBUG]  edges: 1, 3, 0:   15-  37-  59,   28-  46
[DEBUG]  edges: 1, 3, 0:   17-  40-  63,   30-  50
[DEBUG]  [3100] = 0x0c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 1:   20-  40-  61,   25-  56
[DEBUG]  edges: 1, 3, 1:   20-  39-  58,   25-  53
[DEBUG]  edges: 1, 3, 1:   22-  40-  59,   27-  54
[DEBUG]  edges: 1, 3, 1:   21-  40-  59,   26-  54
[DEBUG]  edges: 1, 3, 1:   20-  39-  59,   25-  54
[DEBUG]  edges: 1, 3, 1:   21-  39-  58,   26-  53
[DEBUG]  edges: 1, 3, 1:   21-  39-  57,   26-  52
[DEBUG]  edges: 1, 3, 1:   22-  40-  59,   27-  54
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 1:   24-  43-  63,   29-  58
[DEBUG]  edges: 1, 3, 1:   25-  41-  58,   30-  53
[DEBUG]  edges: 1, 3, 1:   24-  43-  63,   29-  58
[DEBUG]  edges: 1, 3, 1:   22-  40-  58,   27-  53
[DEBUG]  edges: 1, 3, 1:   24-  41-  58,   29-  53
[DEBUG]  edges: 1, 3, 1:   22-  39-  57,   27-  52
[DEBUG]  edges: 1, 3, 1:   23-  39-  55,   28-  50
[DEBUG]  edges: 1, 3, 1:   24-  41-  58,   29-  53
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 1:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 3, 1:   25-  42-  59,   30-  54
[DEBUG]  edges: 1, 3, 1:   25-  42-  59,   30-  54
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 1:   25-  42-  59,   30-  54
[DEBUG]  edges: 1, 3, 1:   24-  40-  56,   29-  51
[DEBUG]  edges: 1, 3, 1:   23-  39-  56,   28-  51
[DEBUG]  edges: 1, 3, 1:   24-  41-  58,   29-  53
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 1:   23-  42-  61,   28-  56
[DEBUG]  edges: 1, 3, 1:   24-  41-  58,   29-  53
[DEBUG]  edges: 1, 3, 1:   25-  42-  60,   30-  55
[DEBUG]  edges: 1, 3, 1:   22-  39-  57,   27-  52
[DEBUG]  edges: 1, 3, 1:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 3, 1:   22-  39-  57,   27-  52
[DEBUG]  edges: 1, 3, 1:   21-  38-  55,   26-  50
[DEBUG]  edges: 1, 3, 1:   23-  42-  61,   28-  56
[DEBUG]  [3100] = 0x2c000000
[DEBUG]  using pattern 0
[DEBUG]  edges: 1, 3, 2:   17-  39-  62,   22-  57
[DEBUG]  edges: 1, 3, 2:   17-  39-  62,   22-  57
[DEBUG]  edges: 1, 3, 2:   20-  40-  60,   25-  55
[DEBUG]  edges: 1, 3, 2:   22-  39-  57,   27-  52
[DEBUG]  edges: 1, 3, 2:   17-  39-  62,   22-  57
[DEBUG]  edges: 1, 3, 2:   19-  38-  58,   24-  53
[DEBUG]  edges: 1, 3, 2:   18-  37-  56,   23-  51
[DEBUG]  edges: 1, 3, 2:   20-  40-  61,   25-  56
[DEBUG]  using pattern 1
[DEBUG]  edges: 1, 3, 2:   23-  42-  61,   28-  56
[DEBUG]  edges: 1, 3, 2:   23-  40-  58,   28-  53
[DEBUG]  edges: 1, 3, 2:   24-  44-  64,   29-  59
[DEBUG]  edges: 1, 3, 2:   24-  42-  60,   29-  55
[DEBUG]  edges: 1, 3, 2:   23-  42-  61,   28-  56
[DEBUG]  edges: 1, 3, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 2:   21-  38-  56,   26-  51
[DEBUG]  edges: 1, 3, 2:   24-  42-  60,   29-  55
[DEBUG]  using pattern 2
[DEBUG]  edges: 1, 3, 2:   21-  40-  60,   26-  55
[DEBUG]  edges: 1, 3, 2:   22-  42-  62,   27-  57
[DEBUG]  edges: 1, 3, 2:   23-  41-  59,   28-  54
[DEBUG]  edges: 1, 3, 2:   24-  42-  61,   29-  56
[DEBUG]  edges: 1, 3, 2:   23-  41-  60,   28-  55
[DEBUG]  edges: 1, 3, 2:   23-  40-  57,   28-  52
[DEBUG]  edges: 1, 3, 2:   20-  37-  55,   25-  50
[DEBUG]  edges: 1, 3, 2:   23-  41-  60,   28-  55
[DEBUG]  using pattern 3
[DEBUG]  edges: 1, 3, 2:   24-  43-  62,   29-  57
[DEBUG]  edges: 1, 3, 2:   25-  43-  61,   30-  56
[DEBUG]  edges: 1, 3, 2:   25-  44-  64,   30-  59
[DEBUG]  edges: 1, 3, 2:   24-  41-  59,   29-  54
[DEBUG]  edges: 1, 3, 2:   23-  42-  62,   28-  57
[DEBUG]  edges: 1, 3, 2:   24-  40-  57,   29-  52
[DEBUG]  edges: 1, 3, 2:   21-  39-  57,   26-  52
[DEBUG]  edges: 1, 3, 2:   24-  43-  62,   29-  57
[DEBUG]  CPA
[DEBUG]  Aggressive write training:
[DEBUG]  tx_dq: 0, 2, 0:    8-  30-  52,   22-  38
[DEBUG]  tx_dq: 0, 2, 0:   30-  53-  76,   44-  62
[DEBUG]  tx_dq: 0, 2, 0:   61-  85- 109,   75-  95
[DEBUG]  tx_dq: 0, 2, 0:    9-  33-  57,   23-  43
[DEBUG]  tx_dq: 0, 2, 0:   36-  59-  83,   50-  69
[DEBUG]  tx_dq: 0, 2, 0:   48-  70-  92,   62-  78
[DEBUG]  tx_dq: 0, 2, 0:   55-  78- 101,   69-  87
[DEBUG]  tx_dq: 0, 2, 0:   64-  86- 109,   78-  95
[DEBUG]  tx_dq: 0, 3, 0:    2-  25-  48,   16-  34
[DEBUG]  tx_dq: 0, 3, 0:   34-  56-  79,   48-  65
[DEBUG]  tx_dq: 0, 3, 0:   56-  80- 104,   70-  90
[DEBUG]  tx_dq: 0, 3, 0:   14-  38-  62,   28-  48
[DEBUG]  tx_dq: 0, 3, 0:   36-  59-  83,   50-  69
[DEBUG]  tx_dq: 0, 3, 0:   51-  73-  95,   65-  81
[DEBUG]  tx_dq: 0, 3, 0:   57-  80- 103,   71-  89
[DEBUG]  tx_dq: 0, 3, 0:   64-  87- 110,   78-  96
[DEBUG]  tx_dq: 0, 2, 0:    9-  30-  51,   23-  37
[DEBUG]  tx_dq: 0, 2, 0:   29-  52-  75,   43-  61
[DEBUG]  tx_dq: 0, 2, 0:   63-  85- 107,   77-  93
[DEBUG]  tx_dq: 0, 2, 0:    9-  32-  56,   23-  42
[DEBUG]  tx_dq: 0, 2, 0:   37-  59-  82,   51-  68
[DEBUG]  tx_dq: 0, 2, 0:   52-  72-  92,   66-  78
[DEBUG]  tx_dq: 0, 2, 0:   56-  77-  99,   70-  85
[DEBUG]  tx_dq: 0, 2, 0:   63-  85- 108,   77-  94
[DEBUG]  tx_dq: 0, 3, 0:    4-  25-  47,   18-  33
[DEBUG]  tx_dq: 0, 3, 0:   32-  55-  79,   46-  65
[DEBUG]  tx_dq: 0, 3, 0:   56-  79- 103,   70-  89
[DEBUG]  tx_dq: 0, 3, 0:   12-  37-  62,   26-  48
[DEBUG]  tx_dq: 0, 3, 0:   36-  59-  82,   50-  68
[DEBUG]  tx_dq: 0, 3, 0:   53-  73-  94,   67-  80
[DEBUG]  tx_dq: 0, 3, 0:   56-  79- 102,   70-  88
[DEBUG]  tx_dq: 0, 3, 0:   62-  84- 106,   76-  92
[DEBUG]  tx_dq: 0, 2, 0:    7-  29-  51,   21-  37
[DEBUG]  tx_dq: 0, 2, 0:   32-  53-  74,   46-  60
[DEBUG]  tx_dq: 0, 2, 0:   60-  84- 108,   74-  94
[DEBUG]  tx_dq: 0, 2, 0:    8-  32-  56,   22-  42
[DEBUG]  tx_dq: 0, 2, 0:   36-  59-  82,   50-  68
[DEBUG]  tx_dq: 0, 2, 0:   51-  71-  91,   65-  77
[DEBUG]  tx_dq: 0, 2, 0:   56-  77-  99,   70-  85
[DEBUG]  tx_dq: 0, 2, 0:   66-  87- 108,   80-  94
[DEBUG]  tx_dq: 0, 3, 0:    1-  24-  47,   15-  33
[DEBUG]  tx_dq: 0, 3, 0:   34-  56-  79,   48-  65
[DEBUG]  tx_dq: 0, 3, 0:   53-  77- 102,   67-  88
[DEBUG]  tx_dq: 0, 3, 0:   11-  36-  61,   25-  47
[DEBUG]  tx_dq: 0, 3, 0:   35-  58-  82,   49-  68
[DEBUG]  tx_dq: 0, 3, 0:   51-  72-  94,   65-  80
[DEBUG]  tx_dq: 0, 3, 0:   57-  79- 101,   71-  87
[DEBUG]  tx_dq: 0, 3, 0:   65-  85- 106,   79-  92
[DEBUG]  tx_dq: 0, 2, 0:    8-  30-  52,   22-  38
[DEBUG]  tx_dq: 0, 2, 0:   33-  53-  74,   47-  60
[DEBUG]  tx_dq: 0, 2, 0:   63-  85- 108,   77-  94
[DEBUG]  tx_dq: 0, 2, 0:   10-  33-  56,   24-  42
[DEBUG]  tx_dq: 0, 2, 0:   36-  59-  82,   50-  68
[DEBUG]  tx_dq: 0, 2, 0:   48-  70-  92,   62-  78
[DEBUG]  tx_dq: 0, 2, 0:   56-  77-  99,   70-  85
[DEBUG]  tx_dq: 0, 2, 0:   63-  86- 109,   77-  95
[DEBUG]  tx_dq: 0, 3, 0:    2-  24-  47,   16-  33
[DEBUG]  tx_dq: 0, 3, 0:   36-  57-  78,   50-  64
[DEBUG]  tx_dq: 0, 3, 0:   56-  79- 103,   70-  89
[DEBUG]  tx_dq: 0, 3, 0:   15-  38-  62,   29-  48
[DEBUG]  tx_dq: 0, 3, 0:   35-  58-  82,   49-  68
[DEBUG]  tx_dq: 0, 3, 0:   49-  72-  95,   63-  81
[DEBUG]  tx_dq: 0, 3, 0:   57-  79- 102,   71-  88
[DEBUG]  tx_dq: 0, 3, 0:   60-  84- 108,   74-  94
[DEBUG]  tx_dq: 1, 2, 0:    9-  30-  51,   23-  37
[DEBUG]  tx_dq: 1, 2, 0:   26-  46-  66,   40-  52
[DEBUG]  tx_dq: 1, 2, 0:   57-  78- 100,   71-  86
[DEBUG]  tx_dq: 1, 2, 0:    9-  32-  55,   23-  41
[DEBUG]  tx_dq: 1, 2, 0:   33-  54-  75,   47-  61
[DEBUG]  tx_dq: 1, 2, 0:   48-  68-  89,   62-  75
[DEBUG]  tx_dq: 1, 2, 0:   48-  68-  89,   62-  75
[DEBUG]  tx_dq: 1, 2, 0:   65-  85- 106,   79-  92
[DEBUG]  tx_dq: 1, 3, 0:    7-  27-  48,   21-  34
[DEBUG]  tx_dq: 1, 3, 0:   33-  53-  73,   47-  59
[DEBUG]  tx_dq: 1, 3, 0:   63-  84- 105,   77-  91
[DEBUG]  tx_dq: 1, 3, 0:    8-  30-  53,   22-  39
[DEBUG]  tx_dq: 1, 3, 0:   38-  59-  80,   52-  66
[DEBUG]  tx_dq: 1, 3, 0:   52-  72-  93,   66-  79
[DEBUG]  tx_dq: 1, 3, 0:   57-  79- 102,   71-  88
[DEBUG]  tx_dq: 1, 3, 0:    7-  28-  50,   21-  36
[DEBUG]  tx_dq: 1, 2, 0:   10-  30-  50,   24-  36
[DEBUG]  tx_dq: 1, 2, 0:   29-  46-  64,   43-  50
[DEBUG]  tx_dq: 1, 2, 0:   56-  77-  98,   70-  84
[DEBUG]  tx_dq: 1, 2, 0:   11-  32-  54,   25-  40
[DEBUG]  tx_dq: 1, 2, 0:   35-  55-  76,   49-  62
[DEBUG]  tx_dq: 1, 2, 0:   51-  70-  89,   65-  75
[DEBUG]  tx_dq: 1, 2, 0:   50-  69-  88,   64-  74
[DEBUG]  tx_dq: 1, 2, 0:   69-  87- 106,   83-  92
[DEBUG]  tx_dq: 1, 3, 0:    6-  26-  47,   20-  33
[DEBUG]  tx_dq: 1, 3, 0:   34-  53-  72,   48-  58
[DEBUG]  tx_dq: 1, 3, 0:   60-  81- 103,   74-  89
[DEBUG]  tx_dq: 1, 3, 0:    7-  29-  52,   21-  38
[DEBUG]  tx_dq: 1, 3, 0:   39-  60-  81,   53-  67
[DEBUG]  tx_dq: 1, 3, 0:   53-  73-  94,   67-  80
[DEBUG]  tx_dq: 1, 3, 0:   59-  80- 102,   73-  88
[DEBUG]  tx_dq: 1, 3, 0:    8-  28-  48,   22-  34
[DEBUG]  tx_dq: 1, 2, 0:   13-  32-  51,   27-  37
[DEBUG]  tx_dq: 1, 2, 0:   25-  45-  66,   39-  52
[DEBUG]  tx_dq: 1, 2, 0:   57-  78-  99,   71-  85
[DEBUG]  tx_dq: 1, 2, 0:    8-  31-  54,   22-  40
[DEBUG]  tx_dq: 1, 2, 0:   34-  55-  76,   48-  62
[DEBUG]  tx_dq: 1, 2, 0:   48-  68-  88,   62-  74
[DEBUG]  tx_dq: 1, 2, 0:   49-  69-  89,   63-  75
[DEBUG]  tx_dq: 1, 2, 0:   66-  86- 106,   80-  92
[DEBUG]  tx_dq: 1, 3, 0:    9-  28-  48,   23-  34
[DEBUG]  tx_dq: 1, 3, 0:   31-  52-  73,   45-  59
[DEBUG]  tx_dq: 1, 3, 0:   61-  82- 104,   75-  90
[DEBUG]  tx_dq: 1, 3, 0:    5-  27-  50,   19-  36
[DEBUG]  tx_dq: 1, 3, 0:   38-  59-  80,   52-  66
[DEBUG]  tx_dq: 1, 3, 0:   53-  73-  94,   67-  80
[DEBUG]  tx_dq: 1, 3, 0:   58-  80- 102,   72-  88
[DEBUG]  tx_dq: 1, 3, 0:    4-  26-  48,   18-  34
[DEBUG]  tx_dq: 1, 2, 0:   10-  30-  51,   24-  37
[DEBUG]  tx_dq: 1, 2, 0:   27-  46-  66,   41-  52
[DEBUG]  tx_dq: 1, 2, 0:   59-  78-  98,   73-  84
[DEBUG]  tx_dq: 1, 2, 0:   10-  32-  54,   24-  40
[DEBUG]  tx_dq: 1, 2, 0:   33-  54-  76,   47-  62
[DEBUG]  tx_dq: 1, 2, 0:   52-  70-  88,   66-  74
[DEBUG]  tx_dq: 1, 2, 0:   48-  68-  89,   62-  75
[DEBUG]  tx_dq: 1, 2, 0:   64-  85- 106,   78-  92
[DEBUG]  tx_dq: 1, 3, 0:    8-  27-  47,   22-  33
[DEBUG]  tx_dq: 1, 3, 0:   33-  53-  73,   47-  59
[DEBUG]  tx_dq: 1, 3, 0:   64-  83- 102,   78-  88
[DEBUG]  tx_dq: 1, 3, 0:    9-  30-  51,   23-  37
[DEBUG]  tx_dq: 1, 3, 0:   39-  59-  80,   53-  66
[DEBUG]  tx_dq: 1, 3, 0:   56-  75-  94,   70-  80
[DEBUG]  tx_dq: 1, 3, 0:   56-  79- 103,   70-  89
[DEBUG]  tx_dq: 1, 3, 0:    5-  26-  48,   19-  34
[DEBUG]  tx_dq: 0, 2, 1:   10-  29-  48,   15-  43
[DEBUG]  tx_dq: 0, 2, 1:   34-  52-  71,   39-  66
[DEBUG]  tx_dq: 0, 2, 1:   65-  84- 103,   70-  98
[DEBUG]  tx_dq: 0, 2, 1:   14-  33-  53,   19-  48
[DEBUG]  tx_dq: 0, 2, 1:   40-  59-  79,   45-  74
[DEBUG]  tx_dq: 0, 2, 1:   53-  70-  87,   58-  82
[DEBUG]  tx_dq: 0, 2, 1:   58-  77-  96,   63-  91
[DEBUG]  tx_dq: 0, 2, 1:   67-  85- 104,   72-  99
[DEBUG]  tx_dq: 0, 3, 1:    6-  25-  45,   11-  40
[DEBUG]  tx_dq: 0, 3, 1:   38-  56-  74,   43-  69
[DEBUG]  tx_dq: 0, 3, 1:   60-  79-  99,   65-  94
[DEBUG]  tx_dq: 0, 3, 1:   18-  37-  57,   23-  52
[DEBUG]  tx_dq: 0, 3, 1:   40-  59-  79,   45-  74
[DEBUG]  tx_dq: 0, 3, 1:   55-  72-  89,   60-  84
[DEBUG]  tx_dq: 0, 3, 1:   62-  80-  98,   67-  93
[DEBUG]  tx_dq: 0, 3, 1:   67-  85- 104,   72-  99
[DEBUG]  tx_dq: 0, 2, 1:   12-  29-  47,   17-  42
[DEBUG]  tx_dq: 0, 2, 1:   33-  52-  71,   38-  66
[DEBUG]  tx_dq: 0, 2, 1:   66-  84- 103,   71-  98
[DEBUG]  tx_dq: 0, 2, 1:   15-  33-  52,   20-  47
[DEBUG]  tx_dq: 0, 2, 1:   41-  59-  78,   46-  73
[DEBUG]  tx_dq: 0, 2, 1:   56-  71-  87,   61-  82
[DEBUG]  tx_dq: 0, 2, 1:   59-  77-  95,   64-  90
[DEBUG]  tx_dq: 0, 2, 1:   67-  85- 103,   72-  98
[DEBUG]  tx_dq: 0, 3, 1:    8-  25-  43,   13-  38
[DEBUG]  tx_dq: 0, 3, 1:   36-  54-  73,   41-  68
[DEBUG]  tx_dq: 0, 3, 1:   61-  80-  99,   66-  94
[DEBUG]  tx_dq: 0, 3, 1:   17-  36-  56,   22-  51
[DEBUG]  tx_dq: 0, 3, 1:   41-  59-  78,   46-  73
[DEBUG]  tx_dq: 0, 3, 1:   57-  72-  88,   62-  83
[DEBUG]  tx_dq: 0, 3, 1:   60-  78-  96,   65-  91
[DEBUG]  tx_dq: 0, 3, 1:   66-  84- 103,   71-  98
[DEBUG]  tx_dq: 0, 2, 1:   11-  29-  47,   16-  42
[DEBUG]  tx_dq: 0, 2, 1:   36-  53-  71,   41-  66
[DEBUG]  tx_dq: 0, 2, 1:   65-  84- 103,   70-  98
[DEBUG]  tx_dq: 0, 2, 1:   13-  33-  53,   18-  48
[DEBUG]  tx_dq: 0, 2, 1:   41-  59-  78,   46-  73
[DEBUG]  tx_dq: 0, 2, 1:   56-  71-  87,   61-  82
[DEBUG]  tx_dq: 0, 2, 1:   61-  77-  93,   66-  88
[DEBUG]  tx_dq: 0, 2, 1:   71-  87- 103,   76-  98
[DEBUG]  tx_dq: 0, 3, 1:    4-  22-  41,    9-  36
[DEBUG]  tx_dq: 0, 3, 1:   39-  55-  72,   44-  67
[DEBUG]  tx_dq: 0, 3, 1:   58-  78-  98,   63-  93
[DEBUG]  tx_dq: 0, 3, 1:   16-  36-  56,   21-  51
[DEBUG]  tx_dq: 0, 3, 1:   40-  59-  78,   45-  73
[DEBUG]  tx_dq: 0, 3, 1:   56-  71-  87,   61-  82
[DEBUG]  tx_dq: 0, 3, 1:   61-  78-  95,   66-  90
[DEBUG]  tx_dq: 0, 3, 1:   69-  85- 101,   74-  96
[DEBUG]  tx_dq: 0, 2, 1:   12-  29-  47,   17-  42
[DEBUG]  tx_dq: 0, 2, 1:   38-  54-  71,   43-  66
[DEBUG]  tx_dq: 0, 2, 1:   68-  86- 104,   73-  99
[DEBUG]  tx_dq: 0, 2, 1:   15-  34-  53,   20-  48
[DEBUG]  tx_dq: 0, 2, 1:   40-  59-  78,   45-  73
[DEBUG]  tx_dq: 0, 2, 1:   52-  69-  87,   57-  82
[DEBUG]  tx_dq: 0, 2, 1:   60-  77-  94,   65-  89
[DEBUG]  tx_dq: 0, 2, 1:   67-  85- 103,   72-  98
[DEBUG]  tx_dq: 0, 3, 1:    6-  24-  42,   11-  37
[DEBUG]  tx_dq: 0, 3, 1:   40-  56-  73,   45-  68
[DEBUG]  tx_dq: 0, 3, 1:   61-  80-  99,   66-  94
[DEBUG]  tx_dq: 0, 3, 1:   19-  37-  56,   24-  51
[DEBUG]  tx_dq: 0, 3, 1:   40-  59-  78,   45-  73
[DEBUG]  tx_dq: 0, 3, 1:   54-  71-  88,   59-  83
[DEBUG]  tx_dq: 0, 3, 1:   61-  78-  96,   66-  91
[DEBUG]  tx_dq: 0, 3, 1:   65-  84- 103,   70-  98
[DEBUG]  tx_dq: 1, 2, 1:   13-  30-  47,   18-  42
[DEBUG]  tx_dq: 1, 2, 1:   31-  47-  63,   36-  58
[DEBUG]  tx_dq: 1, 2, 1:   61-  78-  95,   66-  90
[DEBUG]  tx_dq: 1, 2, 1:   13-  31-  50,   18-  45
[DEBUG]  tx_dq: 1, 2, 1:   38-  54-  71,   43-  66
[DEBUG]  tx_dq: 1, 2, 1:   51-  68-  86,   56-  81
[DEBUG]  tx_dq: 1, 2, 1:   50-  67-  84,   55-  79
[DEBUG]  tx_dq: 1, 2, 1:   69-  85- 102,   74-  97
[DEBUG]  tx_dq: 1, 3, 1:   11-  27-  44,   16-  39
[DEBUG]  tx_dq: 1, 3, 1:   38-  54-  71,   43-  66
[DEBUG]  tx_dq: 1, 3, 1:   66-  83- 100,   71-  95
[DEBUG]  tx_dq: 1, 3, 1:   12-  29-  47,   17-  42
[DEBUG]  tx_dq: 1, 3, 1:   42-  58-  75,   47-  70
[DEBUG]  tx_dq: 1, 3, 1:   56-  72-  88,   61-  83
[DEBUG]  tx_dq: 1, 3, 1:   63-  80-  97,   68-  92
[DEBUG]  tx_dq: 1, 3, 1:   10-  28-  46,   15-  41
[DEBUG]  tx_dq: 1, 2, 1:   14-  30-  46,   19-  41
[DEBUG]  tx_dq: 1, 2, 1:   33-  46-  60,   38-  55
[DEBUG]  tx_dq: 1, 2, 1:   60-  77-  94,   65-  89
[DEBUG]  tx_dq: 1, 2, 1:   16-  32-  48,   21-  43
[DEBUG]  tx_dq: 1, 2, 1:   40-  56-  72,   45-  67
[DEBUG]  tx_dq: 1, 2, 1:   56-  69-  83,   61-  78
[DEBUG]  tx_dq: 1, 2, 1:   56-  69-  83,   61-  78
[DEBUG]  tx_dq: 1, 2, 1:   73-  87- 102,   78-  97
[DEBUG]  tx_dq: 1, 3, 1:   10-  26-  43,   15-  38
[DEBUG]  tx_dq: 1, 3, 1:   39-  53-  67,   44-  62
[DEBUG]  tx_dq: 1, 3, 1:   64-  80-  97,   69-  92
[DEBUG]  tx_dq: 1, 3, 1:   11-  29-  47,   16-  42
[DEBUG]  tx_dq: 1, 3, 1:   43-  59-  75,   48-  70
[DEBUG]  tx_dq: 1, 3, 1:   57-  72-  87,   62-  82
[DEBUG]  tx_dq: 1, 3, 1:   64-  80-  96,   69-  91
[DEBUG]  tx_dq: 1, 3, 1:   12-  27-  43,   17-  38
[DEBUG]  tx_dq: 1, 2, 1:   17-  31-  46,   22-  41
[DEBUG]  tx_dq: 1, 2, 1:   30-  46-  62,   35-  57
[DEBUG]  tx_dq: 1, 2, 1:   62-  78-  94,   67-  89
[DEBUG]  tx_dq: 1, 2, 1:   13-  30-  47,   18-  42
[DEBUG]  tx_dq: 1, 2, 1:   40-  55-  71,   45-  66
[DEBUG]  tx_dq: 1, 2, 1:   51-  67-  84,   56-  79
[DEBUG]  tx_dq: 1, 2, 1:   54-  68-  83,   59-  78
[DEBUG]  tx_dq: 1, 2, 1:   71-  86- 102,   76-  97
[DEBUG]  tx_dq: 1, 3, 1:   13-  27-  42,   18-  37
[DEBUG]  tx_dq: 1, 3, 1:   34-  50-  67,   39-  62
[DEBUG]  tx_dq: 1, 3, 1:   65-  81-  98,   70-  93
[DEBUG]  tx_dq: 1, 3, 1:    9-  27-  45,   14-  40
[DEBUG]  tx_dq: 1, 3, 1:   41-  58-  75,   46-  70
[DEBUG]  tx_dq: 1, 3, 1:   57-  71-  86,   62-  81
[DEBUG]  tx_dq: 1, 3, 1:   63-  79-  96,   68-  91
[DEBUG]  tx_dq: 1, 3, 1:    9-  26-  43,   14-  38
[DEBUG]  tx_dq: 1, 2, 1:   14-  29-  45,   19-  40
[DEBUG]  tx_dq: 1, 2, 1:   32-  47-  63,   37-  58
[DEBUG]  tx_dq: 1, 2, 1:   63-  78-  93,   68-  88
[DEBUG]  tx_dq: 1, 2, 1:   15-  31-  48,   20-  43
[DEBUG]  tx_dq: 1, 2, 1:   39-  55-  71,   44-  66
[DEBUG]  tx_dq: 1, 2, 1:   56-  69-  82,   61-  77
[DEBUG]  tx_dq: 1, 2, 1:   51-  67-  83,   56-  78
[DEBUG]  tx_dq: 1, 2, 1:   69-  85- 102,   74-  97
[DEBUG]  tx_dq: 1, 3, 1:   11-  26-  41,   16-  36
[DEBUG]  tx_dq: 1, 3, 1:   38-  53-  69,   43-  64
[DEBUG]  tx_dq: 1, 3, 1:   66-  80-  95,   71-  90
[DEBUG]  tx_dq: 1, 3, 1:   15-  30-  46,   20-  41
[DEBUG]  tx_dq: 1, 3, 1:   42-  58-  75,   47-  70
[DEBUG]  tx_dq: 1, 3, 1:   59-  73-  87,   64-  82
[DEBUG]  tx_dq: 1, 3, 1:   60-  78-  97,   65-  92
[DEBUG]  tx_dq: 1, 3, 1:    9-  26-  43,   14-  38
[DEBUG]  tx_dq: 0, 2, 2:    6-  27-  48,   11-  43
[DEBUG]  tx_dq: 0, 2, 2:   29-  50-  71,   34-  66
[DEBUG]  tx_dq: 0, 2, 2:   60-  82- 104,   65-  99
[DEBUG]  tx_dq: 0, 2, 2:    8-  30-  52,   13-  47
[DEBUG]  tx_dq: 0, 2, 2:   37-  57-  78,   42-  73
[DEBUG]  tx_dq: 0, 2, 2:   49-  68-  87,   54-  82
[DEBUG]  tx_dq: 0, 2, 2:   55-  75-  95,   60-  90
[DEBUG]  tx_dq: 0, 2, 2:   63-  82- 102,   68-  97
[DEBUG]  tx_dq: 0, 3, 2:    4-  23-  43,    9-  38
[DEBUG]  tx_dq: 0, 3, 2:   34-  53-  72,   39-  67
[DEBUG]  tx_dq: 0, 3, 2:   57-  78-  99,   62-  94
[DEBUG]  tx_dq: 0, 3, 2:   14-  35-  56,   19-  51
[DEBUG]  tx_dq: 0, 3, 2:   38-  57-  77,   43-  72
[DEBUG]  tx_dq: 0, 3, 2:   50-  69-  88,   55-  83
[DEBUG]  tx_dq: 0, 3, 2:   57-  77-  97,   62-  92
[DEBUG]  tx_dq: 0, 3, 2:   62-  82- 103,   67-  98
[DEBUG]  tx_dq: 0, 2, 2:    9-  27-  45,   14-  40
[DEBUG]  tx_dq: 0, 2, 2:   29-  48-  68,   34-  63
[DEBUG]  tx_dq: 0, 2, 2:   61-  82- 103,   66-  98
[DEBUG]  tx_dq: 0, 2, 2:   10-  30-  51,   15-  46
[DEBUG]  tx_dq: 0, 2, 2:   38-  57-  77,   43-  72
[DEBUG]  tx_dq: 0, 2, 2:   51-  68-  86,   56-  81
[DEBUG]  tx_dq: 0, 2, 2:   56-  74-  93,   61-  88
[DEBUG]  tx_dq: 0, 2, 2:   63-  82- 102,   68-  97
[DEBUG]  tx_dq: 0, 3, 2:    3-  21-  40,    8-  35
[DEBUG]  tx_dq: 0, 3, 2:   32-  51-  71,   37-  66
[DEBUG]  tx_dq: 0, 3, 2:   56-  76-  97,   61-  92
[DEBUG]  tx_dq: 0, 3, 2:   13-  34-  56,   18-  51
[DEBUG]  tx_dq: 0, 3, 2:   38-  57-  77,   43-  72
[DEBUG]  tx_dq: 0, 3, 2:   52-  69-  87,   57-  82
[DEBUG]  tx_dq: 0, 3, 2:   56-  75-  95,   61-  90
[DEBUG]  tx_dq: 0, 3, 2:   63-  81- 100,   68-  95
[DEBUG]  tx_dq: 0, 2, 2:    8-  27-  47,   13-  42
[DEBUG]  tx_dq: 0, 2, 2:   33-  50-  68,   38-  63
[DEBUG]  tx_dq: 0, 2, 2:   61-  82- 103,   66-  98
[DEBUG]  tx_dq: 0, 2, 2:    9-  30-  52,   14-  47
[DEBUG]  tx_dq: 0, 2, 2:   37-  57-  77,   42-  72
[DEBUG]  tx_dq: 0, 2, 2:   51-  68-  86,   56-  81
[DEBUG]  tx_dq: 0, 2, 2:   56-  74-  93,   61-  88
[DEBUG]  tx_dq: 0, 2, 2:   66-  84- 102,   71-  97
[DEBUG]  tx_dq: 0, 3, 2:    2-  21-  41,    7-  36
[DEBUG]  tx_dq: 0, 3, 2:   35-  53-  71,   40-  66
[DEBUG]  tx_dq: 0, 3, 2:   56-  76-  97,   61-  92
[DEBUG]  tx_dq: 0, 3, 2:   13-  35-  57,   18-  52
[DEBUG]  tx_dq: 0, 3, 2:   36-  56-  76,   41-  71
[DEBUG]  tx_dq: 0, 3, 2:   52-  69-  87,   57-  82
[DEBUG]  tx_dq: 0, 3, 2:   57-  76-  95,   62-  90
[DEBUG]  tx_dq: 0, 3, 2:   64-  82- 101,   69-  96
[DEBUG]  tx_dq: 0, 2, 2:    8-  27-  46,   13-  41
[DEBUG]  tx_dq: 0, 2, 2:   32-  49-  67,   37-  62
[DEBUG]  tx_dq: 0, 2, 2:   63-  83- 103,   68-  98
[DEBUG]  tx_dq: 0, 2, 2:   12-  32-  52,   17-  47
[DEBUG]  tx_dq: 0, 2, 2:   37-  57-  77,   42-  72
[DEBUG]  tx_dq: 0, 2, 2:   48-  67-  86,   53-  81
[DEBUG]  tx_dq: 0, 2, 2:   56-  74-  93,   61-  88
[DEBUG]  tx_dq: 0, 2, 2:   64-  83- 103,   69-  98
[DEBUG]  tx_dq: 0, 3, 2:    3-  22-  41,    8-  36
[DEBUG]  tx_dq: 0, 3, 2:   36-  53-  71,   41-  66
[DEBUG]  tx_dq: 0, 3, 2:   57-  77-  97,   62-  92
[DEBUG]  tx_dq: 0, 3, 2:   16-  36-  56,   21-  51
[DEBUG]  tx_dq: 0, 3, 2:   37-  57-  77,   42-  72
[DEBUG]  tx_dq: 0, 3, 2:   50-  68-  87,   55-  82
[DEBUG]  tx_dq: 0, 3, 2:   56-  76-  96,   61-  91
[DEBUG]  tx_dq: 0, 3, 2:   62-  81- 101,   67-  96
[DEBUG]  tx_dq: 1, 2, 2:    8-  26-  45,   13-  40
[DEBUG]  tx_dq: 1, 2, 2:   26-  42-  59,   31-  54
[DEBUG]  tx_dq: 1, 2, 2:   58-  76-  95,   63-  90
[DEBUG]  tx_dq: 1, 2, 2:    7-  28-  50,   12-  45
[DEBUG]  tx_dq: 1, 2, 2:   34-  51-  69,   39-  64
[DEBUG]  tx_dq: 1, 2, 2:   50-  65-  81,   55-  76
[DEBUG]  tx_dq: 1, 2, 2:   48-  65-  83,   53-  78
[DEBUG]  tx_dq: 1, 2, 2:   65-  82- 100,   70-  95
[DEBUG]  tx_dq: 1, 3, 2:    8-  25-  42,   13-  37
[DEBUG]  tx_dq: 1, 3, 2:   34-  49-  65,   39-  60
[DEBUG]  tx_dq: 1, 3, 2:   64-  80-  97,   69-  92
[DEBUG]  tx_dq: 1, 3, 2:    8-  27-  47,   13-  42
[DEBUG]  tx_dq: 1, 3, 2:   39-  56-  73,   44-  68
[DEBUG]  tx_dq: 1, 3, 2:   51-  68-  86,   56-  81
[DEBUG]  tx_dq: 1, 3, 2:   58-  76-  95,   63-  90
[DEBUG]  tx_dq: 1, 3, 2:    5-  25-  45,   10-  40
[DEBUG]  tx_dq: 1, 2, 2:    9-  26-  43,   14-  38
[DEBUG]  tx_dq: 1, 2, 2:   28-  43-  58,   33-  53
[DEBUG]  tx_dq: 1, 2, 2:   55-  73-  92,   60-  87
[DEBUG]  tx_dq: 1, 2, 2:    8-  27-  47,   13-  42
[DEBUG]  tx_dq: 1, 2, 2:   35-  51-  68,   40-  63
[DEBUG]  tx_dq: 1, 2, 2:   50-  65-  81,   55-  76
[DEBUG]  tx_dq: 1, 2, 2:   50-  66-  83,   55-  78
[DEBUG]  tx_dq: 1, 2, 2:   68-  83-  99,   73-  94
[DEBUG]  tx_dq: 1, 3, 2:    5-  22-  40,   10-  35
[DEBUG]  tx_dq: 1, 3, 2:   33-  48-  63,   38-  58
[DEBUG]  tx_dq: 1, 3, 2:   59-  77-  95,   64-  90
[DEBUG]  tx_dq: 1, 3, 2:    6-  26-  46,   11-  41
[DEBUG]  tx_dq: 1, 3, 2:   39-  55-  72,   44-  67
[DEBUG]  tx_dq: 1, 3, 2:   51-  67-  84,   56-  79
[DEBUG]  tx_dq: 1, 3, 2:   58-  76-  95,   63-  90
[DEBUG]  tx_dq: 1, 3, 2:    6-  24-  42,   11-  37
[DEBUG]  tx_dq: 1, 2, 2:   11-  27-  43,   16-  38
[DEBUG]  tx_dq: 1, 2, 2:   27-  42-  58,   32-  53
[DEBUG]  tx_dq: 1, 2, 2:   59-  75-  92,   64-  87
[DEBUG]  tx_dq: 1, 2, 2:    8-  27-  47,   13-  42
[DEBUG]  tx_dq: 1, 2, 2:   35-  52-  69,   40-  64
[DEBUG]  tx_dq: 1, 2, 2:   49-  64-  80,   54-  75
[DEBUG]  tx_dq: 1, 2, 2:   48-  65-  83,   53-  78
[DEBUG]  tx_dq: 1, 2, 2:   67-  83-  99,   72-  94
[DEBUG]  tx_dq: 1, 3, 2:    9-  24-  40,   14-  35
[DEBUG]  tx_dq: 1, 3, 2:   32-  48-  64,   37-  59
[DEBUG]  tx_dq: 1, 3, 2:   63-  79-  96,   68-  91
[DEBUG]  tx_dq: 1, 3, 2:    5-  25-  45,   10-  40
[DEBUG]  tx_dq: 1, 3, 2:   38-  55-  73,   43-  68
[DEBUG]  tx_dq: 1, 3, 2:   53-  68-  84,   58-  79
[DEBUG]  tx_dq: 1, 3, 2:   57-  75-  94,   62-  89
[DEBUG]  tx_dq: 1, 3, 2:    4-  23-  43,    9-  38
[DEBUG]  tx_dq: 1, 2, 2:    9-  26-  44,   14-  39
[DEBUG]  tx_dq: 1, 2, 2:   28-  43-  59,   33-  54
[DEBUG]  tx_dq: 1, 2, 2:   58-  75-  92,   63-  87
[DEBUG]  tx_dq: 1, 2, 2:    8-  27-  47,   13-  42
[DEBUG]  tx_dq: 1, 2, 2:   34-  51-  69,   39-  64
[DEBUG]  tx_dq: 1, 2, 2:   54-  67-  81,   59-  76
[DEBUG]  tx_dq: 1, 2, 2:   47-  64-  82,   52-  77
[DEBUG]  tx_dq: 1, 2, 2:   66-  82-  99,   71-  94
[DEBUG]  tx_dq: 1, 3, 2:    7-  23-  40,   12-  35
[DEBUG]  tx_dq: 1, 3, 2:   33-  49-  65,   38-  60
[DEBUG]  tx_dq: 1, 3, 2:   62-  78-  95,   67-  90
[DEBUG]  tx_dq: 1, 3, 2:    8-  26-  44,   13-  39
[DEBUG]  tx_dq: 1, 3, 2:   39-  56-  73,   44-  68
[DEBUG]  tx_dq: 1, 3, 2:   55-  70-  85,   60-  80
[DEBUG]  tx_dq: 1, 3, 2:   56-  75-  95,   61-  90
[DEBUG]  tx_dq: 1, 3, 2:    6-  25-  44,   11-  39
[DEBUG]  CPB
[DEBUG]  tx_dq 0, 2, 0:   30
[DEBUG]  tx_dq 0, 2, 1:   53
[DEBUG]  tx_dq 0, 2, 2:   85
[DEBUG]  tx_dq 0, 2, 3:   33
[DEBUG]  tx_dq 0, 2, 4:   59
[DEBUG]  tx_dq 0, 2, 5:   71
[DEBUG]  tx_dq 0, 2, 6:   77
[DEBUG]  tx_dq 0, 2, 7:   87
[DEBUG]  tx_dq 0, 3, 0:   25
[DEBUG]  tx_dq 0, 3, 1:   57
[DEBUG]  tx_dq 0, 3, 2:   79
[DEBUG]  tx_dq 0, 3, 3:   38
[DEBUG]  tx_dq 0, 3, 4:   59
[DEBUG]  tx_dq 0, 3, 5:   73
[DEBUG]  tx_dq 0, 3, 6:   79
[DEBUG]  tx_dq 0, 3, 7:   85
[DEBUG]  tx_dq 1, 2, 0:   31
[DEBUG]  tx_dq 1, 2, 1:   46
[DEBUG]  tx_dq 1, 2, 2:   78
[DEBUG]  tx_dq 1, 2, 3:   32
[DEBUG]  tx_dq 1, 2, 4:   55
[DEBUG]  tx_dq 1, 2, 5:   70
[DEBUG]  tx_dq 1, 2, 6:   69
[DEBUG]  tx_dq 1, 2, 7:   87
[DEBUG]  tx_dq 1, 3, 0:   28
[DEBUG]  tx_dq 1, 3, 1:   53
[DEBUG]  tx_dq 1, 3, 2:   83
[DEBUG]  tx_dq 1, 3, 3:   29
[DEBUG]  tx_dq 1, 3, 4:   59
[DEBUG]  tx_dq 1, 3, 5:   74
[DEBUG]  tx_dq 1, 3, 6:   80
[DEBUG]  tx_dq 1, 3, 7:   28
[DEBUG]  normalize 0, 2, 8: mat 142
[DEBUG]  normalize 0, 2, 8: delta -5
[DEBUG]  normalize 0, 3, 8: mat 144
[DEBUG]  normalize 0, 3, 8: delta -5
[DEBUG]  normalize 1, 2, 8: mat 179
[DEBUG]  normalize 1, 2, 8: delta -5
[DEBUG]  normalize 1, 3, 8: mat 177
[DEBUG]  normalize 1, 3, 8: delta -5
[DEBUG]  OTHP [400c] = 58b4
[DEBUG]  OTHP [440c] = 58b4
[DEBUG]  t123: 1767, 6000, 6120
[NOTE ]  ME: FWS2: 0x161f0126
[NOTE ]  ME:  Bist in progress: 0x0
[NOTE ]  ME:  ICC Status      : 0x3
[NOTE ]  ME:  Invoke MEBx     : 0x0
[NOTE ]  ME:  CPU replaced    : 0x0
[NOTE ]  ME:  MBP ready       : 0x1
[NOTE ]  ME:  MFS failure     : 0x0
[NOTE ]  ME:  Warm reset req  : 0x0
[NOTE ]  ME:  CPU repl valid  : 0x1
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  FW update req   : 0x0
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  Current state   : 0x1f
[NOTE ]  ME:  Current PM event: 0x6
[NOTE ]  ME:  Progress code   : 0x1
[NOTE ]  PASSED! Tell ME that DRAM is ready
[INFO ]  Timestamp - waiting for ME acknowledgment of raminit: 30716602488
[INFO ]  Timestamp - finished waiting for ME response: 30741789510
[NOTE ]  ME: FWS2: 0x16500126
[NOTE ]  ME:  Bist in progress: 0x0
[NOTE ]  ME:  ICC Status      : 0x3
[NOTE ]  ME:  Invoke MEBx     : 0x0
[NOTE ]  ME:  CPU replaced    : 0x0
[NOTE ]  ME:  MBP ready       : 0x1
[NOTE ]  ME:  MFS failure     : 0x0
[NOTE ]  ME:  Warm reset req  : 0x0
[NOTE ]  ME:  CPU repl valid  : 0x1
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  FW update req   : 0x0
[NOTE ]  ME:  (Reserved)      : 0x0
[NOTE ]  ME:  Current state   : 0x50
[NOTE ]  ME:  Current PM event: 0x6
[NOTE ]  ME:  Progress code   : 0x1
[NOTE ]  ME: Requested BIOS Action: Continue to boot
[DEBUG]  ME: FW Partition Table      : OK
[DEBUG]  ME: Bringup Loader Failure  : NO
[DEBUG]  ME: Firmware Init Complete  : NO
[DEBUG]  ME: Manufacturing Mode      : NO
[DEBUG]  ME: Boot Options Present    : NO
[DEBUG]  ME: Update In Progress      : NO
[DEBUG]  ME: Current Working State   : Normal
[DEBUG]  ME: Current Operation State : M0 with UMA
[DEBUG]  ME: Current Operation Mode  : Normal
[DEBUG]  ME: Error Code              : No Error
[DEBUG]  ME: Progress Phase          : uKernel Phase
[DEBUG]  ME: Power Management Event  : Pseudo-global reset
[DEBUG]  ME: Progress Phase State    : Unknown 0x00
[DEBUG]  memcfg DDR3 ref clock 133 MHz
[DEBUG]  memcfg DDR3 clock 1596 MHz
[DEBUG]  memcfg channel assignment: A: 0, B  1, C  2
[DEBUG]  memcfg channel[0] config (00630020):
[DEBUG]     ECC inactive
[DEBUG]     enhanced interleave mode on
[DEBUG]     rank interleave on
[DEBUG]     DIMMA 8192 MB width x8 dual rank
[DEBUG]     DIMMB 0 MB width x8 single rank, selected
[DEBUG]  memcfg channel[1] config (00630020):
[DEBUG]     ECC inactive
[DEBUG]     enhanced interleave mode on
[DEBUG]     rank interleave on
[DEBUG]     DIMMA 8192 MB width x8 dual rank
[DEBUG]     DIMMB 0 MB width x8 single rank, selected
[INFO ]  Timestamp - after RAM initialization: 31313739589
[DEBUG]  CBMEM:
[DEBUG]  IMD: root @ 0x7ffff000 254 entries.
[DEBUG]  IMD: root @ 0x7fffec00 62 entries.
[DEBUG]  External stage cache:
[DEBUG]  IMD: root @ 0x803ff000 254 entries.
[DEBUG]  IMD: root @ 0x803fec00 62 entries.
[DEBUG]  FMAP: area RW_MRC_CACHE found @ 200000 (65536 bytes)
[DEBUG]  MRC: Checking cached data update for 'RW_MRC_CACHE'.
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 00000004 to 0890
[DEBUG]  read 03040003 from 0894
[DEBUG]  wrote 00001000 to 0890
[DEBUG]  read 09300024 from 0894
[DEBUG]  read 00000000 from 0880
[DEBUG]  wrote 00000000 to 0880
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 9f to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 44 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 001740ef from 07f0
[DEBUG]  read 00 from 07f4
[DEBUG]  wrote 0000 to 0874
[SPEW ]  SF: Got idcode: ef 40 17 00 00 
[INFO ]  Manufacturer: ef
[INFO ]  SF: Detected ef 4017 with sector size 0x1000, total 0x800000
[NOTE ]  MRC: no data in 'RW_MRC_CACHE'
[DEBUG]  MRC: cache data 'RW_MRC_CACHE' needs update.
[SPEW ]  PP: 0xfefef462 => cmd = { 0x02 0x200000 } chunk_len = 2
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200000 to 07e8
[DEBUG]  wrote 05 to 07f0
[DEBUG]  wrote 00 to 07f1
[DEBUG]  wrote 41 to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  SF: : Successfully programmed 2 bytes @ 0x200000
[SPEW ]  PP: 0xfefef4fe => cmd = { 0x02 0x200002 } chunk_len = 2
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200002 to 07e8
[DEBUG]  wrote 6a to 07f0
[DEBUG]  wrote 00 to 07f1
[DEBUG]  wrote 41 to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  SF: : Successfully programmed 2 bytes @ 0x200002
[SPEW ]  PP: 0xfefef49c => cmd = { 0x02 0x200050 } chunk_len = 20
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200050 to 07e8
[DEBUG]  wrote 6443524d to 07f0
[DEBUG]  wrote 00000634 to 07f4
[DEBUG]  wrote 285799c8 to 07f8
[DEBUG]  wrote 4ce1de47 to 07fc
[DEBUG]  wrote 00000005 to 0800
[DEBUG]  wrote 53 to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  SF: : Successfully programmed 20 bytes @ 0x200050
[SPEW ]  PP: 0xfefef90c => cmd = { 0x02 0x200064 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200064 to 07e8
[DEBUG]  wrote 3093fed3 to 07f0
[DEBUG]  wrote 7482fed3 to 07f4
[DEBUG]  wrote 000306a9 to 07f8
[DEBUG]  wrote 00000085 to 07fc
[DEBUG]  wrote 00000006 to 0800
[DEBUG]  wrote 000000fc to 0804
[DEBUG]  wrote 00000140 to 0808
[DEBUG]  wrote 00000d20 to 080c
[DEBUG]  wrote 0000000c to 0810
[DEBUG]  wrote 0000000b to 0814
[DEBUG]  wrote 00000005 to 0818
[DEBUG]  wrote 0000000b to 081c
[DEBUG]  wrote 0000001c to 0820
[DEBUG]  wrote 000000d0 to 0824
[DEBUG]  wrote 00000006 to 0828
[DEBUG]  wrote 00000006 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefef94c => cmd = { 0x02 0x2000a4 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002000a4 to 07e8
[DEBUG]  wrote 00000018 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 0000080b to 07fc
[DEBUG]  wrote 00001860 to 0800
[DEBUG]  wrote 0000000c to 0804
[DEBUG]  wrote 00000008 to 0808
[DEBUG]  wrote 00000006 to 080c
[DEBUG]  wrote 00000004 to 0810
[DEBUG]  wrote 00000014 to 0814
[DEBUG]  wrote 00000005 to 0818
[DEBUG]  wrote 00000008 to 081c
[DEBUG]  wrote 0c0c0193 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00630020 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefef98c => cmd = { 0x02 0x2000e4 } chunk_len = 28
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002000e4 to 07e8
[DEBUG]  wrote 00630020 to 07f0
[DEBUG]  wrote 00002000 to 07f4
[DEBUG]  wrote 00002000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 0000000c to 0804
[DEBUG]  wrote 0000000f to 0808
[DEBUG]  wrote 5b to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefef9a8 => cmd = { 0x02 0x200100 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200100 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000008 to 07f4
[DEBUG]  wrote 0000000d to 07f8
[DEBUG]  wrote 00000005 to 07fc
[DEBUG]  wrote 00000005 to 0800
[DEBUG]  wrote 0000000e to 0804
[DEBUG]  wrote 00000005 to 0808
[DEBUG]  wrote 00000005 to 080c
[DEBUG]  wrote 00000001 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000001 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefef9e8 => cmd = { 0x02 0x200140 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200140 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000001 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefa28 => cmd = { 0x02 0x200180 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200180 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefa68 => cmd = { 0x02 0x2001c0 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002001c0 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefaa8 => cmd = { 0x02 0x200200 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200200 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000228 to 0820
[DEBUG]  wrote fffffffd to 0824
[DEBUG]  wrote 27270006 to 0828
[DEBUG]  wrote 0000001e to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefae8 => cmd = { 0x02 0x200240 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200240 to 07e8
[DEBUG]  wrote 000000c4 to 07f0
[DEBUG]  wrote 26240012 to 07f4
[DEBUG]  wrote 00000035 to 07f8
[DEBUG]  wrote 000000db to 07fc
[DEBUG]  wrote 2825002a to 0800
[DEBUG]  wrote 00000055 to 0804
[DEBUG]  wrote 000000f9 to 0808
[DEBUG]  wrote 2725003a to 080c
[DEBUG]  wrote 00000021 to 0810
[DEBUG]  wrote 00000105 to 0814
[DEBUG]  wrote 26250057 to 0818
[DEBUG]  wrote 0000003b to 081c
[DEBUG]  wrote 00000120 to 0820
[DEBUG]  wrote 24220066 to 0824
[DEBUG]  wrote 00000047 to 0828
[DEBUG]  wrote 00000129 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefb28 => cmd = { 0x02 0x200280 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200280 to 07e8
[DEBUG]  wrote 2623007a to 07f0
[DEBUG]  wrote 0000004d to 07f4
[DEBUG]  wrote 00000131 to 07f8
[DEBUG]  wrote 2525008e to 07fc
[DEBUG]  wrote 00000057 to 0800
[DEBUG]  wrote 00000139 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000228 to 0814
[DEBUG]  wrote fffffffc to 0818
[DEBUG]  wrote 27260007 to 081c
[DEBUG]  wrote 00000019 to 0820
[DEBUG]  wrote 000000c0 to 0824
[DEBUG]  wrote 27240015 to 0828
[DEBUG]  wrote 00000039 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefb68 => cmd = { 0x02 0x2002c0 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002002c0 to 07e8
[DEBUG]  wrote 000000df to 07f0
[DEBUG]  wrote 2725002b to 07f4
[DEBUG]  wrote 0000004f to 07f8
[DEBUG]  wrote 000000f5 to 07fc
[DEBUG]  wrote 2726003b to 0800
[DEBUG]  wrote 00000026 to 0804
[DEBUG]  wrote 00000109 to 0808
[DEBUG]  wrote 26240057 to 080c
[DEBUG]  wrote 0000003b to 0810
[DEBUG]  wrote 00000120 to 0814
[DEBUG]  wrote 2423006b to 0818
[DEBUG]  wrote 00000049 to 081c
[DEBUG]  wrote 0000012c to 0820
[DEBUG]  wrote 2723007c to 0824
[DEBUG]  wrote 0000004f to 0828
[DEBUG]  wrote 00000133 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefba8 => cmd = { 0x02 0x200300 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200300 to 07e8
[DEBUG]  wrote 26240090 to 07f0
[DEBUG]  wrote 00000055 to 07f4
[DEBUG]  wrote 00000139 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefbe8 => cmd = { 0x02 0x200340 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200340 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefc28 => cmd = { 0x02 0x200380 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200380 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefc68 => cmd = { 0x02 0x2003c0 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002003c0 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefca8 => cmd = { 0x02 0x200400 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200400 to 07e8
[DEBUG]  wrote 00000228 to 07f0
[DEBUG]  wrote fffffffe to 07f4
[DEBUG]  wrote 2828002b to 07f8
[DEBUG]  wrote 0000001f to 07fc
[DEBUG]  wrote 000000c6 to 0800
[DEBUG]  wrote 2925003b to 0804
[DEBUG]  wrote 0000002e to 0808
[DEBUG]  wrote 000000d5 to 080c
[DEBUG]  wrote 29270051 to 0810
[DEBUG]  wrote 0000004e to 0814
[DEBUG]  wrote 000000f3 to 0818
[DEBUG]  wrote 2925005f to 081c
[DEBUG]  wrote 00000020 to 0820
[DEBUG]  wrote 00000105 to 0824
[DEBUG]  wrote 2827007e to 0828
[DEBUG]  wrote 00000037 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefce8 => cmd = { 0x02 0x200440 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200440 to 07e8
[DEBUG]  wrote 0000011e to 07f0
[DEBUG]  wrote 2725008d to 07f4
[DEBUG]  wrote 00000046 to 07f8
[DEBUG]  wrote 0000012c to 07fc
[DEBUG]  wrote 242500a3 to 0800
[DEBUG]  wrote 00000045 to 0804
[DEBUG]  wrote 0000012a to 0808
[DEBUG]  wrote 252600b3 to 080c
[DEBUG]  wrote 00000057 to 0810
[DEBUG]  wrote 0000013c to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000228 to 0824
[DEBUG]  wrote fffffffb to 0828
[DEBUG]  wrote 2827002c to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefd28 => cmd = { 0x02 0x200480 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200480 to 07e8
[DEBUG]  wrote 0000001c to 07f0
[DEBUG]  wrote 000000c3 to 07f4
[DEBUG]  wrote 2828003c to 07f8
[DEBUG]  wrote 00000035 to 07fc
[DEBUG]  wrote 000000dc to 0800
[DEBUG]  wrote 29290050 to 0804
[DEBUG]  wrote 00000053 to 0808
[DEBUG]  wrote 000000f9 to 080c
[DEBUG]  wrote 2726005f to 0810
[DEBUG]  wrote 0000001d to 0814
[DEBUG]  wrote 00000103 to 0818
[DEBUG]  wrote 26280082 to 081c
[DEBUG]  wrote 0000003b to 0820
[DEBUG]  wrote 00000121 to 0824
[DEBUG]  wrote 2627008e to 0828
[DEBUG]  wrote 0000004a to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefd68 => cmd = { 0x02 0x2004c0 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002004c0 to 07e8
[DEBUG]  wrote 0000012f to 07f0
[DEBUG]  wrote 262500a7 to 07f4
[DEBUG]  wrote 00000050 to 07f8
[DEBUG]  wrote 00000136 to 07fc
[DEBUG]  wrote 252600b1 to 0800
[DEBUG]  wrote 0000001c to 0804
[DEBUG]  wrote 00000140 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefda8 => cmd = { 0x02 0x200500 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200500 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00030000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefde8 => cmd = { 0x02 0x200540 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200540 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 0000000b to 0804
[DEBUG]  wrote 00000002 to 0808
[DEBUG]  wrote 000000fc to 080c
[DEBUG]  wrote 000011e7 to 0810
[DEBUG]  wrote 0a100208 to 0814
[DEBUG]  wrote 00002000 to 0818
[DEBUG]  wrote 00000140 to 081c
[DEBUG]  wrote 00000d20 to 0820
[DEBUG]  wrote 00000f00 to 0824
[DEBUG]  wrote 00000d20 to 0828
[DEBUG]  wrote 00000600 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefe28 => cmd = { 0x02 0x200580 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200580 to 07e8
[DEBUG]  wrote 00000d20 to 07f0
[DEBUG]  wrote 00002300 to 07f4
[DEBUG]  wrote 00003020 to 07f8
[DEBUG]  wrote 00010400 to 07fc
[DEBUG]  wrote 00000780 to 0800
[DEBUG]  wrote 00000780 to 0804
[DEBUG]  wrote 00001e00 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00070000 to 0810
[DEBUG]  wrote 000305dc to 0814
[DEBUG]  wrote 39399801 to 0818
[DEBUG]  wrote 37343555 to 081c
[DEBUG]  wrote 35302d31 to 0820
[DEBUG]  wrote 30412e30 to 0824
[DEBUG]  wrote 13004c30 to 0828
[DEBUG]  wrote 0034a530 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefe68 => cmd = { 0x02 0x2005c0 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 002005c0 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00000000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 00000000 to 081c
[DEBUG]  wrote 00000000 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00000000 to 0828
[DEBUG]  wrote 00000000 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefea8 => cmd = { 0x02 0x200600 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200600 to 07e8
[DEBUG]  wrote 00000000 to 07f0
[DEBUG]  wrote 00000000 to 07f4
[DEBUG]  wrote 00000000 to 07f8
[DEBUG]  wrote 00000000 to 07fc
[DEBUG]  wrote 00030000 to 0800
[DEBUG]  wrote 00000000 to 0804
[DEBUG]  wrote 00000000 to 0808
[DEBUG]  wrote 00000000 to 080c
[DEBUG]  wrote 00000000 to 0810
[DEBUG]  wrote 00000000 to 0814
[DEBUG]  wrote 00000000 to 0818
[DEBUG]  wrote 0000000b to 081c
[DEBUG]  wrote 00000002 to 0820
[DEBUG]  wrote 000000fc to 0824
[DEBUG]  wrote 000011e7 to 0828
[DEBUG]  wrote 0a100208 to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefefee8 => cmd = { 0x02 0x200640 } chunk_len = 64
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200640 to 07e8
[DEBUG]  wrote 00002000 to 07f0
[DEBUG]  wrote 00000140 to 07f4
[DEBUG]  wrote 00000d20 to 07f8
[DEBUG]  wrote 00000f00 to 07fc
[DEBUG]  wrote 00000d20 to 0800
[DEBUG]  wrote 00000600 to 0804
[DEBUG]  wrote 00000d20 to 0808
[DEBUG]  wrote 00002300 to 080c
[DEBUG]  wrote 00003020 to 0810
[DEBUG]  wrote 00010400 to 0814
[DEBUG]  wrote 00000780 to 0818
[DEBUG]  wrote 00000780 to 081c
[DEBUG]  wrote 00001e00 to 0820
[DEBUG]  wrote 00000000 to 0824
[DEBUG]  wrote 00070000 to 0828
[DEBUG]  wrote 000305dc to 082c
[DEBUG]  wrote 7f to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  PP: 0xfefeff28 => cmd = { 0x02 0x200680 } chunk_len = 24
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 06 to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0001 to 0876
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 0006 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 02 to 0878
[DEBUG]  read 0001 from 0876
[DEBUG]  wrote 0003 to 0876
[DEBUG]  read 0006 from 0874
[DEBUG]  wrote 00200680 to 07e8
[DEBUG]  wrote 39399801 to 07f0
[DEBUG]  wrote 37343555 to 07f4
[DEBUG]  wrote 35302d31 to 07f8
[DEBUG]  wrote 30412e30 to 07fc
[DEBUG]  wrote 11004c30 to 0800
[DEBUG]  wrote 0051f130 to 0804
[DEBUG]  wrote 57 to 0872
[DEBUG]  wrote 06 to 0871
[DEBUG]  read 0484 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  wrote 0000 to 0874
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 05 to 0878
[DEBUG]  read 0003 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 40 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 80 from 07f0
[DEBUG]  wrote 0000 to 0874
[SPEW ]  SF: : Successfully programmed 1588 bytes @ 0x200064
[DEBUG]  MRC: updated 'RW_MRC_CACHE'.
[DEBUG]  CBMEM entry for DIMM info: 0x7ffdb000
[INFO ]  POST: 0x3b
[INFO ]  POST: 0x3c
[INFO ]  POST: 0x3d
[INFO ]  POST: 0x3f
[DEBUG]  SMM Memory Map
[DEBUG]  SMRAM       : 0x80000000 0x800000
[DEBUG]   Subregion 0: 0x80000000 0x300000
[DEBUG]   Subregion 1: 0x80300000 0x100000
[DEBUG]   Subregion 2: 0x80400000 0x400000
[DEBUG]  Normal boot
[SPEW ]  CBFS DEBUG: _cbfs_alloc(name='fallback/postcar', alloc=0xfffe77e0(0xfefeff7c), force_ro=false, type=-1)
[INFO ]  CBFS: Found 'fallback/postcar' @0x31c80 size 0x81a8 in mcache @0xfeff1004
[SPEW ]  CBFS DEBUG: Decompressing 33192 bytes from 'fallback/postcar' to 0x7ffccfc0 with algo 0
[DEBUG]  Loading module at 0x7ffcd000 with entry 0x7ffcd031. filesize: 0x77c8 memsize: 0xdb20
[DEBUG]  Processing 616 relocs. Offset value of 0x7dfcd000
[INFO ]  Timestamp - end of romstage: 46257144456
[DEBUG]  BS: bootblock times (exec / console): total (unknown) / 14648 ms


[NOTE ]  coreboot-25.03-250-g59e4095ecfcb-dirty Mon Apr 21 05:10:24 UTC 2025 x86_32 postcar starting (log level: 7)...
[INFO ]  Timestamp - start of postcar: 46333434444
[INFO ]  Timestamp - end of postcar: 46348470937
[DEBUG]  Normal boot
[INFO ]  Timestamp - starting to load ramstage: 46370539067
[INFO ]  CBFS: Found 'fallback/ramstage' @0x68c0 size 0x1fe6e in mcache @0x7ffdc05c
[INFO ]  Timestamp - starting LZMA decompress (ignore for x86): 46411163666
[INFO ]  Timestamp - finished LZMA decompress (ignore for x86): 46556656506
[DEBUG]  Loading module at 0x7fe79000 with entry 0x7fe79000. filesize: 0x43768 memsize: 0x152878
[DEBUG]  Processing 6504 relocs. Offset value of 0x7be79000
[INFO ]  Timestamp - finished loading ramstage: 46622169319
[DEBUG]  BS: postcar times (exec / console): total (unknown) / 75 ms


[NOTE ]  coreboot-25.03-250-g59e4095ecfcb-dirty Mon Apr 21 05:10:24 UTC 2025 x86_32 ramstage starting (log level: 7)...
[INFO ]  POST: 0x39
[INFO ]  Timestamp - start of ramstage: 46701556145
[INFO ]  POST: 0x6f
[DEBUG]  Normal boot
[INFO ]  POST: 0x70
[DEBUG]  BS: BS_PRE_DEVICE run times (exec / console): 0 / 3 ms
[INFO ]  POST: 0x71
[INFO ]  Timestamp - early chipset initialization: 46764486580
[DEBUG]  BS: BS_DEV_INIT_CHIPS run times (exec / console): 0 / 9 ms
[INFO ]  POST: 0x72
[INFO ]  Timestamp - device enumeration: 46809322733
[INFO ]  Enumerating buses...
[DEBUG]  Root Device scanning...
[DEBUG]  CPU_CLUSTER: 0 enabled
[DEBUG]  DOMAIN: 00000000 enabled
[DEBUG]  DOMAIN: 00000000 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 00
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:00:00.0 [8086/0150] enabled
[DEBUG]  PCI: 00:00:01.0 [8086/0151] enabled
[INFO ]  PCI: Static device PCI: 00:00:01.1 not found, disabling it.
[DEBUG]  PCI: 00:00:01.2 [0000/0000] hidden
[INFO ]  PCI: Static device PCI: 00:00:02.0 not found, disabling it.
[DEBUG]  PCI: 00:00:04.0 [0000/0000] hidden
[DEBUG]  PCI: 00:00:06.0 [0000/0000] hidden
[DEBUG]  PCI: 00:00:14.0 [8086/1e31] enabled
[DEBUG]  PCI: 00:00:16.0 [8086/1e3a] enabled
[DEBUG]  PCI: 00:00:16.1: Disabling device
[DEBUG]  PCI: 00:00:16.1 [8086/1e3b] disabled No operations
[DEBUG]  PCI: 00:00:16.2: Disabling device
[DEBUG]  PCI: 00:00:16.3: Disabling device
[DEBUG]  PCI: 00:00:19.0 [8086/1503] enabled
[DEBUG]  PCI: 00:00:1a.0 [8086/1e2d] enabled
[DEBUG]  PCI: 00:00:1b.0 [8086/1e20] enabled
[DEBUG]  PCI: 00:00:1c.0: Found a downstream device
[DEBUG]  PCI: 00:00:1c.0 [8086/1e10] enabled
[DEBUG]  PCI: 00:00:1c.1: Found a downstream device
[INFO ]  PCI: Static device PCI: 00:00:1c.1 not found, disabling it.
[DEBUG]  PCI: 00:00:1c.2: No downstream device
[DEBUG]  PCI: 00:00:1c.2: Disabling device
[DEBUG]  PCI: 00:00:1c.2 [8086/1e14] disabled
[DEBUG]  PCI: 00:00:1c.3: Found a downstream device
[DEBUG]  PCI: 00:00:1c.3 [8086/1e16] enabled
[DEBUG]  PCI: 00:00:1c.4: Found a downstream device
[DEBUG]  PCI: 00:00:1c.4 [8086/1e18] enabled
[DEBUG]  PCI: 00:00:1c.5: No downstream device
[DEBUG]  PCI: 00:00:1c.5: Disabling device
[DEBUG]  PCI: 00:00:1c.5 [8086/1e1a] disabled
[DEBUG]  PCI: 00:00:1c.6: No downstream device
[DEBUG]  PCI: 00:00:1c.6: Disabling device
[DEBUG]  PCI: 00:00:1c.6 [8086/1e1c] disabled
[DEBUG]  PCI: 00:00:1c.7: Found a downstream device
[DEBUG]  PCI: 00:00:1c.7 [8086/1e1e] enabled
[DEBUG]  PCI: 00:00:1d.0 [8086/1e26] enabled
[DEBUG]  PCI: 00:00:1e.0: Disabling device
[DEBUG]  PCI: 00:00:1e.0 [8086/244e] disabled
[DEBUG]  PCI: 00:00:1f.0 [8086/1e44] enabled
[DEBUG]  PCI: 00:00:1f.2 [8086/1e00] enabled
[DEBUG]  PCI: 00:00:1f.3 [8086/1e22] enabled
[DEBUG]  PCI: 00:00:1f.5: Disabling device
[DEBUG]  PCI: 00:00:1f.5 [8086/1e08] disabled No operations
[DEBUG]  PCI: 00:00:1f.6: Disabling device
[DEBUG]  PCI: 00:00:1f.6 [8086/1e24] disabled No operations
[WARN ]  PCI: Leftover static devices:
[WARN ]  PCI: 00:00:01.1
[WARN ]  PCI: 00:00:02.0
[WARN ]  PCI: 00:00:1c.1
[WARN ]  PCI: Check your devicetree.cb.
[DEBUG]  PCI: 00:00:01.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 01
[INFO ]  POST: 0x24
[INFO ]  POST: 0x25
[INFO ]  PCI: 00:00:01.0: Setting Max_Payload_Size to 256 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:01.0 finished in 19 msecs
[DEBUG]  PCI: 00:00:01.2 scanning...
[DEBUG]  scan_bus: bus PCI: 00:00:01.2 finished in 0 msecs
[DEBUG]  PCI: 00:00:04.0 scanning...
[DEBUG]  scan_bus: bus PCI: 00:00:04.0 finished in 0 msecs
[DEBUG]  PCI: 00:00:06.0 scanning...
[DEBUG]  scan_bus: bus PCI: 00:00:06.0 finished in 0 msecs
[DEBUG]  PCI: 00:00:1c.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 02
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:02:00.0 subordinate bus PCI Express
[DEBUG]  PCI: 00:02:00.0 [12d8/2304] enabled
[DEBUG]  PCI: 00:02:00.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 03
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:03:01.0 subordinate bus PCI Express
[DEBUG]  PCI: 00:03:01.0 [12d8/2304] enabled
[DEBUG]  PCI: 00:03:02.0 subordinate bus PCI Express
[DEBUG]  PCI: 00:03:02.0 [12d8/2304] enabled
[DEBUG]  PCI: 00:03:01.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 04
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:04:00.0 [1b21/0612] enabled
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[DEBUG]  PCI: 00:04:00.0: No LTR support
[DEBUG]  scan_bus: bus PCI: 00:03:01.0 finished in 32 msecs
[DEBUG]  PCI: 00:03:02.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 05
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:05:00.0 [1b6f/7023] enabled
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  ASPM: Enabled None
[DEBUG]  PCI: 00:05:00.0: No LTR support
[DEBUG]  scan_bus: bus PCI: 00:03:02.0 finished in 27 msecs
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[INFO ]  PCIe: Common Clock Configuration already enabled
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[DEBUG]  scan_bus: bus PCI: 00:02:00.0 finished in 137 msecs
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[INFO ]  PCI: 00:00:1c.0: Setting Max_Payload_Size to 128 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:1c.0 finished in 189 msecs
[DEBUG]  PCI: 00:00:1c.3 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 06
[INFO ]  POST: 0x24
[INFO ]  Disabling ASPM for PCI: 00:06:00.0 [1b21/0611]
[INFO ]  Setting AHCI mode for PCI: 00:06:00.0 [1b21/0611]
[DEBUG]  PCI: 00:06:00.0 [1b21/0611] enabled
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  PCIE CLK PM is not supported by endpoint
[DEBUG]  PCI: 00:06:00.0: No LTR support
[INFO ]  PCI: 00:00:1c.3: Setting Max_Payload_Size to 128 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:1c.3 finished in 49 msecs
[DEBUG]  PCI: 00:00:1c.4 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 07
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:07:00.0 subordinate PCI
[DEBUG]  PCI: 00:07:00.0 [1b21/1080] enabled
[DEBUG]  PCI: 00:07:00.0 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 08
[INFO ]  POST: 0x24
[INFO ]  POST: 0x25
[DEBUG]  scan_bus: bus PCI: 00:07:00.0 finished in 10 msecs
[INFO ]  POST: 0x25
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[DEBUG]  PCI: 00:07:00.0: No LTR support
[INFO ]  PCI: 00:00:1c.4: Setting Max_Payload_Size to 128 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:1c.4 finished in 61 msecs
[DEBUG]  PCI: 00:00:1c.7 scanning...
[DEBUG]  PCI: pci_scan_bus for segment group 00 bus 09
[INFO ]  POST: 0x24
[DEBUG]  PCI: 00:09:00.0 [1b21/1042] enabled
[INFO ]  POST: 0x25
[INFO ]  Enabling Common Clock Configuration
[INFO ]  PCIE CLK PM is not supported by endpoint
[INFO ]  ASPM: Enabled None
[DEBUG]  PCI: 00:09:00.0: No LTR support
[INFO ]  PCI: 00:00:1c.7: Setting Max_Payload_Size to 128 for devices under this root port
[DEBUG]  scan_bus: bus PCI: 00:00:1c.7 finished in 41 msecs
[DEBUG]  PCI: 00:00:1f.0 scanning...
[DEBUG]  PNP: 002e.1 disabled
[DEBUG]  PNP: 002e.2 enabled
[DEBUG]  PNP: 002e.3 disabled
[DEBUG]  PNP: 002e.5 enabled
[DEBUG]  PNP: 002e.6 disabled
[DEBUG]  PNP: 002e.7 disabled
[DEBUG]  PNP: 002e.8 disabled
[DEBUG]  PNP: 002e.108 enabled
[DEBUG]  PNP: 002e.109 enabled
[DEBUG]  PNP: 002e.209 enabled
[DEBUG]  PNP: 002e.309 enabled
[DEBUG]  PNP: 002e.509 enabled
[DEBUG]  PNP: 002e.a enabled
[DEBUG]  PNP: 002e.b enabled
[DEBUG]  PNP: 002e.d disabled
[DEBUG]  PNP: 002e.e disabled
[DEBUG]  PNP: 002e.f disabled
[DEBUG]  PNP: 002e.14 disabled
[DEBUG]  PNP: 002e.16 disabled
[DEBUG]  PNP: 0c31.0 enabled
[DEBUG]  PNP: 002e.308 enabled
[DEBUG]  PNP: 002e.409 enabled
[DEBUG]  PNP: 002e.609 enabled
[DEBUG]  PNP: 002e.709 enabled
[DEBUG]  PNP: 002e.9 enabled
[DEBUG]  scan_bus: bus PCI: 00:00:1f.0 finished in 84 msecs
[DEBUG]  PCI: 00:00:1f.3 scanning...
[DEBUG]  scan_bus: bus PCI: 00:00:1f.3 finished in 0 msecs
[INFO ]  POST: 0x25
[DEBUG]  scan_bus: bus DOMAIN: 00000000 finished in 795 msecs
[DEBUG]  scan_bus: bus Root Device finished in 813 msecs
[INFO ]  done
[DEBUG]  BS: BS_DEV_ENUMERATE run times (exec / console): 3 / 833 ms
[DEBUG]  BM-LOCKDOWN: Enabling boot media protection scheme 'readonly' using CTRL...
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 00000004 to 0890
[DEBUG]  read 03040003 from 0894
[DEBUG]  wrote 00001000 to 0890
[DEBUG]  read 09300024 from 0894
[DEBUG]  read 00000000 from 0880
[DEBUG]  wrote 00000000 to 0880
[DEBUG]  read 0080 from 0870
[DEBUG]  wrote 000c to 0870
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 9f to 0878
[DEBUG]  read 0000 from 0876
[DEBUG]  wrote 0000 to 0876
[DEBUG]  read 0000 from 0874
[DEBUG]  wrote 00000000 to 07e8
[DEBUG]  wrote 44 to 0872
[DEBUG]  wrote 02 to 0871
[DEBUG]  read 0084 from 0870
[DEBUG]  wrote 0004 to 0870
[DEBUG]  read 001740ef from 07f0
[DEBUG]  read 00 from 07f4
[DEBUG]  wrote 0000 to 0874
[INFO ]  Manufacturer: ef
[INFO ]  SF: Detected ef 4017 with sector size 0x1000, total 0x800000
[INFO ]  spi_flash_protect: FPR 0 is enabled for range 0x00000000-0x007fffff
[INFO ]  BM-LOCKDOWN: Enabled bootmedia protection
[DEBUG]  BS: BS_DEV_RESOURCES entry times (exec / console): 0 / 104 ms
[INFO ]  POST: 0x73
[INFO ]  Timestamp - device configuration: 49575226573
[INFO ]  Allocating resources...
[INFO ]  Reading resources...
[DEBUG]  Adding PCIe enhanced config space BAR 0xf0000000-0xf4000000.
[DEBUG]  TOUUD 0x47a600000 TOLUD 0x84a00000 TOM 0x400000000
[DEBUG]  MEBASE 0x3ff000000
[DEBUG]  IGD decoded, subtracting 64M UMA and 2M GTT
[DEBUG]  TSEG base 0x80000000 size 8M
[INFO ]  Available memory below 4GB: 2048M
[INFO ]  Available memory above 4GB: 14246M
[INFO ]  Done reading resources.
[INFO ]  === Resource allocator: DOMAIN: 00000000 - Pass 1 (relative placement) ===
[DEBUG]     PCI: 00:03:01.0 io: size: 0 align: 12 gran: 12 limit: ffffffff
[DEBUG]      PCI: 00:04:00.0 20 *  [0x0 - 0x1f] io
[DEBUG]      PCI: 00:04:00.0 10 *  [0x20 - 0x27] io
[DEBUG]      PCI: 00:04:00.0 18 *  [0x28 - 0x2f] io
[DEBUG]      PCI: 00:04:00.0 14 *  [0x30 - 0x33] io
[DEBUG]      PCI: 00:04:00.0 1c *  [0x34 - 0x37] io
[DEBUG]     PCI: 00:03:01.0 io: size: 1000 align: 12 gran: 12 limit: ffff done
[DEBUG]     PCI: 00:03:02.0 io: size: 0 align: 12 gran: 12 limit: ffffffff
[DEBUG]     PCI: 00:03:02.0 io: size: 0 align: 12 gran: 12 limit: ffffffff done
[DEBUG]    PCI: 00:02:00.0 io: size: 0 align: 12 gran: 12 limit: ffffffff
[DEBUG]     PCI: 00:03:01.0 1c *  [0x0 - 0xfff] io
[DEBUG]    PCI: 00:02:00.0 io: size: 1000 align: 12 gran: 12 limit: ffff done
[DEBUG]   PCI: 00:00:1c.0 io: size: 0 align: 12 gran: 12 limit: ffff
[DEBUG]    PCI: 00:02:00.0 1c *  [0x0 - 0xfff] io
[DEBUG]   PCI: 00:00:1c.0 io: size: 1000 align: 12 gran: 12 limit: ffff done
[DEBUG]     PCI: 00:03:01.0 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]      PCI: 00:04:00.0 30 *  [0x0 - 0xffff] mem
[DEBUG]      PCI: 00:04:00.0 24 *  [0x10000 - 0x101ff] mem
[DEBUG]     PCI: 00:03:01.0 mem: size: 100000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]     PCI: 00:03:02.0 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]      PCI: 00:05:00.0 10 *  [0x0 - 0x7fff] mem
[DEBUG]     PCI: 00:03:02.0 mem: size: 100000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]    PCI: 00:02:00.0 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]     PCI: 00:03:01.0 20 *  [0x0 - 0xfffff] mem
[DEBUG]     PCI: 00:03:02.0 20 *  [0x100000 - 0x1fffff] mem
[DEBUG]    PCI: 00:02:00.0 mem: size: 200000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]   PCI: 00:00:1c.0 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]    PCI: 00:02:00.0 20 *  [0x0 - 0x1fffff] mem
[DEBUG]   PCI: 00:00:1c.0 mem: size: 200000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]     PCI: 00:03:01.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]     PCI: 00:03:01.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]     PCI: 00:03:02.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]     PCI: 00:03:02.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]    PCI: 00:02:00.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]    PCI: 00:02:00.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]   PCI: 00:00:1c.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]   PCI: 00:00:1c.0 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]   PCI: 00:00:1c.3 io: size: 0 align: 12 gran: 12 limit: ffff
[DEBUG]    PCI: 00:06:00.0 20 *  [0x0 - 0x1f] io
[DEBUG]    PCI: 00:06:00.0 10 *  [0x20 - 0x27] io
[DEBUG]    PCI: 00:06:00.0 18 *  [0x28 - 0x2f] io
[DEBUG]    PCI: 00:06:00.0 14 *  [0x30 - 0x33] io
[DEBUG]    PCI: 00:06:00.0 1c *  [0x34 - 0x37] io
[DEBUG]   PCI: 00:00:1c.3 io: size: 1000 align: 12 gran: 12 limit: ffff done
[DEBUG]   PCI: 00:00:1c.3 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]    PCI: 00:06:00.0 24 *  [0x0 - 0x1ff] mem
[DEBUG]   PCI: 00:00:1c.3 mem: size: 100000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]   PCI: 00:00:1c.3 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]   PCI: 00:00:1c.3 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]   PCI: 00:00:1c.4 io: size: 0 align: 12 gran: 12 limit: ffff
[DEBUG]   PCI: 00:00:1c.4 io: size: 0 align: 12 gran: 12 limit: ffff done
[DEBUG]   PCI: 00:00:1c.4 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]   PCI: 00:00:1c.4 mem: size: 0 align: 20 gran: 20 limit: ffffffff done
[DEBUG]   PCI: 00:00:1c.4 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]   PCI: 00:00:1c.4 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[DEBUG]   PCI: 00:00:1c.7 io: size: 0 align: 12 gran: 12 limit: ffff
[DEBUG]   PCI: 00:00:1c.7 io: size: 0 align: 12 gran: 12 limit: ffff done
[DEBUG]   PCI: 00:00:1c.7 mem: size: 0 align: 20 gran: 20 limit: ffffffff
[DEBUG]    PCI: 00:09:00.0 10 *  [0x0 - 0x7fff] mem
[DEBUG]   PCI: 00:00:1c.7 mem: size: 100000 align: 20 gran: 20 limit: ffffffff done
[DEBUG]   PCI: 00:00:1c.7 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff
[DEBUG]   PCI: 00:00:1c.7 prefmem: size: 0 align: 20 gran: 20 limit: ffffffffffffffff done
[INFO ]  === Resource allocator: DOMAIN: 00000000 - Pass 2 (allocating resources) ===
[DEBUG]  DOMAIN: 00000000 io: base: 0 size: 0 align: 0 gran: 0 limit: ffff
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 10000000 base 00000000 limit 00000fff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.2 60 base 000003f8 limit 000003ff io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.5 60 base 00000060 limit 00000060 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.5 62 base 00000064 limit 00000064 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.b 60 base 00000290 limit 00000291 io (fixed)
[DEBUG]   avoid_fixed_resources: PNP: 002e.b 62 base 00000000 limit 00000001 io (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.3 20 base 00000400 limit 0000041f io (fixed)
[INFO ]   DOMAIN: 00000000: Resource ranges:
[INFO ]   * Base: 1000, Size: f000, Tag: 100
[DEBUG]    PCI: 00:00:1c.0 1c *  [0xf000 - 0xffff] limit: ffff io
[DEBUG]    PCI: 00:00:1c.3 1c *  [0xe000 - 0xefff] limit: efff io
[DEBUG]    PCI: 00:00:19.0 18 *  [0xdfe0 - 0xdfff] limit: dfff io
[DEBUG]    PCI: 00:00:1f.2 20 *  [0xdfc0 - 0xdfdf] limit: dfdf io
[ERROR]  Resource didn't fit!!!
[DEBUG]    PNP: 002e.308 60 *  size: 0x8 limit: fff io
[DEBUG]    PCI: 00:00:1f.2 10 *  [0xdfb8 - 0xdfbf] limit: dfbf io
[DEBUG]    PCI: 00:00:1f.2 18 *  [0xdfb0 - 0xdfb7] limit: dfb7 io
[DEBUG]    PCI: 00:00:1f.2 14 *  [0xdfac - 0xdfaf] limit: dfaf io
[DEBUG]    PCI: 00:00:1f.2 1c *  [0xdfa8 - 0xdfab] limit: dfab io
[DEBUG]  DOMAIN: 00000000 io: base: 0 size: 0 align: 0 gran: 0 limit: ffff done
[DEBUG]  DOMAIN: 00000000 mem: base: 80000000 size: 0 align: 0 gran: 0 limit: efffffff
[DEBUG]  DOMAIN: 00000000 mem: base: 100000000 size: 0 align: 0 gran: 0 limit: fffffffff
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 60 base f0000000 limit f3ffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 03 base 00000000 limit 0009ffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 04 base 00100000 limit 7fffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 05 base 100000000 limit 47a5fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 06 base 80000000 limit 849fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 07 base 000a0000 limit 000bffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 08 base 000c0000 limit 000fffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 09 base fed90000 limit fed90fff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:00.0 0a base fed91000 limit fed91fff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 10000100 base ff000000 limit ffffffff mem (fixed)
[DEBUG]   avoid_fixed_resources: PCI: 00:00:1f.0 03 base fec00000 limit fec00fff mem (fixed)
[INFO ]   DOMAIN: 00000000: Resource ranges:
[INFO ]   * Base: 84a00000, Size: 6b600000, Tag: 200
[INFO ]   * Base: 47a600000, Size: b85a00000, Tag: 200
[DEBUG]    PCI: 00:00:1c.0 20 *  [0xefe00000 - 0xefffffff] limit: efffffff mem
[DEBUG]    PCI: 00:00:1c.3 20 *  [0xefd00000 - 0xefdfffff] limit: efdfffff mem
[DEBUG]    PCI: 00:00:1c.7 20 *  [0xefc00000 - 0xefcfffff] limit: efcfffff mem
[DEBUG]    PCI: 00:00:19.0 10 *  [0xefbe0000 - 0xefbfffff] limit: efbfffff mem
[DEBUG]    PCI: 00:00:14.0 10 *  [0xefbd0000 - 0xefbdffff] limit: efbdffff mem
[DEBUG]    PCI: 00:00:1b.0 10 *  [0xefbcc000 - 0xefbcffff] limit: efbcffff mem
[DEBUG]    PCI: 00:00:19.0 14 *  [0xefbcb000 - 0xefbcbfff] limit: efbcbfff mem
[DEBUG]    PCI: 00:00:1f.2 24 *  [0xefbca000 - 0xefbca7ff] limit: efbca7ff mem
[DEBUG]    PCI: 00:00:1a.0 10 *  [0xefbc9000 - 0xefbc93ff] limit: efbc93ff mem
[DEBUG]    PCI: 00:00:1d.0 10 *  [0xefbc8000 - 0xefbc83ff] limit: efbc83ff mem
[DEBUG]    PCI: 00:00:1f.3 10 *  [0xefbc7000 - 0xefbc70ff] limit: efbc70ff mem
[DEBUG]    PCI: 00:00:16.0 10 *  [0xefbc6000 - 0xefbc600f] limit: efbc600f mem
[DEBUG]  DOMAIN: 00000000 mem: base: 80000000 size: 0 align: 0 gran: 0 limit: efffffff done
[DEBUG]  DOMAIN: 00000000 mem: base: 100000000 size: 0 align: 0 gran: 0 limit: fffffffff done
[DEBUG]    PCI: 00:02:00.0 1c *  [0xf000 - 0xffff] limit: ffff io
[DEBUG]    PCI: 00:02:00.0 20 *  [0xefe00000 - 0xefffffff] limit: efffffff mem
[DEBUG]    PCI: 00:03:01.0 1c *  [0xf000 - 0xffff] limit: ffff io
[DEBUG]    PCI: 00:03:01.0 20 *  [0xefe00000 - 0xefefffff] limit: efefffff mem
[DEBUG]    PCI: 00:03:02.0 20 *  [0xeff00000 - 0xefffffff] limit: efffffff mem
[DEBUG]    PCI: 00:04:00.0 10 *  [0xf020 - 0xf027] limit: f027 io
[DEBUG]    PCI: 00:04:00.0 14 *  [0xf030 - 0xf033] limit: f033 io
[DEBUG]    PCI: 00:04:00.0 18 *  [0xf028 - 0xf02f] limit: f02f io
[DEBUG]    PCI: 00:04:00.0 1c *  [0xf034 - 0xf037] limit: f037 io
[DEBUG]    PCI: 00:04:00.0 20 *  [0xf000 - 0xf01f] limit: f01f io
[DEBUG]    PCI: 00:04:00.0 24 *  [0xefe10000 - 0xefe101ff] limit: efe101ff mem
[DEBUG]    PCI: 00:04:00.0 30 *  [0xefe00000 - 0xefe0ffff] limit: efe0ffff mem
[DEBUG]    PCI: 00:05:00.0 10 *  [0xeff00000 - 0xeff07fff] limit: eff07fff mem
[DEBUG]    PCI: 00:06:00.0 10 *  [0xe020 - 0xe027] limit: e027 io
[DEBUG]    PCI: 00:06:00.0 14 *  [0xe030 - 0xe033] limit: e033 io
[DEBUG]    PCI: 00:06:00.0 18 *  [0xe028 - 0xe02f] limit: e02f io
[DEBUG]    PCI: 00:06:00.0 1c *  [0xe034 - 0xe037] limit: e037 io
[DEBUG]    PCI: 00:06:00.0 20 *  [0xe000 - 0xe01f] limit: e01f io
[DEBUG]    PCI: 00:06:00.0 24 *  [0xefd00000 - 0xefd001ff] limit: efd001ff mem
[DEBUG]    PCI: 00:09:00.0 10 *  [0xefc00000 - 0xefc07fff] limit: efc07fff mem
[INFO ]  === Resource allocator: DOMAIN: 00000000 - resource allocation complete ===
[DEBUG]  PCI: 00:00:01.0 1c <- [0x000000000000ffff - 0x000000000000fffe] size 0x00000000 gran 0x0c seg 00 bus 01 io
[DEBUG]  PCI: 00:00:01.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 01 prefmem
[DEBUG]  PCI: 00:00:01.0 20 <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x14 seg 00 bus 01 mem
[DEBUG]  PCI: 00:00:14.0 10 <- [0x00000000efbd0000 - 0x00000000efbdffff] size 0x00010000 gran 0x10 mem64
[DEBUG]  PCI: 00:00:16.0 10 <- [0x00000000efbc6000 - 0x00000000efbc600f] size 0x00000010 gran 0x04 mem64
[DEBUG]  PCI: 00:00:19.0 10 <- [0x00000000efbe0000 - 0x00000000efbfffff] size 0x00020000 gran 0x11 mem
[DEBUG]  PCI: 00:00:19.0 14 <- [0x00000000efbcb000 - 0x00000000efbcbfff] size 0x00001000 gran 0x0c mem
[DEBUG]  PCI: 00:00:19.0 18 <- [0x000000000000dfe0 - 0x000000000000dfff] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:00:1a.0 10 <- [0x00000000efbc9000 - 0x00000000efbc93ff] size 0x00000400 gran 0x0a mem
[DEBUG]  PCI: 00:00:1b.0 10 <- [0x00000000efbcc000 - 0x00000000efbcffff] size 0x00004000 gran 0x0e mem64
[DEBUG]  PCI: 00:00:1c.0 1c <- [0x000000000000f000 - 0x000000000000ffff] size 0x00001000 gran 0x0c seg 00 bus 02 io
[DEBUG]  PCI: 00:00:1c.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 02 prefmem
[DEBUG]  PCI: 00:00:1c.0 20 <- [0x00000000efe00000 - 0x00000000efffffff] size 0x00200000 gran 0x14 seg 00 bus 02 mem
[DEBUG]  PCI: 00:02:00.0 1c <- [0x000000000000f000 - 0x000000000000ffff] size 0x00001000 gran 0x0c seg 00 bus 03 io
[DEBUG]  PCI: 00:02:00.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 03 prefmem
[DEBUG]  PCI: 00:02:00.0 20 <- [0x00000000efe00000 - 0x00000000efffffff] size 0x00200000 gran 0x14 seg 00 bus 03 mem
[DEBUG]  PCI: 00:03:01.0 1c <- [0x000000000000f000 - 0x000000000000ffff] size 0x00001000 gran 0x0c seg 00 bus 04 io
[DEBUG]  PCI: 00:03:01.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 04 prefmem
[DEBUG]  PCI: 00:03:01.0 20 <- [0x00000000efe00000 - 0x00000000efefffff] size 0x00100000 gran 0x14 seg 00 bus 04 mem
[DEBUG]  PCI: 00:04:00.0 10 <- [0x000000000000f020 - 0x000000000000f027] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:04:00.0 14 <- [0x000000000000f030 - 0x000000000000f033] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:04:00.0 18 <- [0x000000000000f028 - 0x000000000000f02f] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:04:00.0 1c <- [0x000000000000f034 - 0x000000000000f037] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:04:00.0 20 <- [0x000000000000f000 - 0x000000000000f01f] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:04:00.0 24 <- [0x00000000efe10000 - 0x00000000efe101ff] size 0x00000200 gran 0x09 mem
[DEBUG]  PCI: 00:04:00.0 30 <- [0x00000000efe00000 - 0x00000000efe0ffff] size 0x00010000 gran 0x10 romem
[DEBUG]  PCI: 00:03:02.0 1c <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x0c seg 00 bus 05 io
[DEBUG]  PCI: 00:03:02.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 05 prefmem
[DEBUG]  PCI: 00:03:02.0 20 <- [0x00000000eff00000 - 0x00000000efffffff] size 0x00100000 gran 0x14 seg 00 bus 05 mem
[DEBUG]  PCI: 00:05:00.0 10 <- [0x00000000eff00000 - 0x00000000eff07fff] size 0x00008000 gran 0x0f mem64
[DEBUG]  PCI: 00:00:1c.3 1c <- [0x000000000000e000 - 0x000000000000efff] size 0x00001000 gran 0x0c seg 00 bus 06 io
[DEBUG]  PCI: 00:00:1c.3 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 06 prefmem
[DEBUG]  PCI: 00:00:1c.3 20 <- [0x00000000efd00000 - 0x00000000efdfffff] size 0x00100000 gran 0x14 seg 00 bus 06 mem
[DEBUG]  PCI: 00:06:00.0 10 <- [0x000000000000e020 - 0x000000000000e027] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:06:00.0 14 <- [0x000000000000e030 - 0x000000000000e033] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:06:00.0 18 <- [0x000000000000e028 - 0x000000000000e02f] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:06:00.0 1c <- [0x000000000000e034 - 0x000000000000e037] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:06:00.0 20 <- [0x000000000000e000 - 0x000000000000e01f] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:06:00.0 24 <- [0x00000000efd00000 - 0x00000000efd001ff] size 0x00000200 gran 0x09 mem
[DEBUG]  PCI: 00:00:1c.4 1c <- [0x000000000000ffff - 0x000000000000fffe] size 0x00000000 gran 0x0c seg 00 bus 07 io
[DEBUG]  PCI: 00:00:1c.4 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 07 prefmem
[DEBUG]  PCI: 00:00:1c.4 20 <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x14 seg 00 bus 07 mem
[DEBUG]  PCI: 00:07:00.0 1c <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x0c seg 00 bus 08 io
[DEBUG]  PCI: 00:07:00.0 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 08 prefmem
[DEBUG]  PCI: 00:07:00.0 20 <- [0x00000000ffffffff - 0x00000000fffffffe] size 0x00000000 gran 0x14 seg 00 bus 08 mem
[DEBUG]  PCI: 00:00:1c.7 1c <- [0x000000000000ffff - 0x000000000000fffe] size 0x00000000 gran 0x0c seg 00 bus 09 io
[DEBUG]  PCI: 00:00:1c.7 24 <- [0xffffffffffffffff - 0xfffffffffffffffe] size 0x00000000 gran 0x14 seg 00 bus 09 prefmem
[DEBUG]  PCI: 00:00:1c.7 20 <- [0x00000000efc00000 - 0x00000000efcfffff] size 0x00100000 gran 0x14 seg 00 bus 09 mem
[DEBUG]  PCI: 00:09:00.0 10 <- [0x00000000efc00000 - 0x00000000efc07fff] size 0x00008000 gran 0x0f mem64
[DEBUG]  PCI: 00:00:1d.0 10 <- [0x00000000efbc8000 - 0x00000000efbc83ff] size 0x00000400 gran 0x0a mem
[DEBUG]  PNP: 002e.2 60 <- [0x00000000000003f8 - 0x00000000000003ff] size 0x00000008 gran 0x03 io
[DEBUG]  PNP: 002e.2 70 <- [0x0000000000000004 - 0x0000000000000004] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.5 60 <- [0x0000000000000060 - 0x0000000000000060] size 0x00000001 gran 0x00 io
[DEBUG]  PNP: 002e.5 62 <- [0x0000000000000064 - 0x0000000000000064] size 0x00000001 gran 0x00 io
[DEBUG]  PNP: 002e.5 70 <- [0x0000000000000001 - 0x0000000000000001] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.5 72 <- [0x000000000000000c - 0x000000000000000c] size 0x00000001 gran 0x00 irq
[DEBUG]  PNP: 002e.5 f0 <- [0x0000000000000082 - 0x0000000000000081] size 0x00000000 gran 0x00 drq
[DEBUG]  PNP: 002e.209 e0 <- [0x00000000000000df - 0x00000000000000de] size 0x00000000 gran 0x00 drq
[NOTE ]  PNP: 002e.509 f4 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.509 f5 irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PNP: 002e.a e3 <- [0x0000000000000004 - 0x0000000000000003] size 0x00000000 gran 0x00 drq
[DEBUG]  PNP: 002e.a e7 <- [0x0000000000000011 - 0x0000000000000010] size 0x00000000 gran 0x00 drq
[DEBUG]  PNP: 002e.a f2 <- [0x000000000000005d - 0x000000000000005d] size 0x00000001 gran 0x00 drq
[DEBUG]  PNP: 002e.b 60 <- [0x0000000000000290 - 0x0000000000000291] size 0x00000002 gran 0x01 io
[DEBUG]  PNP: 002e.b 62 <- [0x0000000000000000 - 0x0000000000000001] size 0x00000002 gran 0x01 io
[DEBUG]  PNP: 002e.b 70 <- [0x0000000000000000 - 0x0000000000000000] size 0x00000001 gran 0x00 irq
[NOTE ]  PNP: 002e.b f0 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.308 60 io size: 0x0000000008 not assigned in devicetree
[NOTE ]  PNP: 002e.609 f4 irq size: 0x0000000001 not assigned in devicetree
[NOTE ]  PNP: 002e.609 f5 irq size: 0x0000000001 not assigned in devicetree
[DEBUG]  PCI: 00:00:1f.2 10 <- [0x000000000000dfb8 - 0x000000000000dfbf] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:00:1f.2 14 <- [0x000000000000dfac - 0x000000000000dfaf] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:00:1f.2 18 <- [0x000000000000dfb0 - 0x000000000000dfb7] size 0x00000008 gran 0x03 io
[DEBUG]  PCI: 00:00:1f.2 1c <- [0x000000000000dfa8 - 0x000000000000dfab] size 0x00000004 gran 0x02 io
[DEBUG]  PCI: 00:00:1f.2 20 <- [0x000000000000dfc0 - 0x000000000000dfdf] size 0x00000020 gran 0x05 io
[DEBUG]  PCI: 00:00:1f.2 24 <- [0x00000000efbca000 - 0x00000000efbca7ff] size 0x00000800 gran 0x0b mem
[DEBUG]  PCI: 00:00:1f.3 10 <- [0x00000000efbc7000 - 0x00000000efbc70ff] size 0x00000100 gran 0x08 mem64
[INFO ]  Done setting resources.
[INFO ]  Done allocating resources.
[DEBUG]  BS: BS_DEV_RESOURCES run times (exec / console): 3 / 1801 ms
[INFO ]  POST: 0x74
[INFO ]  Timestamp - device enable: 54826629724
[INFO ]  Enabling resources...
[DEBUG]  PCI: 00:00:00.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:00.0 cmd <- 06
[DEBUG]  PCI: 00:00:01.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:01.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:01.0 cmd <- 00
[DEBUG]  PCI: 00:00:14.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:14.0 cmd <- 102
[DEBUG]  PCI: 00:00:16.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:16.0 cmd <- 02
[DEBUG]  PCI: 00:00:19.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:19.0 cmd <- 103
[DEBUG]  PCI: 00:00:1a.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1a.0 cmd <- 102
[DEBUG]  PCI: 00:00:1b.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1b.0 cmd <- 102
[DEBUG]  PCI: 00:00:1c.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:1c.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1c.0 cmd <- 107
[DEBUG]  PCI: 00:00:1c.3 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:1c.3 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1c.3 cmd <- 107
[DEBUG]  PCI: 00:00:1c.4 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:1c.4 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1c.4 cmd <- 100
[DEBUG]  PCI: 00:00:1c.7 bridge ctrl <- 0013
[DEBUG]  PCI: 00:00:1c.7 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1c.7 cmd <- 106
[DEBUG]  PCI: 00:00:1d.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1d.0 cmd <- 102
[DEBUG]  PCI: 00:00:1f.0 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1f.0 cmd <- 107
[DEBUG]  PCI: 00:00:1f.2 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1f.2 cmd <- 03
[DEBUG]  PCI: 00:00:1f.3 subsystem <- 1043/84ca
[DEBUG]  PCI: 00:00:1f.3 cmd <- 103
[DEBUG]  PCI: 00:02:00.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:02:00.0 cmd <- 07
[DEBUG]  PCI: 00:03:01.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:03:01.0 cmd <- 07
[DEBUG]  PCI: 00:03:02.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:03:02.0 cmd <- 06
[DEBUG]  PCI: 00:04:00.0 cmd <- 03
[DEBUG]  PCI: 00:05:00.0 cmd <- 02
[DEBUG]  PCI: 00:06:00.0 cmd <- 03
[DEBUG]  PCI: 00:07:00.0 bridge ctrl <- 0013
[DEBUG]  PCI: 00:07:00.0 cmd <- 00
[DEBUG]  PCI: 00:09:00.0 cmd <- 02
[INFO ]  done.
[DEBUG]  BS: BS_DEV_ENABLE run times (exec / console): 0 / 217 ms
[DEBUG]  read 6000 from 07e4
[DEBUG]  wrote 00000004 to 0890
[DEBUG]  read 03040003 from 0894
[DEBUG]  wrote 00001000 to 0890
[DEBUG]  read 09300024 from 0894
[DEBUG]  read 00000000 from 0880
[DEBUG]  wrote 00000000 to 0880
[DEBUG]  BS: BS_DEV_INIT entry times (exec / console): 0 / 25 ms
[INFO ]  POST: 0x75
[INFO ]  Timestamp - device initialization: 55566728559
[INFO ]  Initializing devices...
[INFO ]  POST: 0x75
[DEBUG]  CPU_CLUSTER: 0 init
[INFO ]  LAPIC 0x0 switched to X2APIC mode.
[DEBUG]  MTRR: Physical address space:
[DEBUG]  0x0000000000000000 - 0x000000000009ffff size 0x000a0000 type 6
[DEBUG]  0x00000000000a0000 - 0x00000000000bffff size 0x00020000 type 0
[DEBUG]  0x00000000000c0000 - 0x000000007fffffff size 0x7ff40000 type 6
[DEBUG]  0x0000000080000000 - 0x00000000ffffffff size 0x80000000 type 0
[DEBUG]  0x0000000100000000 - 0x000000047a5fffff size 0x37a600000 type 6
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x250 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x258 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x259 0x0000000000000000
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x268 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x269 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26a 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26b 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26c 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26d 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26e 0x0606060606060606
[DEBUG]  apic_id 0x0: MTRR: Fixed MSR 0x26f 0x0606060606060606
[DEBUG]  apic_id 0x0 setup mtrr for CPU physical address size: 36 bits
[DEBUG]  MTRR: default type WB/UC MTRR counts: 1/4.
[DEBUG]  MTRR: WB selected as default type.
[DEBUG]  MTRR: 0 base 0x0000000080000000 mask 0x0000000f80000000 type 0

[DEBUG]  MTRR check
[DEBUG]  Fixed MTRRs   : Enabled
[DEBUG]  Variable MTRRs: Enabled

[INFO ]  POST: 0x93
[DEBUG]  CPU has 4 cores, 4 threads enabled.
[DEBUG]  Setting up SMI for CPU
[INFO ]  Will perform SMM setup.
[DEBUG]  microcode: sig=0x306a9 pf=0x2 revision=0x21
[INFO ]  CBFS: Found 'cpu_microcode_blob.bin' @0x80 size 0x6800 in mcache @0x7ffdc02c
[INFO ]  CPU: Intel(R) Core(TM) i5-3475S CPU @ 2.90GHz.
[INFO ]  LAPIC 0x0 in X2APIC mode.
[DEBUG]  CPU: APIC: 00 enabled
[DEBUG]  CPU: APIC: 01 enabled
[DEBUG]  CPU: APIC: 02 enabled
[DEBUG]  CPU: APIC: 03 enabled
[DEBUG]  Loading module at 0x00030000 with entry 0x00030000. filesize: 0x178 memsize: 0x178
[DEBUG]  Processing 16 relocs. Offset value of 0x00030000
[DEBUG]  Attempting to start 3 APs
[DEBUG]  Waiting for 10ms after sending INIT.
[DEBUG]  Waiting for SIPI to complete...
[DEBUG]  done.
[DEBUG]  Waiting for SIPI to complete...
[DEBUG]  done.
[INFO ]  LAPIC 0x2 switched to X2APIC mode.
[INFO ]  AP: slot 1 apic_id 2, MCU rev: 0x00000021
[INFO ]  LAPIC 0x4 switched to X2APIC mode.
[INFO ]  LAPIC 0x6 switched to X2APIC mode.
[INFO ]  AP: slot 2 apic_id 4, MCU rev: 0x00000021
[INFO ]  AP: slot 3 apic_id 6, MCU rev: 0x00000021
[DEBUG]  Loading module at 0x00038000 with entry 0x00038000. filesize: 0x1a0 memsize: 0x1a0
[DEBUG]  Processing 9 relocs. Offset value of 0x00038000
[DEBUG]  smm_module_setup_stub: stack_top = 0x80001000
[DEBUG]  smm_module_setup_stub: per cpu stack_size = 0x400
[DEBUG]  smm_module_setup_stub: runtime.smm_size = 0x10000
[DEBUG]  SMM Module: stub loaded at 38000. Will call 0x7fe95c9a
[DEBUG]  Installing permanent SMM handler to 0x80000000
[DEBUG]  HANDLER      [0x802fe000-0x802ff62f]

[DEBUG]  CPU 0
[DEBUG]    ss0        [0x802fdc00-0x802fdfff]
[DEBUG]    stub0      [0x802f6000-0x802f619f]

[DEBUG]  CPU 1
[DEBUG]    ss1        [0x802fd800-0x802fdbff]
[DEBUG]    stub1      [0x802f5c00-0x802f5d9f]

[DEBUG]  CPU 2
[DEBUG]    ss2        [0x802fd400-0x802fd7ff]
[DEBUG]    stub2      [0x802f5800-0x802f599f]

[DEBUG]  CPU 3
[DEBUG]    ss3        [0x802fd000-0x802fd3ff]
[DEBUG]    stub3      [0x802f5400-0x802f559f]

[DEBUG]  stacks       [0x80000000-0x80000fff]
[DEBUG]  Loading module at 0x802fe000 with entry 0x802ff37c. filesize: 0x15d0 memsize: 0x1630
[DEBUG]  Processing 77 relocs. Offset value of 0x802fe000
[DEBUG]  Loading module at 0x802f6000 with entry 0x802f6000. filesize: 0x1a0 memsize: 0x1a0
[DEBUG]  Processing 9 relocs. Offset value of 0x802f6000
[DEBUG]  smm_module_setup_stub: stack_top = 0x80001000
[DEBUG]  smm_module_setup_stub: per cpu stack_size = 0x400
[DEBUG]  smm_module_setup_stub: runtime.smm_size = 0x300000
[DEBUG]  SMM Module: placing smm entry code at 802f5c00,  cpu # 0x1
[DEBUG]  SMM Module: placing smm entry code at 802f5800,  cpu # 0x2
[DEBUG]  SMM Module: placing smm entry code at 802f5400,  cpu # 0x3
[DEBUG]  SMM Module: stub loaded at 802f6000. Will call 0x802ff37c
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ee000, cpu = 0
[DEBUG]  In relocation handler: cpu 0
[DEBUG]  New SMBASE=0x802ee000 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802edc00, cpu = 1
[DEBUG]  In relocation handler: cpu 1
[DEBUG]  New SMBASE=0x802edc00 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ed800, cpu = 2
[DEBUG]  In relocation handler: cpu 2
[DEBUG]  New SMBASE=0x802ed800 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  smm_do_relocation : curr_smbase 0x30000 perm_smbase 0x802ed400, cpu = 3
[DEBUG]  In relocation handler: cpu 3
[DEBUG]  New SMBASE=0x802ed400 IEDBASE=0x80400000
[DEBUG]  Writing SMRR. base = 0x80000006, mask=0xff800800
[DEBUG]  Relocation complete.
[INFO ]  microcode: Update skipped, already up-to-date
[INFO ]  Initializing CPU #0
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[INFO ]  CPU: Intel(R) Core(TM) i5-3475S CPU @ 2.90GHz.
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  IA32_FEATURE_CONTROL already locked; VMX status: enabled
[DEBUG]  IA32_FEATURE_CONTROL already locked
[INFO ]  APIC: 00: PP0 current limit not set in devicetree
[INFO ]  APIC: 00: PP0 PSI0 not set in devicetree
[INFO ]  APIC: 00: PP0 PSI1 not set in devicetree
[INFO ]  APIC: 00: PP0 PSI2 not set in devicetree
[INFO ]  APIC: 00: PP1 current limit not set in devicetree
[INFO ]  APIC: 00: PP1 PSI0 not set in devicetree
[INFO ]  APIC: 00: PP1 PSI1 not set in devicetree
[INFO ]  APIC: 00: PP1 PSI2 not set in devicetree
[INFO ]  APIC: 00: Programmable ratio limit for turbo mode is disabled
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 2900
[INFO ]  Turbo is available but hidden
[INFO ]  Turbo is available and visible
[INFO ]  CPU #0 initialized
[INFO ]  Initializing CPU #1
[INFO ]  Initializing CPU #2
[INFO ]  Initializing CPU #3
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[INFO ]  CPU: Intel(R) Core(TM) i5-3475S CPU @ 2.90GHz.
[INFO ]  CPU: Intel(R) Core(TM) i5-3475S CPU @ 2.90GHz.
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  CPU: vendor Intel device 306a9
[DEBUG]  CPU: family 06, model 3a, stepping 09
[DEBUG]  IA32_FEATURE_CONTROL already locked; VMX status: enabled
[INFO ]  CPU: Intel(R) Core(TM) i5-3475S CPU @ 2.90GHz.
[DEBUG]  IA32_FEATURE_CONTROL already locked
[INFO ]  CPU: cpuid(1) 0x306a9
[INFO ]  APIC: 02: Programmable ratio limit for turbo mode is disabled
[INFO ]  CPU: AES supported
[INFO ]  CPU: TXT supported
[INFO ]  CPU: VT supported
[DEBUG]  IA32_FEATURE_CONTROL already locked; VMX status: enabled
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  IA32_FEATURE_CONTROL already locked
[DEBUG]  IA32_FEATURE_CONTROL already locked; VMX status: enabled
[INFO ]  APIC: 04: Programmable ratio limit for turbo mode is disabled
[DEBUG]  IA32_FEATURE_CONTROL already locked
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 2900
[INFO ]  CPU #1 initialized
[DEBUG]  model_x06ax: frequency set to 2900
[INFO ]  CPU #2 initialized
[INFO ]  APIC: 06: Programmable ratio limit for turbo mode is disabled
[DEBUG]  cpu: energy policy set to 6
[DEBUG]  model_x06ax: frequency set to 2900
[INFO ]  CPU #3 initialized
[INFO ]  bsp_do_flight_plan done after 625 msecs.
[DEBUG]  SMI_STS: 
[DEBUG]  GPE0_STS: GPIO14 GPIO11 GPIO10 GPIO9 GPIO6 
[DEBUG]  ALT_GP_SMI_STS: GPI14 GPI13 GPI11 GPI10 GPI9 GPI8 GPI6 GPI5 GPI4 GPI3 GPI2 GPI1 
[DEBUG]  TCO_STS: 
[DEBUG]  Locking SMM.
[DEBUG]  CPU_CLUSTER: 0 init finished in 897 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:00.0 init
[DEBUG]  Disabling PEG11.
[DEBUG]  Disabling IGD.
[DEBUG]  Disabling Device 7.
[DEBUG]  Set BIOS_RESET_CPL
[DEBUG]  CPU TDP: 65 Watts
[DEBUG]  PCI: 00:00:00.0 init finished in 16 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:01.0 init
[DEBUG]  PCI: 00:00:01.0 init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:14.0 init
[DEBUG]  XHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:14.0 init finished in 4 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:16.0 init
[DEBUG]  ME: FW Partition Table      : OK
[DEBUG]  ME: Bringup Loader Failure  : NO
[DEBUG]  ME: Firmware Init Complete  : YES
[DEBUG]  ME: Manufacturing Mode      : YES
[DEBUG]  ME: Boot Options Present    : NO
[DEBUG]  ME: Update In Progress      : NO
[DEBUG]  ME: Current Working State   : Normal
[DEBUG]  ME: Current Operation State : M0 with UMA
[DEBUG]  ME: Current Operation Mode  : Normal
[DEBUG]  ME: Error Code              : No Error
[DEBUG]  ME: Progress Phase          : Host Communication
[DEBUG]  ME: Power Management Event  : Pseudo-global reset
[DEBUG]  ME: Progress Phase State    : Host communication established
[NOTE ]  ME: BIOS path: Normal
[DEBUG]  No CMOS option 'me_state'.
[DEBUG]  No CMOS option 'me_state_prev'.
[DEBUG]  ME: me_state=0, me_state_prev=0
[DEBUG]  ME: Extend SHA-256: 89c5086d985c68d6817725b46ce96d1c2f968bae63d77eb5bd9b9a92920ffd04
[INFO ]  ME: MBP item header 00020103
[INFO ]  ME: MBP item header 00050102
[INFO ]  ME: MBP item header 00020501
[INFO ]  ME: MBP item header 00020201
[INFO ]  ME: MBP item header 02030101
[INFO ]  ME: MBP item header 02060301
[INFO ]  ME: MBP item header 02090401
[DEBUG]  ME: found version 8.1.0.1248
[DEBUG]  ME Capability: Full Network manageability                : disabled
[DEBUG]  ME Capability: Regular Network manageability             : disabled
[DEBUG]  ME Capability: Manageability                             : disabled
[DEBUG]  ME Capability: Small business technology                 : disabled
[DEBUG]  ME Capability: Level III manageability                   : disabled
[DEBUG]  ME Capability: IntelR Anti-Theft (AT)                    : disabled
[DEBUG]  ME Capability: IntelR Capability Licensing Service (CLS) :  enabled
[DEBUG]  ME Capability: IntelR Power Sharing Technology (MPC)     :  enabled
[DEBUG]  ME Capability: ICC Over Clocking                         :  enabled
[DEBUG]  ME Capability: Protected Audio Video Path (PAVP)         :  enabled
[DEBUG]  ME Capability: IPV6                                      : disabled
[DEBUG]  ME Capability: KVM Remote Control (KVM)                  : disabled
[DEBUG]  ME Capability: Outbreak Containment Heuristic (OCH)      : disabled
[DEBUG]  ME Capability: Virtual LAN (VLAN)                        :  enabled
[DEBUG]  ME Capability: TLS                                       : disabled
[DEBUG]  ME Capability: Wireless LAN (WLAN)                       : disabled
[DEBUG]  PCI: 00:00:16.0 init finished in 241 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:19.0 init
[DEBUG]  PCI: 00:00:19.0 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1a.0 init
[DEBUG]  EHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:1a.0 init finished in 4 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1b.0 init
[DEBUG]  Azalia: base = 0xefbcc000
[DEBUG]  Azalia: codec_mask = 09
[DEBUG]  azalia_audio: initializing codec #3...
[DEBUG]  azalia_audio:  - vendor/device id: 0x80862806
[DEBUG]  azalia_audio:  - verb size: 16
[DEBUG]  azalia_audio:  - verb loaded
[DEBUG]  azalia_audio: initializing codec #0...
[DEBUG]  azalia_audio:  - vendor/device id: 0x10ec0892
[DEBUG]  azalia_audio:  - verb size: 60
[DEBUG]  azalia_audio:  - verb loaded
[DEBUG]  PCI: 00:00:1b.0 init finished in 49 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1c.0 init
[DEBUG]  Initializing PCH PCIe bridge.
[DEBUG]  PCI: 00:00:1c.0 init finished in 4 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1c.3 init
[DEBUG]  Initializing PCH PCIe bridge.
[DEBUG]  PCI: 00:00:1c.3 init finished in 4 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1c.4 init
[DEBUG]  Initializing PCH PCIe bridge.
[DEBUG]  PCI: 00:00:1c.4 init finished in 4 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1c.7 init
[DEBUG]  Initializing PCH PCIe bridge.
[DEBUG]  PCI: 00:00:1c.7 init finished in 4 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1d.0 init
[DEBUG]  EHCI: Setting up controller.. done.
[DEBUG]  PCI: 00:00:1d.0 init finished in 4 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1f.0 init
[DEBUG]  pch: lpc_init
[INFO ]  PCH: detected Z77, device id: 0x1e44, rev id 0x4
[DEBUG]  IOAPIC: Initializing IOAPIC at fec00000
[DEBUG]  IOAPIC: ID = 0x00
[DEBUG]  IOAPIC: 24 interrupts
[DEBUG]  IOAPIC: Clearing IOAPIC at fec00000
[DEBUG]  IOAPIC: Bootstrap Processor Local APIC = 0x00
[INFO ]  Set power off after power failure.
[INFO ]  NMI sources disabled.
[DEBUG]  PantherPoint PM init
[DEBUG]  RTC: failed = 0x0
[DEBUG]  RTC Init
[DEBUG]  apm_control: Disabling ACPI.
[DEBUG]  APMC done.
[DEBUG]  pch_spi_init
[DEBUG]  PCI: 00:00:1f.0 init finished in 56 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1f.2 init
[DEBUG]  SATA: Initializing...
[DEBUG]  SATA: Controller in AHCI mode.
[DEBUG]  ABAR: 0xefbca000
[DEBUG]  PCI: 00:00:1f.2 init finished in 10 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:00:1f.3 init
[DEBUG]  PCI: 00:00:1f.3 init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:04:00.0 init
[DEBUG]  PCI: 00:04:00.0 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:05:00.0 init
[DEBUG]  PCI: 00:05:00.0 init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PCI: 00:09:00.0 init
[DEBUG]  PCI: 00:09:00.0 init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.2 init
[DEBUG]  PNP: 002e.2 init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.5 init
[DEBUG]  Keyboard init...
[DEBUG]  PS/2 keyboard initialized on primary channel
[DEBUG]  PNP: 002e.5 init finished in 423 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.108 init
[DEBUG]  PNP: 002e.108 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.109 init
[DEBUG]  PNP: 002e.109 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.209 init
[DEBUG]  PNP: 002e.209 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.309 init
[DEBUG]  PNP: 002e.309 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.509 init
[DEBUG]  PNP: 002e.509 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.a init
[DEBUG]  PNP: 002e.a init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.b init
[DEBUG]  PNP: 002e.b init finished in 0 msecs
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.308 init
[DEBUG]  PNP: 002e.308 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.409 init
[DEBUG]  PNP: 002e.409 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.609 init
[DEBUG]  PNP: 002e.609 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.709 init
[DEBUG]  PNP: 002e.709 init finished in 0 msecs
[INFO ]  POST: 0x75
[DEBUG]  PNP: 002e.9 init
[DEBUG]  PNP: 002e.9 init finished in 0 msecs
[INFO ]  Devices initialized
[DEBUG]  BS: BS_DEV_INIT run times (exec / console): 740 / 1440 ms
[DEBUG]  clear_memory: Clearing DRAM 0000000000000000-0000000000005000
[ERROR]  Null dereference at eip: 0x7fea0e22
[DEBUG]  clear_memory: Clearing DRAM 000000000000a000-00000000000a0000
[DEBUG]  clear_memory: Clearing DRAM 00000000000c0000-000000007fe68000
[DEBUG]  clear_memory: Clearing DRAM 0000000100000000-000000047a600000
[DEBUG]  memset_pae: Using virtual address 0x00400000 as scratchpad
[DEBUG]  init_pae_pagetables: Using address 0x00005000 for page tables
[DEBUG]  clear_memory: Clearing DRAM 0000000000005000-000000000000a000
[DEBUG]  BS: BS_DEV_INIT exit times (exec / console): 735 / 53 ms
[INFO ]  POST: 0x76
[INFO ]  Finalize devices...
[DEBUG]  PCI: 00:00:1f.0 final
[DEBUG]  read 6008 from 07e4
[DEBUG]  wrote 5006 to 0874
[DEBUG]  wrote 01 to 0878
[DEBUG]  wrote 02 to 0879
[DEBUG]  wrote 03 to 087a
[DEBUG]  wrote 05 to 087b
[DEBUG]  wrote 20 to 087c
[DEBUG]  wrote 9f to 087d
[DEBUG]  wrote d8 to 087e
[DEBUG]  wrote 0b to 087f
[DEBUG]  wrote b32d to 0876
[INFO ]  Devices finalized
[INFO ]  Timestamp - device setup done: 64339362021
[DEBUG]  BS: BS_POST_DEVICE run times (exec / console): 0 / 52 ms
[INFO ]  POST: 0x77
[INFO ]  Timestamp - cbmem post: 64380736613
[DEBUG]  BS: BS_OS_RESUME_CHECK run times (exec / console): 0 / 7 ms
[INFO ]  POST: 0x79
[INFO ]  Timestamp - write tables: 64421109901
[INFO ]  POST: 0x9c
[INFO ]  CBFS: Found 'fallback/dsdt.aml' @0x2ec80 size 0x2332 in mcache @0x7ffdc158
[WARN ]  CBFS: 'fallback/slic' not found.
[INFO ]  ACPI: Writing ACPI tables at 7fe3c000.
[DEBUG]  ACPI:    * FACS
[DEBUG]  ACPI:    * FACP
[DEBUG]  ACPI: added table 1/32, length now 44
[DEBUG]  Found 1 CPU(s) with 4 core(s) each.
[DEBUG]  Supported C-states:  C0 C1 C1E C3 C6
[DEBUG]  PSS: 2901MHz power 65000 control 0x2400 status 0x2400
[DEBUG]  PSS: 2900MHz power 65000 control 0x1d00 status 0x1d00
[DEBUG]  PSS: 2600MHz power 56259 control 0x1a00 status 0x1a00
[DEBUG]  PSS: 2400MHz power 50690 control 0x1800 status 0x1800
[DEBUG]  PSS: 2200MHz power 45377 control 0x1600 status 0x1600
[DEBUG]  PSS: 2000MHz power 40306 control 0x1400 status 0x1400
[DEBUG]  PSS: 1800MHz power 35383 control 0x1200 status 0x1200
[DEBUG]  PSS: 1600MHz power 30693 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 2901MHz power 65000 control 0x2400 status 0x2400
[DEBUG]  PSS: 2900MHz power 65000 control 0x1d00 status 0x1d00
[DEBUG]  PSS: 2600MHz power 56259 control 0x1a00 status 0x1a00
[DEBUG]  PSS: 2400MHz power 50690 control 0x1800 status 0x1800
[DEBUG]  PSS: 2200MHz power 45377 control 0x1600 status 0x1600
[DEBUG]  PSS: 2000MHz power 40306 control 0x1400 status 0x1400
[DEBUG]  PSS: 1800MHz power 35383 control 0x1200 status 0x1200
[DEBUG]  PSS: 1600MHz power 30693 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 2901MHz power 65000 control 0x2400 status 0x2400
[DEBUG]  PSS: 2900MHz power 65000 control 0x1d00 status 0x1d00
[DEBUG]  PSS: 2600MHz power 56259 control 0x1a00 status 0x1a00
[DEBUG]  PSS: 2400MHz power 50690 control 0x1800 status 0x1800
[DEBUG]  PSS: 2200MHz power 45377 control 0x1600 status 0x1600
[DEBUG]  PSS: 2000MHz power 40306 control 0x1400 status 0x1400
[DEBUG]  PSS: 1800MHz power 35383 control 0x1200 status 0x1200
[DEBUG]  PSS: 1600MHz power 30693 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PSS: 2901MHz power 65000 control 0x2400 status 0x2400
[DEBUG]  PSS: 2900MHz power 65000 control 0x1d00 status 0x1d00
[DEBUG]  PSS: 2600MHz power 56259 control 0x1a00 status 0x1a00
[DEBUG]  PSS: 2400MHz power 50690 control 0x1800 status 0x1800
[DEBUG]  PSS: 2200MHz power 45377 control 0x1600 status 0x1600
[DEBUG]  PSS: 2000MHz power 40306 control 0x1400 status 0x1400
[DEBUG]  PSS: 1800MHz power 35383 control 0x1200 status 0x1200
[DEBUG]  PSS: 1600MHz power 30693 control 0x1000 status 0x1000
[INFO ]  Requested C-state C7 not supported, using C6 instead
[DEBUG]  Advertising ACPI C State type C1 as CPU C1
[DEBUG]  Advertising ACPI C State type C2 as CPU C3
[DEBUG]  Advertising ACPI C State type C3 as CPU C6
[DEBUG]  PCI space above 4GB MMIO is at 0x47a600000, len = 0xb85a00000
[DEBUG]  Generating ACPI PIRQ entries
[DEBUG]  ACPI:    * SSDT
[DEBUG]  ACPI: added table 2/32, length now 52
[DEBUG]  ACPI:    * MCFG
[DEBUG]  ACPI: added table 3/32, length now 60
[DEBUG]  IOAPIC: 24 interrupts
[DEBUG]  ACPI:    * APIC
[DEBUG]  ACPI: added table 4/32, length now 68
[DEBUG]  ACPI:    * SPCR
[DEBUG]  ACPI: added table 5/32, length now 76
[DEBUG]  current = 7fe3fc30
[DEBUG]  ACPI:     * DMAR
[DEBUG]  ACPI: added table 6/32, length now 84
[DEBUG]  current = 7fe3fcc0
[DEBUG]  ACPI:    * HPET
[DEBUG]  ACPI: added table 7/32, length now 92
[INFO ]  ACPI: done.
[DEBUG]  ACPI tables: 15616 bytes.
[DEBUG]  smbios_write_tables: 7fe34000
[DEBUG]  SMBIOS firmware version is set to coreboot_version: '25.03-250-g59e4095ecfcb-dirty'
[INFO ]  Create SMBIOS type 16
[INFO ]  Create SMBIOS type 17
[INFO ]  Create SMBIOS type 20
[DEBUG]  SMBIOS tables: 956 bytes.
[DEBUG]  Writing table forward entry at 0x00000500
[DEBUG]  Wrote coreboot table at: 0x00000500, 0x10 bytes, checksum 7ff8
[DEBUG]  Writing coreboot table at 0x7fe60000
[INFO ]  CBFS: Found 'cmos_layout.bin' @0x31680 size 0x5ac in mcache @0x7ffdc1dc
[DEBUG]  CFR: Written 16 bytes of CFR structures at 0x7fe605dc, with CRC32 0x00000000
[DEBUG]   0. 0000000000000000-0000000000000fff: CONFIGURATION TABLES
[DEBUG]   1. 0000000000001000-000000000009ffff: RAM
[DEBUG]   2. 00000000000a0000-00000000000f5fff: RESERVED
[DEBUG]   3. 00000000000f6000-00000000000f6fff: CONFIGURATION TABLES
[DEBUG]   4. 00000000000f7000-00000000000fffff: RESERVED
[DEBUG]   5. 0000000000100000-000000007fe33fff: RAM
[DEBUG]   6. 000000007fe34000-000000007fe78fff: CONFIGURATION TABLES
[DEBUG]   7. 000000007fe79000-000000007ffcbfff: RAMSTAGE
[DEBUG]   8. 000000007ffcc000-000000007fffffff: CONFIGURATION TABLES
[DEBUG]   9. 0000000080000000-00000000849fffff: RESERVED
[DEBUG]  10. 00000000f0000000-00000000f3ffffff: RESERVED
[DEBUG]  11. 00000000fed90000-00000000fed91fff: RESERVED
[DEBUG]  12. 0000000100000000-000000047a5fffff: RAM
[DEBUG]  Wrote coreboot table at: 0x7fe60000, 0x98c bytes, checksum df11
[DEBUG]  coreboot table: 2468 bytes.
[DEBUG]  IMD ROOT    0. 0x7ffff000 0x00001000
[DEBUG]  IMD SMALL   1. 0x7fffe000 0x00001000
[DEBUG]  CONSOLE     2. 0x7ffde000 0x00020000
[DEBUG]  TIME STAMP  3. 0x7ffdd000 0x00000910
[DEBUG]  RO MCACHE   4. 0x7ffdc000 0x000003d0
[DEBUG]  MEM INFO    5. 0x7ffdb000 0x00000f48
[DEBUG]  AFTER CAR   6. 0x7ffcc000 0x0000f000
[DEBUG]  RAMSTAGE    7. 0x7fe78000 0x00154000
[DEBUG]  SMM BACKUP  8. 0x7fe68000 0x00010000
[DEBUG]  COREBOOT    9. 0x7fe60000 0x00008000
[DEBUG]  ACPI       10. 0x7fe3c000 0x00024000
[DEBUG]  SMBIOS     11. 0x7fe34000 0x00008000
[DEBUG]  IMD small region:
[DEBUG]    IMD ROOT    0. 0x7fffec00 0x00000400
[DEBUG]    FMAP        1. 0x7fffeb20 0x000000e0
[DEBUG]    ROMSTAGE    2. 0x7fffeb00 0x00000004
[DEBUG]    ROMSTG STCK 3. 0x7fffea40 0x000000a8
[DEBUG]    ACPI GNVS   4. 0x7fffe940 0x00000100
[INFO ]  Timestamp - finalize chips: 66283089553
[DEBUG]  BS: BS_WRITE_TABLES run times (exec / console): 3 / 646 ms
[INFO ]  POST: 0x7a
[INFO ]  Timestamp - starting to load payload: 66324214645
[INFO ]  CBFS: Found 'fallback/payload' @0x51000 size 0x11c61 in mcache @0x7ffdc298
[DEBUG]  Checking segment from ROM address 0xffa6122c
[DEBUG]  Payload being loaded at below 1MiB without region being marked as RAM usable.
[DEBUG]  Checking segment from ROM address 0xffa61248
[DEBUG]  Loading segment from ROM address 0xffa6122c
[DEBUG]    code (compression=1)
[DEBUG]    New segment dstaddr 0x000de1a0 memsize 0x21e60 srcaddr 0xffa61264 filesize 0x11c29
[DEBUG]  Loading Segment: addr: 0x000de1a0 memsz: 0x0000000000021e60 filesz: 0x0000000000011c29
[DEBUG]  using LZMA
[INFO ]  Timestamp - starting LZMA decompress (ignore for x86): 66505518801
[INFO ]  Timestamp - finished LZMA decompress (ignore for x86): 66589639489
[DEBUG]  Loading segment from ROM address 0xffa61248
[DEBUG]    Entry Point 0x000fd246
[DEBUG]  BS: BS_PAYLOAD_LOAD run times (exec / console): 21 / 89 ms
[INFO ]  POST: 0x7b
[DEBUG]  ICH-NM10-PCH: watchdog disabled
[DEBUG]  Jumping to boot code at 0x000fd246(0x7fe60000)
[INFO ]  POST: 0xf8
[INFO ]  Timestamp - selfboot jump: 66699733245
SeaBIOS (version rel-1.16.3-0-ga6ed6b7)
BUILD: gcc: (coreboot toolchain v2024-08-28_0abdb8b8a9) 14.2.0 binutils: (GNU Binutils) 2.43.1
SeaBIOS (version rel-1.16.3-0-ga6ed6b7)
BUILD: gcc: (coreboot toolchain v2024-08-28_0abdb8b8a9) 14.2.0 binutils: (GNU Binutils) 2.43.1
Found coreboot cbmem console @ 7ffde000
Found mainboard ASUS P8Z77-V
Relocating init from 0x000df900 to 0x7ee26c20 (size 54080)
Found CBFS header at 0xffa1022c
multiboot: eax=0, ebx=7d8
Found 23 PCI devices (max PCI bus is 09)
Copying SMBIOS from 0x7fe34000 to 0x000f5b40
Copying SMBIOS 3.0 from 0x7fe34020 to 0x000f5b20
Copying ACPI RSDP from 0x7fe3c000 to 0x000f5af0
table(50434146)=0x7fe3e5d0 (via xsdt)
Using pmtimer, ioport 0x508
Scan for VGA option rom
No VGA found, scan for other display
Running option rom at c000:0003
Start SeaVGABIOS (version rel-1.16.3-0-ga6ed6b7)
VGABUILD: gcc: (coreboot toolchain v2024-08-28_0abdb8b8a9) 14.2.0 binutils: (GNU Binutils) 2.43.1
enter vga_post:
   a=00000000  b=0000ffff  c=00000000  d=0000ffff ds=0000 es=f000 ss=0000
  si=00000000 di=000066e0 bp=00000000 sp=00006da2 cs=f000 ip=cff4  f=0000
coreboot vga init
Did not find coreboot framebuffer - assuming EGA text
Attempting to allocate 512 bytes lowmem via pmm call to f000:d06c
pmm call arg1=0
VGA stack allocated at ec180
Hooking hardware timer irq (old=f000fea5 new=c0003ef8)
sercon: using ioport 0x3f8
sercon: configuring in splitmode (vgabios c000:3e1f)
Turning on vga text mode console
set VGA mode 3
SeaBIOS (version rel-1.16.3-0-ga6ed6b7PCI: XHCI at 00:14.0 (mmio 0xefbd0000)
XHCI init: regs @ 0xefbd0000, 8 ports, 32 slots, 32 byte contexts
XHCI    protocol USB  2.00, 4 ports (offset 1), def 3001
XHCI    protocol USB  3.00, 4 ports (offset 5), def 1000
XHCI    extcap 0xc1 @ 0xefbd8040
XHCI    extcap 0xc0 @ 0xefbd8070
XHCI    extcap 0x1 @ 0xefbd8330
)
PCI: XHCI at 05:00.0 (mmio 0xeff00000)
XHCI init: regs @ 0xeff00000, 4 ports, 64 slots, 64 byte contexts
XHCI    extcap 0x1 @ 0xeff01000
XHCI    protocol USB  2.00, 2 ports (offset 1), def 0
XHCI    protocol USB  3.00, 2 ports (offset 3), def 0
PCI: XHCI at 09:00.0 (mmio 0xefc00000)
XHCI init: regs @ 0xefc00000, 4 ports, 32 slots, 32 byte contexts
XHCI    extcap 0x1 @ 0xefc00800
XHCI    protocol USB  3.00, 2 ports (offset 1), def 0
XHCI    protocol USB  2.00, 2 ports (offset 3), def 1
EHCI init on dev 00:1a.0 (regs=0xefbc9020)
EHCI init on dev 00:1d.0 (regs=0xefbc8020)
AHCI controller at 00:1f.2, iobase 0xefbca000, irq 11
AHCI controller at 04:00.0, iobase 0xefe10000, irq 11
AHCI controller at 06:00.0, iobase 0xefd00000, irq 11
Searching bootorder for: HALT
Found 0 lpt ports
Found 1 serial ports
Searching bootorder for: /rom@img/grub2
Searching bootorder for: /rom@img/nvramcui
Searching bootorder for: /rom@img/coreinfo
XHCI no devices found
XHCI no devices found
XHCI port #3: 0x00200a03, powered, enabled, pls 0, speed 2 [Low]
USB mouse initialized
Initialized USB HUB (0 ports used)
Initialized USB HUB (0 ports used)
PS2 keyboard initialized
Searching bootorder for: /pci@i0cf8/*@1f,2/drive@0/disk@0
AHCI/0: Set transfer mode to UDMA-5
Searching bios-geometry for: /pci@i0cf8/*@1f,2/drive@0/disk@0
AHCI/0: registering: "AHCI/0: ADATA SP600 ATA-9 Hard-Disk (30533 MiBytes)"
All threads complete.
Scan for option roms

Press ESC for boot menu.

Searching bootorder for: HALT
drive 0x000f5a40: PCHS=16383/16/63 translation=lba LCHS=1024/255/63 s=62533296
Space available for UMB: c7800-eb000, f5360-f5a40
Returned 16683008 bytes of ZoneHigh
e820 map has 8 items:
  0: 0000000000000000 - 000000000009fc00 = 1 RAM
  1: 000000000009fc00 - 00000000000a0000 = 2 RESERVED
  2: 00000000000f0000 - 0000000000100000 = 2 RESERVED
  3: 0000000000100000 - 000000007fe1d000 = 1 RAM
  4: 000000007fe1d000 - 0000000084a00000 = 2 RESERVED
  5: 00000000f0000000 - 00000000f4000000 = 2 RESERVED
  6: 00000000fed90000 - 00000000fed92000 = 2 RESERVED
  7: 0000000100000000 - 000000047a600000 = 1 RAM
enter handle_19:
  NULL
Booting from Hard Disk..Booting from 0000:7c00
.
GRUB loading.
Welcome to GRUB!

VBE current mode=3
stub vbe_104fXX:435:
   a=00004f11  b=00000001  c=0007fbcc  d=00000004 ds=0000 es=6000 ss=ec18
  si=0007fbac di=00008080 bp=00001ff0 sp=000001f6 cs=0000 ip=9104  f=0202
set VGA mode 12








set VGA mode 3
